Altium Designer Pick and Place Locations
C:\Users\buldoant\OneDrive - STMicroelectronics\Desktop\EVL9965A\EVL9965A-R.0.0\EVL9965A\Projects Output for EVL9965A-R.0.0\GERBER FILES EVL99BM218\Pick Place\Pick Place for EVL9965A-R.0.0-Third(EVL99BM218 R0.0).txt

========================================================================================================================
File Design Information:

Date:       15/12/25
Time:       19:42
Revision:   Not in VersionControl
Variant:    EVL99BM218 R0.0
Units used: mil

Designator  Comment                Layer       Footprint                                  Center-X(mil) Center-Y(mil) Rotation Description                                                                                                                                
*           LogoAutomotive         TopLayer    LOGO_Automotive                            -30017.716    -15195.866    0        ""                                                                                                                                         
Log3        "LOGO ST SERIGRAFIA"   TopLayer    LOGO_ST_PICCOLO_-_NO_LIFE_AUGMENTED        -30017.716    -15195.866    90       "LOGO ST SERIGRAFIA"                                                                                                                       
SB12        OPEN                   TopLayer    JP2_SMD                                    223.622       1282.284      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB11        OPEN                   TopLayer    JP2_SMD                                    224.409       1377.953      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB10        OPEN                   TopLayer    JP2_SMD                                    218.002       1556.299      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB9         OPEN                   TopLayer    JP2_SMD                                    215.748       1642.913      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
CMC_L       ACT45B-101-2P-TL003    TopLayer    ACT45B                                     -156.496      1040.354      90       "CMC 100UH 150MA 2LN SMD AEC-Q200"                                                                                                         
SB5         OPEN                   BottomLayer JP2_SMD                                    -218.110      1322.835      90       "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB8         OPEN                   BottomLayer JP2_SMD                                    -232.677      1687.402      270      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB7         OPEN                   BottomLayer JP2_SMD                                    -113.779      1689.262      270      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB6         OPEN                   BottomLayer JP2_SMD                                    -97.638       1320.079      90       "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
R1          CRCW120610R0JNTA       BottomLayer RESC3216X60N                               1894.882      1084.252      180      "SMD Chip Resistor, 10 Ohm, ± 5%, 250 mW, 1206 [3216 Metric], Thick Film, General Purpose"                                                 
C62B        885012205025           BottomLayer CAPC1005X55N                               3387.008      2602.756      0        "WCAP-CSGP 0402 (1005Metric) Ceramic Capacitor 0.039Lx0.020W 1.00mmx0.50mm X7R ±10% 1000pF"                                                
C24C        VJ0402A101KXJPW1BC     TopLayer    CAPC1005X55N                               422.047       1794.882      180      "Cap Ceramic 100pF 16V C0G 10% SMD 0402 125°C Paper T/R"                                                                                   
C24B        885012205025           TopLayer    CAPC1005X55N                               422.835       1832.677      180      "WCAP-CSGP 0402 (1005Metric) Ceramic Capacitor 0.039Lx0.020W 1.00mmx0.50mm X7R ±10% 1000pF"                                                
ISOLP       "Test Point"           TopLayer    TPOINTSMD                                  18.110        1243.701      0        ""                                                                                                                                         
ISOLM       "Test Point"           TopLayer    TPOINTSMD                                  -328.346      1246.850      0        ""                                                                                                                                         
ISOHP       "Test Point"           TopLayer    TPOINTSMD                                  10.453        1658.661      0        ""                                                                                                                                         
ISOHM       "Test Point"           TopLayer    TPOINTSMD                                  -348.425      1658.661      0        ""                                                                                                                                         
SB4         CLOSE                  TopLayer    JP2_SMD                                    -209.055      1685.827      270      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB3         CLOSE                  TopLayer    JP2_SMD                                    -140.157      1687.402      270      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB2         CLOSE                  TopLayer    JP2_SMD                                    -120.866      1212.598      90       "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
SB1         CLOSE                  TopLayer    JP2_SMD                                    -188.189      1212.598      90       "Circuit Breaker 0603 - NOT MOUNTED"                                                                                                       
J_L         70551-0001             TopLayer    70551-0001                                 -155.905      272.441       0        Connector                                                                                                                                  
J_H         70551-0001             BottomLayer 70551-0001                                 -182.677      2676.378      0        Connector                                                                                                                                  
T3          ESMIT4180\C            TopLayer    ESMIT4180\C                                -156.299      717.716       270      "Telecom Transformer 3750Vrms 250mOhm Prim. 250mOhm Sec. DCR 4-Pin SMD"                                                                    
T2          ESMIT4180\C            TopLayer    ESMIT4180\C                                -179.134      2200.787      90       "Telecom Transformer 3750Vrms 250mOhm Prim. 250mOhm Sec. DCR 4-Pin SMD"                                                                    
ISOL_P      "Test Point"           TopLayer    TPOINTSMD                                  27.559        566.929       0        ""                                                                                                                                         
ISOL_M      "Test Point"           TopLayer    TPOINTSMD                                  -334.646      566.929       0        ""                                                                                                                                         
ISOH_P      "Test Point"           TopLayer    TPOINTSMD                                  -86.614       2661.417      0        ""                                                                                                                                         
ISOH_M      "Test Point"           TopLayer    TPOINTSMD                                  -271.654      2661.417      0        ""                                                                                                                                         
R48         39R                    TopLayer    R0402-RS                                   976.378       1960.630      0        "Surface Mount Chip Resistor, Thick Film, AEC-Q200 CRCW Series, 39 ohm, 50 mW, ± 1%, 30 V"                                                 
J1_NTCF     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1460.630      728.346       180      Resistor                                                                                                                                   
J1_NTCG     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1820.866      728.346       180      Resistor                                                                                                                                   
J1_NTCH     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2209.646      728.346       180      Resistor                                                                                                                                   
J1_NTCI     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2563.976      718.504       180      Resistor                                                                                                                                   
J1_NTCJ     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2923.228      723.425       180      Resistor                                                                                                                                   
J2_NTCF     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1396.654      580.709       270      Resistor                                                                                                                                   
J2_NTCG     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1756.890      581.693       270      Resistor                                                                                                                                   
J2_NTCH     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2145.669      580.708       270      Resistor                                                                                                                                   
J2_NTCI     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2500.000      570.866       270      Resistor                                                                                                                                   
J2_NTCJ     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2859.252      575.788       270      Resistor                                                                                                                                   
J1_NTCE     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1451.772      1166.339      180      Resistor                                                                                                                                   
J2_NTCE     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1387.795      1018.701      270      Resistor                                                                                                                                   
J1_NTCC     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2209.646      1166.339      180      Resistor                                                                                                                                   
J1_NTCD     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1830.709      1166.339      180      Resistor                                                                                                                                   
J2_NTCC     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2145.669      1019.685      270      Resistor                                                                                                                                   
J2_NTCD     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               1766.732      1019.685      270      Resistor                                                                                                                                   
J1_NTCB     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2573.819      1164.370      180      Resistor                                                                                                                                   
J2_NTCB     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2495.079      1016.732      270      Resistor                                                                                                                                   
J1_NTCA     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2933.071      1171.260      180      Resistor                                                                                                                                   
J2_NTCA     "Solder Jumoer_1"      TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805               2859.252      1023.622      270      Resistor                                                                                                                                   
TVS4        ESDAVLC8-1BT2Y         TopLayer    SOD-882                                    921.260       1976.378      270      "ESD Suppressor Diode TVS Bi-Dir 3V Automotive 2-Pin SOD-882T T/R"                                                                         
TVS3        ESDAVLC8-1BT2Y         TopLayer    SOD-882                                    921.260       1899.606      90       "ESD Suppressor Diode TVS Bi-Dir 3V Automotive 2-Pin SOD-882T T/R"                                                                         
TVS2        ESDAVLC8-1BT2Y         TopLayer    SOD-882                                    921.260       1818.898      270      "ESD Suppressor Diode TVS Bi-Dir 3V Automotive 2-Pin SOD-882T T/R"                                                                         
TVS1        ESDAVLC8-1BT2Y         TopLayer    SOD-882                                    921.260       1748.032      90       "ESD Suppressor Diode TVS Bi-Dir 3V Automotive 2-Pin SOD-882T T/R"                                                                         
R47         39R                    TopLayer    R0402-RS                                   976.378       1917.323      0        "Surface Mount Chip Resistor, Thick Film, AEC-Q200 CRCW Series, 39 ohm, 50 mW, ± 1%, 30 V"                                                 
R46         39R                    TopLayer    R0402-RS                                   974.951       1763.780      0        "Surface Mount Chip Resistor, Thick Film, AEC-Q200 CRCW Series, 39 ohm, 50 mW, ± 1%, 30 V"                                                 
R45         39R                    TopLayer    R0402-RS                                   976.378       1803.150      0        "Surface Mount Chip Resistor, Thick Film, AEC-Q200 CRCW Series, 39 ohm, 50 mW, ± 1%, 30 V"                                                 
C7          "100pF 50V"            TopLayer    C0402-C                                    1035.433      1976.378      90       "Multilayer Ceramic Capacitor, 100 pF, 50 V, ± 5%, C0G (NP0), 0402 [1005 Metric]"                                                          
C6          "100pF 50V"            TopLayer    C0402-C                                    1035.433      1900.000      90       "Multilayer Ceramic Capacitor, 100 pF, 50 V, ± 5%, C0G (NP0), 0402 [1005 Metric]"                                                          
C5          "100pF 50V"            TopLayer    C0402-C                                    1035.433      1746.958      270      "Multilayer Ceramic Capacitor, 100 pF, 50 V, ± 5%, C0G (NP0), 0402 [1005 Metric]"                                                          
C4          "100pF 50V"            TopLayer    C0402-C                                    1035.433      1822.835      270      "Multilayer Ceramic Capacitor, 100 pF, 50 V, ± 5%, C0G (NP0), 0402 [1005 Metric]"                                                          
C3          C0603C683J4RACTU       BottomLayer C0603-c                                    1015.748      2047.244      0        "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
FidT3       Fiducial               TopLayer    Fiducial_1mm                               108.268       2585.630      90       "Fiducial 1mm"                                                                                                                             
FidT2       Fiducial               TopLayer    Fiducial_1mm                               3385.827      59.055        90       "Fiducial 1mm"                                                                                                                             
FidT1       Fiducial               TopLayer    Fiducial_1mm                               88.081        59.055        90       "Fiducial 1mm"                                                                                                                             
FidB3       Fiducial               BottomLayer Fiducial_1mm                               3385.827      2890.265      90       "Fiducial 1mm"                                                                                                                             
FidB2       Fiducial               BottomLayer Fiducial_1mm                               59.055        59.055        90       "Fiducial 1mm"                                                                                                                             
FidB1       Fiducial               BottomLayer Fiducial_1mm                               3385.827      59.055        90       "Fiducial 1mm"                                                                                                                             
Log2        "LOGO RICICLO"         TopLayer    LOGO_CHINA_ROHS_10                         -30017.716    -15195.866    0        "LOGO RICICLO"                                                                                                                             
P3          2MM-HSP-D06-HT-02-H-TB TopLayer    2MM-HSP-D06-HT-02-H-TB                     3256.929      590.551       270      "12P,2MM,PL HDR,DRRT,2.8,0.76AU,TB"                                                                                                        
P1          2MM-HSP-D12-HT-02-H-TB TopLayer    2MM-HSP-D12-HT-02-H-TB                     3256.934      2114.173      270      "24P,2MM,PL HDR,DRRT,2.8,0.76AU,TB"                                                                                                        
GND1        "Test Point"           TopLayer    4952K                                      3031.496      196.850       180      ""                                                                                                                                         
GND2        "Test Point"           TopLayer    4952K                                      935.827       997.244       180      ""                                                                                                                                         
GND3        "Test Point"           TopLayer    4952K                                      1240.158      240.157       180      ""                                                                                                                                         
R62         ERJ-P06J332V           TopLayer    R0805-RS                                   900.394       817.323       0        "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
LED1        VERDE                  TopLayer    0805_LED                                   1077.441      814.961       180      "Green LED"                                                                                                                                
C110        C0603C104J4RAC3190     TopLayer    C0805-B                                    1973.425      1560.039      180      "ESD SMD Auto X7R 0805 (2012Metric) Ceramic Capacitor 0.079Lx0.049W 2.00mmx1.25mm X7R ±5% 0.22muF"                                         
BBM         "Test Point"           TopLayer    TEST_POINT_-_SIP1                          1929.134      1368.110      180      ""                                                                                                                                         
BBP         "Test Point"           TopLayer    TEST_POINT_-_SIP1                          1801.181      1368.110      180      ""                                                                                                                                         
C38         C0603C104J4RAC3190     TopLayer    C0603-C                                    2172.244      2373.607      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C40         C0603C104J4RAC3190     TopLayer    C0603-C                                    2305.118      2216.127      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C42         C0603C104J4RAC3190     TopLayer    C0603-C                                    2305.118      2112.780      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C43         C0603C104J4RAC3190     TopLayer    C0603-C                                    2305.118      2009.434      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C56         C0603C683J4RACTU       BottomLayer C0603-c                                    1801.181      2209.646      90       "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C57         C0603C683J4RACTU       BottomLayer C0603-c                                    1801.181      2116.142      90       "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C58         C0603C683J4RACTU       BottomLayer C0603-c                                    1801.181      2017.716      90       "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C59         C0603C683J4RACTU       BottomLayer C0603-c                                    1801.181      1909.449      90       "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C60         C0603C683J4RACTU       BottomLayer C0603-c                                    1801.181      1806.102      90       "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C61         C0603C683J4RACTU       BottomLayer C0603-c                                    1806.102      1707.677      90       "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
R15         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2874.016      1953.740      180      ""                                                                                                                                         
R16         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2869.095      1845.473      180      ""                                                                                                                                         
R17         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2874.016      1737.205      180      ""                                                                                                                                         
R18         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2869.095      1638.780      180      ""                                                                                                                                         
R19         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2224.409      1722.441      180      ""                                                                                                                                         
R20         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2229.331      1579.724      180      ""                                                                                                                                         
R21         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2997.047      1486.220      270      ""                                                                                                                                         
R22         SG73P1JTTD2400F        TopLayer    R0603-RS                                   3051.181      1486.220      270      ""                                                                                                                                         
R23         SG73P1JTTD2400F        TopLayer    R0603-RS                                   1993.110      1811.024      180      ""                                                                                                                                         
VBS         "Test Point"           TopLayer    TEST_POINT_-_SIP1                          2002.953      1727.362      180      ""                                                                                                                                         
L9965       L99BM218               TopLayer    TQFP64_(10x10)_0.5_pitch_-_EXPAD_(4.5x4.5) 1496.063      1968.504      180      ""                                                                                                                                         
GND4        "Test Point"           TopLayer    4952K                                      3085.630      2854.331      180      ""                                                                                                                                         
R44_NTCJ    RCC120610K0FKEA        TopLayer    R1206-RS                                   2908.465      423.228       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCI    RCC120610K0FKEA        TopLayer    R1206-RS                                   2559.055      428.150       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCH    RCC120610K0FKEA        TopLayer    R1206-RS                                   2189.961      433.071       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCG    RCC120610K0FKEA        TopLayer    R1206-RS                                   1815.945      437.992       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCF    RCC120610K0FKEA        TopLayer    R1206-RS                                   1446.850      433.071       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCB    RCC120610K0FKEA        TopLayer    R1206-RS                                   2554.134      866.142       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCA    RCC120610K0FKEA        TopLayer    R1206-RS                                   2908.465      871.063       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R43_NTCJ    ERJ-P06J332V           TopLayer    R0805-RS                                   2955.709      649.606       180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCI    ERJ-P06J332V           TopLayer    R0805-RS                                   2598.425      644.685       180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCH    ERJ-P06J332V           TopLayer    R0805-RS                                   2244.095      654.528       180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCG    ERJ-P06J332V           TopLayer    R0805-RS                                   1860.236      654.528       180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCF    ERJ-P06J332V           TopLayer    R0805-RS                                   1504.921      654.528       180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCB    ERJ-P06J332V           TopLayer    R0805-RS                                   2603.347      1090.551      180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCA    ERJ-P06J332V           TopLayer    R0805-RS                                   2967.520      1097.441      180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
JVBS_VB     Jumper                 TopLayer    SIP2                                       2603.347      1426.378      90       ""                                                                                                                                         
JGND_C0     Jumper                 TopLayer    SIP2                                       255.905       1906.693      90       ""                                                                                                                                         
J43         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2515.748      1633.318      180      Resistor                                                                                                                                   
J42         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2515.748      1715.650      180      Resistor                                                                                                                                   
J41         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2515.748      1797.983      180      Resistor                                                                                                                                   
J40         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2515.748      1880.315      180      Resistor                                                                                                                                   
J39         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2515.748      1962.648      180      Resistor                                                                                                                                   
J38         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2515.748      2044.980      180      Resistor                                                                                                                                   
J37         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2514.764      2125.984      180      Resistor                                                                                                                                   
J36         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2514.764      2214.567      180      Resistor                                                                                                                                   
J35         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               543.307       2800.196      0        Resistor                                                                                                                                   
J34         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               543.307       2716.535      0        Resistor                                                                                                                                   
J33         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               543.307       2632.874      0        Resistor                                                                                                                                   
J32         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               543.307       2549.213      0        Resistor                                                                                                                                   
J31         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               543.307       2465.551      0        Resistor                                                                                                                                   
J30         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               543.307       2381.889      0        Resistor                                                                                                                                   
J29         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               543.307       2298.228      0        Resistor                                                                                                                                   
J28         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2514.764      2347.441      180      Resistor                                                                                                                                   
J27         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2513.780      2431.102      180      Resistor                                                                                                                                   
J26         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2514.764      2514.764      180      Resistor                                                                                                                                   
J25         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2514.764      2598.425      180      Resistor                                                                                                                                   
J24         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1994.597      2728.347      270      Resistor                                                                                                                                   
J23         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1897.929      2728.347      270      Resistor                                                                                                                                   
J22         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1801.261      2728.347      270      Resistor                                                                                                                                   
J21         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1704.592      2728.347      270      Resistor                                                                                                                                   
J20         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1607.924      2728.347      270      Resistor                                                                                                                                   
J19         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1511.256      2728.346      270      Resistor                                                                                                                                   
J18         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1414.587      2728.347      270      Resistor                                                                                                                                   
J17         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1317.919      2728.347      270      Resistor                                                                                                                                   
J16         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1221.251      2728.347      270      Resistor                                                                                                                                   
J15         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1124.583      2728.347      270      Resistor                                                                                                                                   
J14         "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1027.914      2728.347      270      Resistor                                                                                                                                   
J8          "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1664.370      235.236       90       Resistor                                                                                                                                   
J7          "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1763.779      235.236       90       Resistor                                                                                                                                   
J6          "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1863.189      235.236       90       Resistor                                                                                                                                   
J5          "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               1962.598      235.236       90       Resistor                                                                                                                                   
C_FIL_NTCJ  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    3011.811      551.181       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCI  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    2642.717      546.260       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCH  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    2298.229      556.102       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCG  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    1909.449      556.102       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCF  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    1554.134      551.181       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCB  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    2637.795      987.205       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCA  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    3001.968      994.095       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_ESD_NTCJ  C0603X682M1RECAUTO     TopLayer    C0603-B                                    2933.071      551.181       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCI  C0603X682M1RECAUTO     TopLayer    C0603-B                                    2573.819      546.260       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCH  C0603X682M1RECAUTO     TopLayer    C0603-B                                    2224.409      556.102       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCG  C0603X682M1RECAUTO     TopLayer    C0603-B                                    1835.630      556.102       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCF  C0603X682M1RECAUTO     TopLayer    C0603-B                                    1475.394      551.181       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCB  C0603X682M1RECAUTO     TopLayer    C0603-B                                    2568.898      987.205       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCA  C0603X682M1RECAUTO     TopLayer    C0603-B                                    2933.071      994.095       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
J4          "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2062.008      235.236       90       Resistor                                                                                                                                   
C90         C0603C104J4RAC3190     TopLayer    C0603-C                                    2305.118      1906.087      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C88         CGA9P3X7T2E225M250KA   BottomLayer C2220-B                                    1440.053      1199.339      0        "Cap Ceramic 2.2uF 250V X7T 20% SMD 5.7 x 5.0 mm 125 C Plastic T/R"                                                                        
P2          "Header 13"            TopLayer    SIP13                                      2162.205      63.976        0        "Header, 13-Pin"                                                                                                                           
CMC_H       ACT45B-101-2P-TL003    TopLayer    ACT45B                                     -175.197      1862.205      270      "CMC 100UH 150MA 2LN SMD AEC-Q200"                                                                                                         
"LOGO RAEE" "LOGO RAEE"            TopLayer    LOGO_CESTINO                               -30017.716    -15195.866    0        "LOGO RAEE"                                                                                                                                
"LOGO RoHS" "LOGO RoHS"            TopLayer    LOGO_RoHS_-_3                              -30017.716    -15195.866    0        "LOGO RoHS"                                                                                                                                
Log1        "LOGO ST SERIGRAFIA"   TopLayer    LOGO_ST_PICCOLO_-_NO_LIFE_AUGMENTED        -30017.716    -15195.866    90       "LOGO ST SERIGRAFIA"                                                                                                                       
C113        CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    1328.740      1687.008      270      "TDK         CGA3E3X7S2A473K080AB             SMD Multilayer Ceramic Capacitor, 0603 [1608 Metric], 0.047 F, 100 V,  10%, X7S, CGA Series" 
C106        C0603C104J4RAC3190     TopLayer    C0603-C                                    2145.669      1692.913      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C104        C0603C104J4RAC3190     TopLayer    C0603-C                                    2691.929      1614.173      180      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C98         C0603C104J4RAC3190     TopLayer    C0603-C                                    2790.354      1899.606      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C96         C0603C104J4RAC3190     TopLayer    C0603-C                                    2790.354      2007.874      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
VPRE        "Test Point"           TopLayer    TEST_POINT_-_SIP1                          1038.386      1328.740      180      ""                                                                                                                                         
VCP         "Test Point"           TopLayer    TEST_POINT_-_SIP1                          1117.126      1205.709      90       ""                                                                                                                                         
VB          "Test Point"           TopLayer    TEST_POINT_-_SIP1                          1348.425      1353.347      270      ""                                                                                                                                         
VANA        "Test Point"           TopLayer    TEST_POINT_-_SIP1                          905.512       1555.118      270      ""                                                                                                                                         
V5V         "Test Point"           TopLayer    TEST_POINT_-_SIP1                          759.055       809.449       0        ""                                                                                                                                         
R67         RC0603FR-071RL         TopLayer    R0603-RS                                   1235.236      1456.693      0        "Res General Purpose Thick Film 0603 1 Ohm 1% 1/10W ±200ppm/°C Molded SMD Paper T/R"                                                       
R44_NTCE    RCC120610K0FKEA        TopLayer    R1206-RS                                   1441.929      866.142       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCD    RCC120610K0FKEA        TopLayer    R1206-RS                                   1811.024      866.142       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R44_NTCC    RCC120610K0FKEA        TopLayer    R1206-RS                                   2189.961      866.142       180      "Res, 10K, 1%, 0.5W, 1206, Thick Film;"                                                                                                    
R43_NTCE    ERJ-P06J332V           TopLayer    R0805-RS                                   1491.142      1092.520      180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCD    ERJ-P06J332V           TopLayer    R0805-RS                                   1870.079      1092.520      180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R43_NTCC    ERJ-P06J332V           TopLayer    R0805-RS                                   2244.095      1092.520      180      "Res Thick Film 0805 3.3K Ohm 5% 0.25W ±200ppm/°C Molded SMD Punched Carrier T/R"                                                          
R42         12R                    BottomLayer R0805-RS                                   2317.913      1476.378      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R41         12R                    BottomLayer R0805-RS                                   2911.461      1588.747      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R40         12R                    BottomLayer R0805-RS                                   2911.461      1656.825      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R39         12R                    BottomLayer R0805-RS                                   2911.461      1724.902      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R38         12R                    BottomLayer R0805-RS                                   2911.461      1792.979      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R37         12R                    BottomLayer R0805-RS                                   2911.461      1861.057      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R36         12R                    BottomLayer R0805-RS                                   2911.461      1929.134      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R35         12R                    BottomLayer R0805-RS                                   2911.461      1997.212      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R34         12R                    BottomLayer R0805-RS                                   2911.461      2065.289      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R33         12R                    BottomLayer R0805-RS                                   2911.461      2133.366      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R32         12R                    BottomLayer R0805-RS                                   2911.461      2201.444      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R31         12R                    BottomLayer R0805-RS                                   2911.461      2269.521      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R30         12R                    BottomLayer R0805-RS                                   2911.461      2337.599      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R29         12R                    BottomLayer R0805-RS                                   2911.461      2405.676      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R28         12R                    BottomLayer R0805-RS                                   2911.461      2473.753      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R27         12R                    BottomLayer R0805-RS                                   2911.461      2541.831      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R26         12R                    BottomLayer R0805-RS                                   2911.461      2609.908      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R25         12R                    BottomLayer R0805-RS                                   2911.461      2677.986      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R24         12R                    BottomLayer R0805-RS                                   2911.461      2746.063      180      "Thick Film Resistors - SMD 0.5W 12ohm 1% AEC-Q200"                                                                                        
R14         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2864.173      2057.087      180      ""                                                                                                                                         
R13         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2378.937      1856.875      180      ""                                                                                                                                         
R12         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2378.937      1955.300      180      ""                                                                                                                                         
R11         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2378.937      2058.646      180      ""                                                                                                                                         
R10         SG73P1JTTD2400F        TopLayer    R0603-RS                                   2378.937      2161.993      180      ""                                                                                                                                         
R9          SG73P1JTTD2400F        TopLayer    R0603-RS                                   2255.905      2344.079      180      ""                                                                                                                                         
R8          SG73P1JTTD2400F        TopLayer    R0603-RS                                   1825.787      2637.795      270      ""                                                                                                                                         
R7          SG73P1JTTD2400F        TopLayer    R0603-RS                                   1589.567      2637.795      270      ""                                                                                                                                         
R6          SG73P1JTTD2400F        TopLayer    R0603-RS                                   1323.819      2637.795      270      ""                                                                                                                                         
R5          SG73P1JTTD2400F        TopLayer    R0603-RS                                   1107.284      2637.795      270      ""                                                                                                                                         
R4          SG73P1JTTD2400F        TopLayer    R0603-RS                                   885.827       2582.677      270      ""                                                                                                                                         
R3          SG73P1JTTD2400F        TopLayer    R0603-RS                                   432.233       2014.764      0        ""                                                                                                                                         
R2          SG73P1JTTD2400F        TopLayer    R0603-RS                                   433.071       1960.630      0        ""                                                                                                                                         
L1          VLS3015CX-470M-H       TopLayer    VLS3015CX                                  1269.685      1574.803      0        "3.0Mm X 3.0Mm, -40 To +125 Deg C, 47 uH, 1392M / Tape And Reel Rohs Compliant: Yes"                                                       
JC18        Jumper                 TopLayer    SIP2                                       2480.315      1426.378      270      ""                                                                                                                                         
J_ISOLP     "Solder Jumoer"        TopLayer    R0603-RS                                   -52.165       1039.370      270      ""                                                                                                                                         
J_ISOLM     "Solder Jumoer"        TopLayer    R0603-RS                                   -259.842      1039.370      270      ""                                                                                                                                         
J_ISOHP     "Solder Jumoer"        TopLayer    R0603-RS                                   -281.506      1864.173      90       ""                                                                                                                                         
J_ISOHM     "Solder Jumoer"        TopLayer    R0603-RS                                   -68.888       1864.173      90       ""                                                                                                                                         
J3          "Solder Jumoer_1"      BottomLayer JUMP_A_SALDARE_TRIPLO_-_0805               2161.417      235.236       90       Resistor                                                                                                                                   
D3          BAS19LT1G              TopLayer    SOT-23-RS                                  1444.882      1570.866      0        "BAS19LT1G - High-speed switching diode"                                                                                                   
D2          BAV99-QVL              TopLayer    SOT-23-RS                                  1205.709      1353.346      270      "BAV99-Q - High-speed switching diode"                                                                                                     
C109        C0603C104J4RAC3190     BottomLayer C0603-C                                    1845.472      1550.197      180      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C102        C0603C104J4RAC3190     TopLayer    C0603-C                                    2790.354      1683.071      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C100        C0603C104J4RAC3190     TopLayer    C0603-C                                    2790.354      1791.339      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C93         C0603C104J4RAC3190     TopLayer    C0603-C                                    2347.441      1766.732      270      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C92         12101C475K4T2A         TopLayer    C1210-B                                    1086.614      1570.866      180      "1210 100V X7R 4.7uF 10% automotive grade multilayer ceramic capacitor"                                                                    
C91         CL21B103KCANNNC        TopLayer    C0805-B                                    1358.268      1456.693      0        "CL21 Series 10 nF 100 V ±10% Tolerance X7R SMT Multilayer Ceramic Capacitor"                                                              
C_ESD_NTCE  C0603X682M1RECAUTO     TopLayer    C0603-B                                    1466.536      989.173       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCD  C0603X682M1RECAUTO     TopLayer    C0603-B                                    1840.551      989.173       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_ESD_NTCC  C0603X682M1RECAUTO     TopLayer    C0603-B                                    2219.488      994.095       270      "Cap Cer 0603 6.8nF 100V X7R 4K 7" Reel"                                                                                                   
C_FIL_NTCE  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    1540.354      989.173       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCD  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    1914.370      989.173       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C_FIL_NTCC  CGA3E3X7S2A104M080AB   TopLayer    C0603-B                                    2293.307      994.095       270      "Cap Ceramic 0.1uF 100V X7S 20% Pad SMD 0603 125C Automotive T/R"                                                                          
C84         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      1681.102      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C83         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      1759.843      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C82         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      1760.335      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C81         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      1839.075      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C80         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      1839.567      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C79         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      1918.307      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C78         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      1918.799      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C77         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      1997.539      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C76         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      1998.031      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C75         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      2076.771      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C74         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3129.921      2057.087      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C73         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      2156.003      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C72         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3129.921      2155.512      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C71         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      2235.236      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C70         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      2235.728      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C69         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      2314.468      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C68         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      2314.960      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C67         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      2393.700      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C66         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      2394.192      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C65         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      2472.932      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C63         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3128.981      2473.424      180      "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C62         CGA3E3X7S2A473K080AB   BottomLayer C0603-C                                    3384.886      2552.165      0        "Multilayer Ceramic Capacitor, 0.022 uF, 100 V, ± 10%, X7R, 0603 [1608 Metric]"                                                            
C55         C0603C683J4RACTU       BottomLayer C0603-c                                    1786.853      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C54         C0603C683J4RACTU       BottomLayer C0603-c                                    1677.000      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C53         C0603C683J4RACTU       BottomLayer C0603-c                                    1567.147      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C52         C0603C683J4RACTU       BottomLayer C0603-c                                    1457.294      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C51         C0603C683J4RACTU       BottomLayer C0603-c                                    1347.441      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C50         C0603C683J4RACTU       BottomLayer C0603-c                                    1237.588      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C49         C0603C683J4RACTU       BottomLayer C0603-c                                    1127.735      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C48         C0603C683J4RACTU       BottomLayer C0603-c                                    1017.882      2291.482      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C47         C0603C683J4RACTU       BottomLayer C0603-c                                    1018.701      2230.492      0        "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C46         C0603C683J4RACTU       BottomLayer C0603-c                                    1015.748      2170.364      0        "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C45         C0603C683J4RACTU       BottomLayer C0603-c                                    1015.748      2110.236      180      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C44         C0603C683J4RACTU       BottomLayer C0603-c                                    929.134       2090.551      270      "Cap Ceramic 0.068uF 16V X7R  SMD 0603"                                                                                                    
C35         C0603C104J4RAC3190     TopLayer    C0603-C                                    1796.260      2553.150      0        "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C34         C0603C104J4RAC3190     TopLayer    C0603-C                                    1555.118      2553.150      0        "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C32         C0603C104J4RAC3190     TopLayer    C0603-C                                    1309.055      2558.071      0        "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C30         C0603C104J4RAC3190     TopLayer    C0603-C                                    1067.913      2558.071      0        "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C28         C0603C104J4RAC3190     TopLayer    C0603-C                                    531.496       2166.063      180      "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C26         C0603C104J4RAC3190     TopLayer    C0603-C                                    520.815       1990.689      90       "Cap Cer 0.1UF 16V X7R 0603"                                                                                                               
C24         ""                     TopLayer    C0805-B                                    442.075       1891.191      180      "Cap Cer 0805 100NF 16V X7R 5%"                                                                                                            
C23         CGA4J3X7T2E104M125AA   BottomLayer C0805-B                                    1452.756      1606.299      0        "Cap Ceramic 0.1uF 250V X7T 20% SMD 0805 125°C Blister Plastic T/R"                                                                        
C22         CGA9P3X7T2E225M250KA   BottomLayer C2220-B                                    1525.591      1451.772      0        "Cap Ceramic 2.2uF 250V X7T 20% SMD 5.7 x 5.0 mm 125 C Plastic T/R"                                                                        
C21         CGA3E3X7R1E474K080AB   TopLayer    C0603-B                                    1212.598      1748.032      90       "Cap Ceramic 470nF 25V X7R 10% Pad SMD 0603 +125°C Automotive T/R"                                                                         
C20         TMK107AB7105KAHT       TopLayer    C0603-C                                    1133.858      1736.220      90       None                                                                                                                                       
