Altium Designer Pick and Place Locations
C:\Users\buldoant\OneDrive - STMicroelectronics\Desktop\EVL9965A\PromoT\GERBER_FILE EVL99BM2T\Pick Place\Pick Place for EVL9965T(EVL99BM2T R.0.0).txt

========================================================================================================================
File Design Information:

Date:       19/12/25
Time:       16:24
Revision:   Not in VersionControl
Variant:    EVL99BM2T R.0.0
Units used: mil

Designator    Comment                        Layer    Footprint                           Center-X(mil) Center-Y(mil) Rotation Description                                                                                                                 
GND2          GND                            TopLayer TP-BIG-SLOT-HOLE                    2520.669      504.921       0        "PCB test point - Raised Loops - Oriented as pad on TOP"                                                                    
GND1          GND                            TopLayer TP-BIG-SLOT-HOLE                    2467.520      2329.724      0        "PCB test point - Raised Loops - Oriented as pad on TOP"                                                                    
LogST         "LOGO ST SERIGRAFIA"           TopLayer LOGO_ST_PICCOLO_-_NO_LIFE_AUGMENTED 0.000         0.000         90       "LOGO ST SERIGRAFIA"                                                                                                        
LogST2        "LOGO ST SERIGRAFIA"           TopLayer LOGO_ST_PICCOLO_-_NO_LIFE_AUGMENTED 0.000         0.000         90       "LOGO ST SERIGRAFIA"                                                                                                        
"Log Riciclo" "LOGO RICICLO"                 TopLayer LOGO_CHINA_ROHS_10                  0.000         0.000         0        "LOGO RICICLO"                                                                                                              
"LOGO RoHS"   "LOGO RoHS"                    TopLayer LOGO_RoHS_-_3                       0.000         0.000         0        "LOGO RoHS"                                                                                                                 
"LOGO RAEE"   "LOGO RAEE"                    TopLayer LOGO_CESTINO                        0.000         0.000         0        "LOGO RAEE"                                                                                                                 
FidT4         Fiducial                       TopLayer Fiducial_1mm                        3315.000      185.000       0        "Fiducial 1mm"                                                                                                              
FidT3         Fiducial                       TopLayer Fiducial_1mm                        3300.000      2590.000      0        "Fiducial 1mm"                                                                                                              
FidT2         Fiducial                       TopLayer Fiducial_1mm                        1455.000      2405.000      0        "Fiducial 1mm"                                                                                                              
FidT1         Fiducial                       TopLayer Fiducial_1mm                        1285.000      360.000       0        "Fiducial 1mm"                                                                                                              
R15           RCS0603100KFKEA                TopLayer RESC1608X50N                        2485.000      1045.000      180      Resistor                                                                                                                    
R14           RCS0603100KFKEA                TopLayer RESC1608X50N                        2255.000      1050.000      0        Resistor                                                                                                                    
R13           RCS0603100KFKEA                TopLayer RESC1608X50N                        2125.591      2455.000      180      Resistor                                                                                                                    
R12           RCS0603100KFKEA                TopLayer RESC1608X50N                        2070.866      1960.630      180      Resistor                                                                                                                    
VBAT1         MSTB2                          TopLayer MORS-2P-P381-MALE                   350.000       2555.000      270      "Terminal box 2 poles male 90° (See Mech Part)"                                                                             
EMIF          EMIF04-0410M8Y                 TopLayer 8QFN_2X1.5_0.5_EP                   2920.000      1380.000      270      "Automotive isolated communication port interface for L9965"                                                                
L9965T        L99BM2T                        TopLayer 32_LQFP                             2355.000      1355.000      180      "Device UR1T/L9965T LQFP32(5V) - Supplied by ST"                                                                            
T2            ESMIT-4180_C                   TopLayer ESMIT-4180_C                        3080.395      874.410       180      "Telecom Transformer 3750Vrms 250mOhm Prim. 250mOhm Sec. DCR 4-Pin SMD"                                                     
T1            ESMIT-4180_C                   TopLayer ESMIT-4180_C                        3080.000      1889.134      0        "Telecom Transformer 3750Vrms 250mOhm Prim. 250mOhm Sec. DCR 4-Pin SMD"                                                     
STM2          Open                           TopLayer JP2_SMD                             2395.000      353.750       90       "Circuit Breaker 0603 - NOT MOUNTED"                                                                                        
STM1          Open                           TopLayer JP2_SMD                             1625.000      50.000        0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                                        
SB1           Open                           TopLayer JP2_SMD                             1861.250      50.000        180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                                        
R4            RESISTOR                       TopLayer RES-0603-SMALL                      2365.000      2118.500      270      "SMD Resistor"                                                                                                              
R3            RESISTOR                       TopLayer RES-0603-SMALL                      2485.000      2118.500      270      "SMD Resistor"                                                                                                              
R8            RCS0603100KFKEA                TopLayer RESC1608X50N                        2660.000      1355.000      180      Resistor                                                                                                                    
R5            RCS0603100KFKEA                TopLayer RESC1608X50N                        2007.835      1375.748      0        Resistor                                                                                                                    
R7            RESISTOR                       TopLayer RES-0603-SMALL                      2485.000      665.000       90       "SMD Resistor"                                                                                                              
R6            RESISTOR                       TopLayer RES-0603-SMALL                      2365.000      665.000       90       "SMD Resistor"                                                                                                              
R1            CRCW0402267KFKED               TopLayer RESC1005X40N                        945.000       2190.000      180      Resistor                                                                                                                    
R2            CRCW0402267KFKED               TopLayer RESC1005X40N                        985.000       2700.000      0        Resistor                                                                                                                    
R9            100                            TopLayer 0603_R                              1845.000      997.500       270      "SMD Chip Resistor, 100 ohm, ï¿½ 0.1%, 125 mW, 0603 [1608 Metric], Thin Film, High Stability"                               
R10           ERJ-P06D1200V                  TopLayer ERJP06D1000V                        1405.000      470.000       270      "Res Thick Film 0805 120 Ohm 0.5% 0.25W ±100ppm/°C Molded SMD Punched Carrier T/R"                                          
R11           100                            TopLayer 0603_R                              1655.000      997.500       270      "SMD Chip Resistor, 100 ohm, ï¿½ 0.1%, 125 mW, 0603 [1608 Metric], Thin Film, High Stability"                               
Q2            MOSN                           TopLayer SOT23_GSD_T                         2348.031      1823.500      90       "SMD N-ch Mosfet"                                                                                                           
Q3            MOSN                           TopLayer SOT23_GSD_T                         2360.000      948.032       180      "SMD N-ch Mosfet"                                                                                                           
Q1            MOSN                           TopLayer SOT23_GSD_T                         2485.000      1829.327      0        "SMD N-ch Mosfet"                                                                                                           
Q4            MOSN                           TopLayer SOT23_GSD_T                         2501.968      955.000       270      "SMD N-ch Mosfet"                                                                                                           
LED_FLT0      LED                            TopLayer LED_SMD_0805_RED                    2365.000      1988.500      90       "SMD Led Diode Red 640nm 100mcd"                                                                                            
LED_FLT1      LED                            TopLayer LED_SMD_0805_RED                    2485.984      795.000       270      "SMD Led Diode Red 640nm 100mcd"                                                                                            
LED_BNE0      LED                            TopLayer LED_SMD_0805_GREEN                  2485.000      1988.500      90       "SMD Led Diode Green 570nm 50mcd"                                                                                           
LED_BNE1      LED                            TopLayer LED_SMD_0805_GREEN                  2365.984      795.000       270      "SMD Led Diode Green 570nm 50mcd"                                                                                           
JVCC          Open                           TopLayer JP2_SMD                             1165.354      2446.850      0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                                        
J_ISO1P       "NC (Normally closed)"         TopLayer JP_SMD-2-OPEN-SMALL                 3195.000      1205.512      90       "Jumper_SMD MEDIUM - NC (Normally closed)"                                                                                  
J_ISO1M       "NC (Normally closed)"         TopLayer JP_SMD-2-OPEN-SMALL                 2960.000      1205.512      90       "Jumper_SMD MEDIUM - NC (Normally closed)"                                                                                  
J_ISO0P       "NC (Normally closed)"         TopLayer JP_SMD-2-OPEN-SMALL                 2960.000      1555.000      270      "Jumper_SMD MEDIUM - NC (Normally closed)"                                                                                  
J_ISO0M       "NC (Normally closed)"         TopLayer JP_SMD-2-OPEN-SMALL                 3195.000      1555.000      270      "Jumper_SMD MEDIUM - NC (Normally closed)"                                                                                  
JSCK1         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        1820.000      1744.155      0        Resistor                                                                                                                    
JSIN1         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        1820.000      2115.000      0        Resistor                                                                                                                    
JCAN_EN       "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2027.008      415.000       0        Resistor                                                                                                                    
JFLT0         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2065.000      2365.000      180      Resistor                                                                                                                    
ISO0          ISO1                           TopLayer CONN_MOLEX_705510001                3054.921      2290.000      270      "Molex Connector 70551 Series 90° 2,54mm pitch"                                                                             
ISO1          ISO1                           TopLayer CONN_MOLEX_705510001                3044.921      480.000       270      "Molex Connector 70551 Series 90° 2,54mm pitch"                                                                             
JBNE0         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2065.000      1864.745      180      Resistor                                                                                                                    
JCAN_TX       "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2027.008      565.000       0        Resistor                                                                                                                    
JCAN_RX       "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2027.008      700.000       0        Resistor                                                                                                                    
JBNE1         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        1820.000      1864.745      180      Resistor                                                                                                                    
JSOUT0        "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2065.000      2235.000      0        Resistor                                                                                                                    
J1            "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        762.008       2705.000      180      Resistor                                                                                                                    
JNCS1         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        1820.000      1995.000      0        Resistor                                                                                                                    
JFLT1         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        1820.000      2365.000      0        Resistor                                                                                                                    
JSCK0         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2065.000      1744.155      180      Resistor                                                                                                                    
JSIN0         "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        2065.000      2115.000      0        Resistor                                                                                                                    
JSOUT1        "Solder Jumoer_1"              TopLayer JUMP_A_SALDARE_TRIPLO_-_0805        1820.000      2235.000      0        Resistor                                                                                                                    
IC2           TJA1057GT_3                    TopLayer SOIC127P600X175-8N                  1745.000      795.000       270      "TJA1057 Series 5.25V Surface Mount High-Speed CAN Transceiver - SOIC-8"                                                    
IC1           L99VR02XP                      TopLayer SOP50P1030X245-37N                  873.268       2438.976      90       "Integrated Circuit"                                                                                                        
DS1           SCHOTTKY                       TopLayer SMA                                 275.000       2255.000      0        "SMD Power Schottky Rectifier"                                                                                              
D1            ESDCAN03-2BWY                  TopLayer SOT65P210X110-3N                    1305.000      475.000       180      "ESD Suppressor TVS Dual Bi-Dir ï¿½30kV@Air Gap/ï¿½30kV@Contact Disc 3-Pin SOT-323 T/R"                                     
CN10          "Header 19X2 Female"           TopLayer STRIP-19X2-M-V                      2294.882      2583.465      0        "Female Strip SAMTEC SSW, Dual row, vertical - With long Square terminal pin - Do not cut the soldered terminal - See Note" 
CN7           "Header 19X2 Female"           TopLayer STRIP-19X2-M-V                      2294.882      183.465       0        "Female Strip SAMTEC SSW, Dual row, vertical - With long Square terminal pin - Do not cut the soldered terminal - See Note" 
CMC_H1        "NM 100uH ACT45B-101-2P-TL003" TopLayer CHOKE                               1587.500      470.000       270      "Common Mode Chokes Dual 100uH 5.8kOhm 100kHz 0.15A 2Ohm DCR SMD Automotive T/R"                                            
CMC_1         "NM 100uH ACT45B-101-2P-TL003" TopLayer ACT45B_TDK_IND                      3080.000      1559.055      270      "Common Mode Chokes Dual 100uH 5.8kOhm 100kHz 0.15A 2Ohm DCR SMD Automotive T/R"                                            
CMC_2         "NM 100uH ACT45B-101-2P-TL003" TopLayer ACT45B_TDK_IND                      3080.000      1205.000      90       "Common Mode Chokes Dual 100uH 5.8kOhm 100kHz 0.15A 2Ohm DCR SMD Automotive T/R"                                            
C18           2.2uF                          TopLayer 0603_C                              2540.335      1525.748      180      "Cap Ceramic 2.2uF 50V X5R 10% Pad SMD 0603 85C T/R"                                                                        
C12           2.2uF                          TopLayer 0603_C                              2160.335      1550.748      180      "Cap Ceramic 2.2uF 50V X5R 10% Pad SMD 0603 85C T/R"                                                                        
C22           VJ0402Y103KCAAC                TopLayer CAPC1005X61N                        2627.835      1250.748      270      "Cap Ceramic 0.01uF 50V X7R 10% Pad SMD 0402 125°C T/R"                                                                     
C13           VJ0402Y103KCAAC                TopLayer CAPC1005X61N                        2075.000      1455.000      90       "Cap Ceramic 0.01uF 50V X7R 10% Pad SMD 0402 125°C T/R"                                                                     
C23           100nF                          TopLayer 0603_C                              2672.835      1238.248      90       MAJCU168BB7104KTEA01                                                                                                        
C24           2.2uF                          TopLayer 0603_C                              2717.835      1238.248      90       "Cap Ceramic 2.2uF 50V X5R 10% Pad SMD 0603 85C T/R"                                                                        
C17           100nF                          TopLayer 0603_C                              2540.335      1570.748      180      MAJCU168BB7104KTEA01                                                                                                        
C20           100nF                          TopLayer 0603_C                              2550.334      1155.748      0        MAJCU168BB7104KTEA01                                                                                                        
C27           2.2uF                          TopLayer 0603_C                              2170.335      1150.748      0        "Cap Ceramic 2.2uF 50V X5R 10% Pad SMD 0603 85C T/R"                                                                        
C11           100nF                          TopLayer 0603_C                              2160.335      1505.748      180      MAJCU168BB7104KTEA01                                                                                                        
C21           2.2uF                          TopLayer 0603_C                              2550.335      1205.748      0        "Cap Ceramic 2.2uF 50V X5R 10% Pad SMD 0603 85C T/R"                                                                        
C26           100nF                          TopLayer 0603_C                              2170.335      1200.748      0        MAJCU168BB7104KTEA01                                                                                                        
C7            KGM31AR71H475KU                TopLayer CAPC3216X180N                       1210.000      2260.000      0        Capacitor                                                                                                                   
C2            GCM31CD71H106KE36K             TopLayer GCM31C5C2E183FX03L                  545.000       2605.000      180      Capacitor                                                                                                                   
C6            KGM31AR71H475KU                TopLayer CAPC3216X180N                       545.000       2430.000      180      Capacitor                                                                                                                   
C8            GCM31CD71H106KE36K             TopLayer GCM31C5C2E183FX03L                  1210.000      2340.000      0        Capacitor                                                                                                                   
C10           GCM31CD71H106KE36K             TopLayer GCM31C5C2E183FX03L                  1210.000      2515.000      0        Capacitor                                                                                                                   
C9            KGM31AR71H475KU                TopLayer CAPC3216X180N                       1210.000      2600.000      0        Capacitor                                                                                                                   
C5            GCM31CD71H106KE36K             TopLayer GCM31C5C2E183FX03L                  545.000       2350.000      180      Capacitor                                                                                                                   
C4            VJ0603Y104JXAAC                TopLayer CAPC1608X97N                        576.772       2285.433      180      Capacitor                                                                                                                   
C31           C0603C104K1RACTU               TopLayer CAP-0603-SMALL                      1635.000      610.000       0        "Cap Cer 0603 0.1UF 100VDC X7R"                                                                                             
C30           C0603C104K1RACTU               TopLayer CAP-0603-SMALL                      1750.000      975.000       180      "Cap Cer 0603 0.1UF 100VDC X7R"                                                                                             
C15           2.2uF                          TopLayer 0603_C                              1987.835      1468.248      270      "Cap Ceramic 2.2uF 50V X5R 10% Pad SMD 0603 85C T/R"                                                                        
C14           100nF                          TopLayer 0603_C                              2032.835      1468.248      270      MAJCU168BB7104KTEA01                                                                                                        
C1            KGM31AR71H475KU                TopLayer CAPC3216X180N                       545.000       2525.000      180      Capacitor                                                                                                                   
C3            VJ0603Y104JXAAC                TopLayer CAPC1608X97N                        569.038       2668.180      180      Capacitor                                                                                                                   
C29           GRM1885C2A470GA01J             TopLayer CAPC1608X90N                        535.000       535.000       0        "Cap Ceramic 47pF 100V C0G 2% SMD 0603 125°C Paper T/R"                                                                     
C32           GRM1885C2A470GA01J             TopLayer CAPC1608X90N                        645.000       535.000       180      "Cap Ceramic 47pF 100V C0G 2% SMD 0603 125°C Paper T/R"                                                                     
