Altium Designer Pick and Place Locations
C:\Users\Gasnot Jordane\Documents\Projets\ATE\STM_Le Mans\Projets\MB1242B\BASE\MB1242B\02-Manufacturing\MB1242B_PCB\Assembly\MB1242B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       06/02/20
Time:       17:18
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment           Layer       Footprint                        Center-X(mm) Center-Y(mm) Rotation Description                                                                                
SHEETBOX1  Comment           TopLayer    Sheetbox_4L2S                    30.0931      -17.1484     0        ""                                                                                         
C1         Capacitor         TopLayer    C0402                            14.7500      13.7500      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C2         Capacitor         TopLayer    C0402                            18.2500      20.2500      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C3         Capacitor         TopLayer    C0402                            22.0000      11.0000      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
CN1        "Header 10x2"     BottomLayer CON_SAMTEC_ERM8-010-020-L-DV-TR  6.7500       13.0000      90       "HEADER High speed, 10x2, 0.8mm, VR, SMT, Height 5.97mm"                                   
CN2        "Header 10x2"     BottomLayer CON_SAMTEC_ERM8-010-020-L-DV-TR  32.7501      13.0000      90       "HEADER High speed, 10x2, 0.8mm, VR, SMT, Height 5.97mm"                                   
CN3        "Socket 10x2"     TopLayer    CON_SAMTEC_ERF8-010-050-L-DV-TR  4.8500       13.0000      270      "SOCKET High Speed, 10x2, 0.8mm, VR, SMT, Height 5.1 mm"                                   
CN4        "Socket 10x2"     TopLayer    CON_SAMTEC_ERF8-010-050-L-DV-TR  30.8501      13.0000      270      "SOCKET High Speed, 10x2, 0.8mm, VR, SMT, Height 5.1 mm"                                   
R1         Resistor          TopLayer    R0603                            24.5001      11.0000      270      Resistor,4K7,0603,1%,1/10W                                                                 
R2         Resistor          TopLayer    R0603                            26.0001      19.2500      90       Resistor,4K7,0603,1%,1/10W                                                                 
R3         Resistor          TopLayer    R0603                            26.0001      15.5000      90       Resistor,4K7,0603,1%,1/10W                                                                 
R4         Resistor          TopLayer    R0603                            12.0000      17.5000      360      Resistor,0R,0603,5%,1/10W                                                                  
R5         Resistor          TopLayer    R0603                            12.0000      19.5000      360      Resistor,0R,0603,5%,1/10W                                                                  
R6         Resistor          TopLayer    R0603                            32.0002      22.5252      180      Resistor,0R,0603,5%,1/10W                                                                  
R7         Resistor          TopLayer    R0603                            29.3502      22.5252      180      Resistor,4K7,0603,1%,1/10W                                                                 
R8         Resistor          TopLayer    R0603                            29.3502      21.1001      360      Resistor,4K7,0603,1%,1/10W                                                                 
U1         S26KS512SDPBHV020 TopLayer    ICC_FBGA24_5X5-BALL-ARRAY_6X8_P1 20.5000      15.7500      270      "Memory, HyperFlash, OctalSPI, 512Mb, up to 166MHz@1V8, 100MHz@3V0, CS and RWDS supported" 
SW1        SWITCH_2WAY       TopLayer    SWI_MULTICOMP_MCDHN-02F-V_4P     14.5000      9.0000       270      "DIP Switch Slide Type x2 poles 25mA 24VDC 100mR SMD"                                      
SW2        SWITCH_2WAY       TopLayer    SWI_MULTICOMP_MCDHN-02F-V_4P     14.5000      3.9999       270      "DIP Switch Slide Type x2 poles 25mA 24VDC 100mR SMD"                                      
MIRE1      Comment           BottomLayer MIRE_PLACE_SMD_0P8MM             34.0000      22.5500      180      ""                                                                                         
MIRE2      Comment           BottomLayer MIRE_PLACE_SMD_0P8MM             3.5250       3.2500       180      ""                                                                                         
MIRE3      Comment           TopLayer    MIRE_PLACE_SMD_0P8MM             3.0000       22.7500      0        ""                                                                                         
MIRE4      Comment           TopLayer    MIRE_PLACE_SMD_0P8MM             34.2501      3.5000       0        ""                                                                                         
