Altium Designer Pick and Place Locations
C:\Data\derouet\ST\MDG\MB1297\IoT1.5\02-Manufacturing\MB1297 revEBoard_PCB_Revision_PCB\Assembly\MB1297 revEBoard_PCB_Revision_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       03-04-20
Time:       15:14
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                       Layer       Footprint                             Center-X(mm) Center-Y(mm) Rotation Description                                                                               
M3         "Not Fitted (SPSGRF)"         TopLayer    SPSGRF                                77.7118      43.5976      270      "SPSGRF-915or SPSGRF-868"                                                                 
R13        0R                            TopLayer    0402                                  56.7234      22.8394      90       Resistor                                                                                  
R6         0R                            TopLayer    0402                                  57.7394      25.3286      90       Resistor                                                                                  
TP9        Comment                       BottomLayer LOGO_CE                               -278.1248    -200.7568    180      ""                                                                                        
C76        2.2uF                         BottomLayer 0603_CAP_NPOL                         10.6732      27.5130      180      "Capacitor_not polarized"                                                                 
C75        2.2uF                         BottomLayer 0603_CAP_NPOL                         10.6478      46.7408      360      "Capacitor_not polarized"                                                                 
Logo_ST    Comment                       TopLayer    LOGO_ST_Size3                         -278.1248    -200.7568    0        ""                                                                                        
U10        MP34DT01-M                    TopLayer    HCLGA-4LD_3x4x1                       76.8402      22.2656      90       "MEMS audio microphone"                                                                   
C74        100nF                         TopLayer    0402                                  74.2250      21.9000      90       "Capacitor_not polarized"                                                                 
C46        10uF                          TopLayer    0603_CAP_NPOL                         72.8524      22.4076      90       "Capacitor_not polarized"                                                                 
U21        TSV631AILT                    TopLayer    SOT23-5                               44.4552      42.5244      90       "TSV631AILT  Rail-to-rail input/output, 60 ľA, 880 kHz, 5 V CMOS  operational amplifiers" 
M1         "BT Module"                   TopLayer    SPBTLE-RF                             77.7118      11.5936      270      SPBTLE-RF                                                                                 
CN10       HEADER_2X6_PMOD               TopLayer    Header_F_2x6x2.54_TH_H_PMOD           23.6526      8.0312       180      "PMOD Connector Warning Specific Pinout"                                                  
CN4        "Header 6X1_Female_SMD"       TopLayer    F-V50XC-1X06R-LF                      64.7762      -0.2188      180      "Header, 6-Pin, SMD, Single row,female"                                                   
CN3        "Header 8X1_Female_SMD"       TopLayer    F-V50XC-1X08R-LF                      62.2362      47.9112      360      "Header, 8-Pin, SMD, Single row,female"                                                   
CN2        "Header 8X1_Female_SMD"       TopLayer    F-V50XC-1X08R-LF                      44.4562      -0.3488      180      "Header, 8-Pin, SMD, Single row,female"                                                   
CN1        "Header 10X1_Female_SMD"      TopLayer    F-V50XC-1X10R-LF                      37.8522      47.9112      360      "Header, 10-Pin, SMD, Single row,female"                                                  
X3         NX3225GD-8.00M                TopLayer    CRY_NX3225GD_2P                       67.3406      25.3793      180      "Crystal 8Mhz, 8pF, -+50PPM, SMD"                                                         
X2         NX3215SA-32.768K              TopLayer    CRY_NX3215SA_2P                       40.8992      16.1592      360      "Crystal 32.768kHz, 6pF, -+20PPM, R=50K, SMD"                                             
X1         "Not Fitted (NX3225GD-8.00M)" TopLayer    CRY_NX3225GD_2P                       44.7346      15.1686      180      "Crystal 8Mhz, 8pF, -+50PPM, SMD"                                                         
SB21       Close                         BottomLayer SB                                    22.0524      11.7912      270      "Solder Jumper"                                                                           
SB20       Open                          BottomLayer SB                                    26.2108      11.7912      270      "Solder Jumper"                                                                           
SB19       Open                          BottomLayer SB                                    31.5520      11.9008      90       "Solder Jumper"                                                                           
SB18       Close                         BottomLayer SB                                    24.8246      11.8912      90       "Solder Jumper"                                                                           
SB17       Close                         BottomLayer SB                                    38.3346      18.1912      180      "Solder Jumper"                                                                           
SB16       Open                          BottomLayer SB                                    23.4385      11.8658      90       "Solder Jumper"                                                                           
SB15       Close                         BottomLayer SB                                    27.5969      11.8912      90       "Solder Jumper"                                                                           
SB14       Close                         BottomLayer SB                                    30.2820      11.8968      90       "Solder Jumper"                                                                           
SB13       Close                         BottomLayer SB                                    39.2490      27.6908      180      "Solder Jumper"                                                                           
SB12       Open                          BottomLayer SB                                    28.9830      11.8912      90       "Solder Jumper"                                                                           
SB11       Open                          BottomLayer SB                                    68.8892      43.4134      360      "Solder Jumper"                                                                           
SB10       Close                         BottomLayer SB                                    36.9122      45.5978      180      "Solder Jumper"                                                                           
SB9        Open                          BottomLayer SB                                    39.2490      26.1160      180      "Solder Jumper"                                                                           
SB8        Close                         BottomLayer SB                                    73.5898      34.8028      180      "Solder Jumper"                                                                           
SB7        Close                         BottomLayer SB                                    67.9256      40.0352      180      "Solder Jumper"                                                                           
SB6        Close                         BottomLayer SB                                    73.5644      33.1517      180      "Solder Jumper"                                                                           
SB5        Close                         BottomLayer SB                                    68.0272      37.1650      180      "Solder Jumper"                                                                           
SB4        Close                         BottomLayer SB                                    61.4978      33.8122      360      "Solder Jumper"                                                                           
SB3        Close                         BottomLayer SB                                    38.3346      19.7406      180      "Solder Jumper"                                                                           
SB2        Close                         BottomLayer SB                                    48.9756      16.5402      360      "Solder Jumper"                                                                           
SB1        Close                         BottomLayer SB                                    42.7034      42.3720      180      "Solder Jumper"                                                                           
R66        "Not Fitted (10K)"            TopLayer    0402                                  24.1860      37.3428      360      Resistor                                                                                  
R65        "Not Fitted (10K)"            TopLayer    0402                                  24.1860      38.3334      360      Resistor                                                                                  
R64        "Not Fitted (10K)"            TopLayer    0402                                  24.1750      39.3500      360      Resistor                                                                                  
R62        47K                           TopLayer    0402                                  30.5500      40.1000      270      Resistor                                                                                  
R61        0R                            TopLayer    0603_RES                              27.5134      43.1848      270      Resistor                                                                                  
R59        100K                          TopLayer    0402                                  26.8277      40.0860      90       Resistor                                                                                  
R58        47K                           TopLayer    0402                                  29.6750      40.1000      270      Resistor                                                                                  
R57        47K                           TopLayer    0402                                  27.9000      40.0750      90       Resistor                                                                                  
R56        1K                            TopLayer    0402                                  25.4000      44.9500      180      Resistor                                                                                  
R55        330R                          TopLayer    0402                                  25.4052      43.9468      180      Resistor                                                                                  
R54        100K                          TopLayer    0402                                  57.2568      43.3626      90       Resistor                                                                                  
R53        2K2                           BottomLayer 0402                                  66.1250      43.6500      360      Resistor                                                                                  
R52        1K                            BottomLayer 0402                                  73.9192      54.6783      90       Resistor                                                                                  
R51        10K                           BottomLayer 0402                                  72.1000      43.4750      270      Resistor                                                                                  
R50        1K5                           TopLayer    0402_RES                              65.0292      42.8038      360      Resistor                                                                                  
R49        100K                          BottomLayer 0402_RES                              66.2738      50.9064      90       Resistor                                                                                  
R48        10K                           TopLayer    0402                                  56.2662      43.3626      270      Resistor                                                                                  
R47        330R                          TopLayer    0402                                  76.0020      52.0748      360      Resistor                                                                                  
R46        36K                           TopLayer    0402                                  55.2248      43.3626      270      Resistor                                                                                  
R45        100R                          TopLayer    0402                                  54.1580      43.3626      90       Resistor                                                                                  
R44        330R                          TopLayer    0402                                  78.8468      52.0748      180      Resistor                                                                                  
R43        0R                            TopLayer    0402_RES                              73.5890      30.9927      360      Resistor                                                                                  
R42        0R                            TopLayer    0402_RES                              73.5890      29.9767      360      Resistor                                                                                  
R41        4K7                           TopLayer    0402                                  72.2750      28.4750      270      Resistor                                                                                  
R40        4K7                           TopLayer    0402                                  71.2750      28.4750      270      Resistor                                                                                  
R39        100R                          TopLayer    0402                                  69.7790      40.2638      180      Resistor                                                                                  
R38        200K                          TopLayer    0402                                  40.4420      42.0672      90       Resistor                                                                                  
R36        "Not Fitted (10K)"            TopLayer    0402                                  65.7912      28.1988      270      Resistor                                                                                  
R35        22R                           TopLayer    0402                                  77.5133      31.7041      180      Resistor                                                                                  
R34        22R                           TopLayer    0402                                  77.5133      26.5479      180      Resistor                                                                                  
R33        22R                           TopLayer    0402                                  77.5133      27.8687      180      Resistor                                                                                  
R32        22R                           TopLayer    0402                                  77.5133      30.3833      180      Resistor                                                                                  
R31        10K                           TopLayer    0402                                  64.8006      28.1988      270      Resistor                                                                                  
R30        "Not Fitted (0R)"             TopLayer    0402_RES                              60.9000      36.4250      360      Resistor                                                                                  
R29        100K                          TopLayer    0402                                  60.5250      33.4500      180      Resistor                                                                                  
R28        2K7                           TopLayer    0402                                  60.9000      35.4750      360      Resistor                                                                                  
R27        4K7                           TopLayer    0402                                  60.5250      34.4500      180      Resistor                                                                                  
R26        47K                           TopLayer    0402                                  7.1500       32.5000      90       Resistor                                                                                  
R25        330R                          TopLayer    0402                                  46.7250      51.6000      360      Resistor                                                                                  
R24        1K                            TopLayer    0402                                  36.3750      18.3000      270      Resistor                                                                                  
R23        100K                          TopLayer    0402                                  3.2250       37.9000      360      Resistor                                                                                  
R22        680R                          TopLayer    0402                                  78.2118      19.9946      360      Resistor                                                                                  
R21        1K                            TopLayer    0402                                  17.5820      27.3352      180      Resistor                                                                                  
R20        330R                          TopLayer    0402                                  58.5750      54.3500      360      Resistor                                                                                  
R19        1K                            TopLayer    0402                                  51.7500      13.8750      270      Resistor                                                                                  
R18        1K                            TopLayer    0402                                  58.5750      53.3500      180      Resistor                                                                                  
R16        10K                           TopLayer    0402                                  41.4326      42.0672      90       Resistor                                                                                  
R15        10K                           TopLayer    0402                                  4.6280       3.1290       270      Resistor                                                                                  
R14        10K                           TopLayer    0402                                  5.6250       3.1250       270      Resistor                                                                                  
R12        0R                            TopLayer    0402                                  41.1250      18.8000      270      Resistor                                                                                  
R11        2K2                           TopLayer    0402                                  49.8000      13.5750      90       Resistor                                                                                  
R10        2K2                           TopLayer    0402                                  48.7750      13.5750      90       Resistor                                                                                  
R9         2K2                           TopLayer    0402                                  32.6500      26.7750      0        Resistor                                                                                  
R8         2K2                           TopLayer    0402                                  32.6500      25.4186      0        Resistor                                                                                  
R7         "Not Fitted (0R)"             TopLayer    0402                                  44.9000      18.6600      270      Resistor                                                                                  
R5         "Not Fitted (0R)"             TopLayer    0402                                  43.9000      18.6500      270      Resistor                                                                                  
R4         20K                           TopLayer    0402                                  20.7500      15.4250      270      Resistor                                                                                  
R3         1K                            TopLayer    0402                                  38.0750      2.8250       180      Resistor                                                                                  
R2         0R                            BottomLayer 0402                                  30.7000      50.6000      180      Resistor                                                                                  
R1         30K                           TopLayer    0402                                  14.6750      18.2000      270      Resistor                                                                                  
M2         ISM43362-M3G-L44              TopLayer    ISM43362-M3G-L44                      15.3468      38.8160      90       "ISM43362-M3G-L44 Wifi Module 802.11 bgn"                                                 
LD9        LED                           TopLayer    0603_LED_GREEN                        27.1324      53.8782      180      "Light-Emitting Diode"                                                                    
LD8        LED                           TopLayer    0603_LED_RED                          27.1324      52.4050      180      "Light-Emitting Diode"                                                                    
LD7        LED                           TopLayer    0603_LED_RED                          74.4018      54.6910      270      "Light-Emitting Diode"                                                                    
LD6        LD_BICOLOR_CMS                TopLayer    LED_BI-GR_HSMF-A201-A00J1             77.4244      54.9704      180      "Bicolor Led"                                                                             
LD5        LED                           TopLayer    0603_LED_GREEN                        49.6368      51.5922      180      "Light-Emitting Diode"                                                                    
LD4        LED                           TopLayer    0603_LED_Blue                         80.2184      21.0614      90       "Light-Emitting Diode"                                                                    
LD3        LED                           TopLayer    0603_LED_Yellow                       14.7372      27.2336      360      "Light-Emitting Diode"                                                                    
LD2        LED                           TopLayer    0603_LED_GREEN                        61.5748      53.9544      180      "Light-Emitting Diode"                                                                    
LD1        LED                           TopLayer    0603_LED_GREEN                        55.2756      53.8528      360      "Light-Emitting Diode"                                                                    
L2         742792042                     TopLayer    0603L                                 18.9536      18.5468      270      Inductor                                                                                  
L1         FCM1608KF-601T03              TopLayer    0603L                                 48.6589      17.3276      360      Inductor                                                                                  
JP8        Jumper_2.54mm                 BottomLayer CON_SAMTEC_TSW-102-07-G-S             60.3556      25.2778      270      "Connector jumper 1 position"                                                             
JP7        Jumper_2.54mm                 BottomLayer CON_SAMTEC_TSW-102-07-G-S             24.4908      23.2752      270      "Connector jumper 1 position"                                                             
JP6        Jumper_2.54mm                 BottomLayer CON_SAMTEC_TSW-102-07-G-S             58.1204      18.8262      360      "Connector jumper 1 position"                                                             
JP5        Jumper_2.54mm                 BottomLayer CON_SAMTEC_TSW-102-07-G-S             50.9282      41.0766      360      "Connector jumper 1 position"                                                             
JP4        HEADER_2X5                    BottomLayer Header_M_2x5x2.54_TH_V                45.0902      55.5038      180      ""                                                                                        
U20        EMIF02-USB03F2                TopLayer    ESD_FLIP-CHIP-BGA11_1P44X1P94_P050    33.3046      51.7954      270      "2-line IPAD, EMI filter including ESD protection"                                        
U19        STMPS2141STR                  TopLayer    MOS_SOT23-5L                          30.3582      43.1594      270      "Enhanced single channel power switches"                                                  
U18        EMIF02-USB03F2                TopLayer    ESD_FLIP-CHIP-BGA11_1P44X1P94_P050    68.7630      51.6938      90       "2-line IPAD, EMI filter including ESD protection"                                        
U17        ST890CDR                      BottomLayer ICC_SO8_5X4_P127                      68.8392      46.7916      270      "1.2 A current limited high-side power switch with thermal shutdown"                      
U16        LD3985M33R                    BottomLayer REG_SOT23-5L                          40.9934      47.1762      90       "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible"       
U15        STM32F103CBT6                 TopLayer    ICC_LQFP48_7X7_P050                   67.2136      34.5233      360      "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"                   
U14        LD1117S33TR                   BottomLayer REG_SOT223-TAB                        60.1058      40.6194      180      "LOW DROP FIXED AND ADJUSTABLE POSITIVE VOLTAGE REGULATORS (3.3 Volts)"                   
U13        LD1117S50TR                   BottomLayer REG_SOT223-TAB                        55.2798      4.5514       180      "IC REG LDO 5V 0.8A SOT223"                                                               
U11        MX25R6435F                    TopLayer    SOP8L                                 56.1900      31.8056      90       "MX25R6435F Serial Flash Memory 64M"                                                      
U9         STSAFE-A110                   BottomLayer SOP8                                  21.0110      -0.0714      360      STSAFE-A110                                                                               
U8         ST25DV04K                     TopLayer    SOP8                                  16.3628      14.3558      0        "ST25DV04K  64K_EEPROM NFC/RFID"                                                          
U7         LPS22HB                       TopLayer    HLGA10L-2X2X0.76                      45.6744      8.5392       180      IC,Sensor                                                                                 
U6         HTS221                        TopLayer    HLGA6L-2x2x0.9                        13.2894      3.0528       360      "Humidity + Temp MEMS"                                                                    
U5         LIS3MDL                       TopLayer    VFLGA12-2x2x1                         66.3286      11.9040      0        IC,Sensor                                                                                 
U4         VL53L0X                       TopLayer    LGA12-optical                         6.6272       0.3096       360      "Proximity sensor MEMS"                                                                   
U3         LSM6DSL                       TopLayer    LGA14L-2.5X3X0.86p0.5                 39.4514      7.6502       360      "Accelero + Gyro MEMS (6 Axis)"                                                           
U2         MP34DT01-M                    TopLayer    HCLGA-4LD_3x4x1                       76.8068      1.2616       90       "MEMS audio microphone"                                                                   
U1         STM32L4S5VITx                 TopLayer    LQFP100_14x14x1.6                     43.7440      29.2656      90       STM32L4S5VITx                                                                             
D5         BAT60JFILM                    BottomLayer DIO_SOD323                            36.0168      48.7462      270      BAT60JFILM                                                                                
D4         BAT60JFILM                    BottomLayer DIO_SOD323                            34.3023      48.7462      270      BAT60JFILM                                                                                
D3         BAT60JFILM                    BottomLayer DIO_SOD323                            37.6988      48.7474      270      BAT60JFILM                                                                                
D2         BAT60JFILM                    TopLayer    DIO_SOD323                            59.9564      37.9016      360      BAT60JFILM                                                                                
CN9        475900001                     TopLayer    CON_USBMICROAB_MOLEX_47590-0001_H3    33.2284      55.2919      180      "USB-MICRO-AB, 47590-0001, SMT, MOLEX"                                                    
CN8        "Header 4 pins"               BottomLayer CON_SAMTEC_TSW-104-07-G-S             58.2474      56.3674      180      "Header, 4-Pin"                                                                           
CN7        1050170001                    TopLayer    CON_USBMICROB_MOLEX_105017-0001_H2P90 68.8900      55.1676      180      "USB-MICRO-B, 1050170001, SMT, MOLEX"                                                     
CN6        "header 2 pins 2.54mm"        BottomLayer CON_SAMTEC_TSW-102-07-G-S             67.4422      20.1724      360      "Header 2 pins"                                                                           
CN5        TC2050-IDC-NL                 TopLayer    CON_TAG-C_TC2050-IDC-NL               82.6141      27.8432      90       "Tag_Connector Header, 10-Pin, Dual row No legs"                                          
C73        100nF                         TopLayer    0402                                  42.4250      42.0672      270      "Capacitor_not polarized"                                                                 
C72        "Not Fitted"                  TopLayer    0402                                  10.9691      11.7818      270      "Capacitor_not polarized"                                                                 
C71        10pF                          TopLayer    0402                                  11.9623      11.7754      270      "Capacitor_not polarized"                                                                 
C70        "Not Fitted"                  TopLayer    0402                                  11.9250      14.3750      90       "Capacitor_not polarized"                                                                 
C69        "Not Fitted"                  TopLayer    0402                                  10.9250      17.0500      90       "Capacitor_not polarized"                                                                 
C68        1uF                           TopLayer    0402                                  16.8250      18.6500      90       "Capacitor_not polarized"                                                                 
C67        100pF                         TopLayer    0402                                  15.8000      18.6500      90       "Capacitor_not polarized"                                                                 
C66        4.7uF                         TopLayer    0603_CAP_NPOL                         33.8380      40.8226      360      "Capacitor_not polarized"                                                                 
C65        100nF                         BottomLayer 0402                                  64.6000      46.3250      270      "Capacitor_not polarized"                                                                 
C64        1uF                           BottomLayer 0402                                  71.8750      50.3750      180      "Capacitor_not polarized"                                                                 
C63        100nF                         TopLayer    0402                                  63.9806      40.1368      180      "Capacitor_not polarized"                                                                 
C62        100nF                         TopLayer    0402                                  73.0250      38.2250      360      "Capacitor_not polarized"                                                                 
C61        100nF                         TopLayer    0402                                  68.8500      28.2750      270      "Capacitor_not polarized"                                                                 
C60        100nF                         TopLayer    0402                                  63.7846      28.1987      270      "Capacitor_not polarized"                                                                 
C59        1uF                           BottomLayer 0402                                  44.3746      47.1984      360      "Capacitor_not polarized"                                                                 
C58        10nF                          BottomLayer 0402                                  43.7250      49.3250      360      "Capacitor_not polarized"                                                                 
C57        100nF                         BottomLayer 0402                                  40.4202      49.3852      360      "Capacitor_not polarized"                                                                 
C56        1uF                           BottomLayer 0402                                  40.4420      50.3984      360      "Capacitor_not polarized"                                                                 
C55        100nF                         BottomLayer 0402                                  44.3746      46.2078      360      "Capacitor_not polarized"                                                                 
C54        100nF                         TopLayer    0402                                  67.6000      28.0250      270      "Capacitor_not polarized"                                                                 
C53        10pF                          TopLayer    0402                                  11.9250      17.0500      90       "Capacitor_not polarized"                                                                 
C52        10pF                          TopLayer    0402                                  66.3500      23.3500      180      "Capacitor_not polarized"                                                                 
C51        10pF                          TopLayer    0402                                  68.3314      23.3473      360      "Capacitor_not polarized"                                                                 
C50        10uF                          BottomLayer 0603_CAP_NPOL                         13.5434      33.6344      360      "Capacitor_not polarized"                                                                 
C49        10uF                          BottomLayer 0603_CAP_NPOL                         20.3760      35.2092      270      "Capacitor_not polarized"                                                                 
C48        100nF                         TopLayer    0402                                  53.5500      37.0000      90       "Capacitor_not polarized"                                                                 
C47        100nF                         TopLayer    0402                                  10.2500      27.5250      180      "Capacitor_not polarized"                                                                 
C45        100nF                         TopLayer    0402                                  74.1736      50.0170      270      "Capacitor_not polarized"                                                                 
C44        100nF                         TopLayer    0402                                  7.2250       45.6000      270      "Capacitor_not polarized"                                                                 
C43        100nF                         TopLayer    0402                                  73.8750      18.1750      270      "Capacitor_not polarized"                                                                 
C42        100nF                         BottomLayer 0402                                  62.5654      35.1838      360      "Capacitor_not polarized"                                                                 
C41        10uF                          BottomLayer 0603_CAP_NPOL                         64.9276      38.1302      90       "Capacitor_not polarized"                                                                 
C40        10uF                          BottomLayer 0603_CAP_NPOL                         55.6566      38.0032      90       "Capacitor_not polarized"                                                                 
C39        10uF                          BottomLayer 0603_CAP_NPOL                         56.2662      -0.4778      360      "Capacitor_not polarized"                                                                 
C38        10uF                          BottomLayer 0603_CAP_NPOL                         50.6020      1.9352       90       "Capacitor_not polarized"                                                                 
C37        10pF                          TopLayer    0402                                  37.5110      18.3517      90       "Capacitor_not polarized"                                                                 
C36        100nF                         TopLayer    0402                                  35.3750      18.3000      270      "Capacitor_not polarized"                                                                 
C35        10pF                          TopLayer    0402                                  50.7500      14.1500      90       "Capacitor_not polarized"                                                                 
C34        100nF                         TopLayer    0402                                  51.7500      16.1000      90       "Capacitor_not polarized"                                                                 
C33        100nF                         BottomLayer 0402                                  16.2750      -1.0750      180      "Capacitor_not polarized"                                                                 
C32        100nF                         TopLayer    0402                                  17.8250      18.6500      90       "Capacitor_not polarized"                                                                 
C31        100nF                         TopLayer    0402                                  47.8000      8.4000       90       "Capacitor_not polarized"                                                                 
C30        4.7uF                         TopLayer    0603_CAP_NPOL                         45.8014      5.6182       180      "Capacitor_not polarized"                                                                 
C29        100nF                         TopLayer    0402                                  45.6500      6.8250       180      "Capacitor_not polarized"                                                                 
C28        100nF                         TopLayer    0402                                  13.5250      5.6500       90       "Capacitor_not polarized"                                                                 
C27        2.2uF                         TopLayer    0603_CAP_NPOL                         14.7118      5.6182       90       "Capacitor_not polarized"                                                                 
C26        100nF                         TopLayer    0402                                  67.0000      7.7500       270      "Capacitor_not polarized"                                                                 
C25        100nF                         TopLayer    0402                                  65.9000      7.7500       270      "Capacitor_not polarized"                                                                 
C24        1uF                           TopLayer    0402                                  64.7750      7.7500       270      "Capacitor_not polarized"                                                                 
C23        100nF                         TopLayer    0402                                  62.2272      11.1750      180      "Capacitor_not polarized"                                                                 
C22        100nF                         TopLayer    0402                                  9.5810       0.3096       90       "Capacitor_not polarized"                                                                 
C21        4.7uF                         TopLayer    0603_CAP_NPOL                         8.5904       -1.6970      180      "Capacitor_not polarized"                                                                 
C20        100nF                         TopLayer    0402                                  41.8500      7.4000       90       "Capacitor_not polarized"                                                                 
C19        100nF                         TopLayer    0402                                  40.0000      5.6500       360      "Capacitor_not polarized"                                                                 
C18        4.7uF                         TopLayer    0603_CAP_NPOL                         39.5784      4.4752       360      "Capacitor_not polarized"                                                                 
C17        100nF                         TopLayer    0402                                  75.4250      -1.8250      90       "Capacitor_not polarized"                                                                 
C16        10uF                          TopLayer    0603_CAP_NPOL                         77.4244      -1.0366      360      "Capacitor_not polarized"                                                                 
C15        5.1pF                         TopLayer    0402                                  41.7628      14.7114      180      "Capacitor_not polarized"                                                                 
C14        5.1pF                         TopLayer    0402                                  39.4260      14.7114      360      "Capacitor_not polarized"                                                                 
C13        100nF                         TopLayer    0402                                  33.1014      23.3220      180      "Capacitor_not polarized"                                                                 
C12        100nF                         TopLayer    0402                                  36.0250      36.9750      180      "Capacitor_not polarized"                                                                 
C11        100nF                         TopLayer    0402                                  52.6500      35.7250      90       "Capacitor_not polarized"                                                                 
C10        100nF                         TopLayer    0402                                  53.0000      23.9250      270      "Capacitor_not polarized"                                                                 
C9         100nF                         TopLayer    0402                                  42.9058      18.6484      270      "Capacitor_not polarized"                                                                 
C8         1uF                           TopLayer    0402                                  40.0250      18.8000      90       "Capacitor_not polarized"                                                                 
C7         100nF                         TopLayer    0402                                  36.0250      38.1000      180      "Capacitor_not polarized"                                                                 
C6         1uF                           TopLayer    0402                                  48.7500      19.5250      180      "Capacitor_not polarized"                                                                 
C5         100nF                         TopLayer    0402                                  48.7500      18.4750      360      "Capacitor_not polarized"                                                                 
C4         "Not Fitted (8.2pF)"          TopLayer    0402                                  45.7000      13.2750      180      "Capacitor_not polarized"                                                                 
C3         100nF                         TopLayer    0402                                  45.9000      18.7500      90       "Capacitor_not polarized"                                                                 
C2         "Not Fitted (8.2pF)"          TopLayer    0402                                  43.7750      13.2750      360      "Capacitor_not polarized"                                                                 
C1         100nF                         BottomLayer 0402                                  30.7000      51.6000      360      "Capacitor_not polarized"                                                                 
B2         SW-PUSH-CMS_BLUE              TopLayer    SWI_WEALTHMETAL_TD-0341_4P_-_BLUE     3.0278       43.3880      360      "Push-button SMD"                                                                         
B1         SW-PUSH-CMS_BLACK             TopLayer    SWI_WEALTHMETAL_TD-0341_4P_-_BACK     3.0278       31.0182      360      "Push-button SMD"                                                                         
Q2         BSR14                         TopLayer    SOT23-3                               33.7872      43.2544      360      "BSR14 NPN switching transistor SOT23 (Marking U8)"                                       
Q1         BSR14                         TopLayer    SOT23-3                               56.2088      40.3908      270      "BSR14 NPN switching transistor SOT23 (Marking U8)"                                       
U12        LT1963EST-3.3                 BottomLayer SOT223_SC73                           15.8294      38.6636      180      "LT1963EST-3.3 LDO Low Noise 1.5A fast Transient Response"                                
R67        10K                           TopLayer    0402                                  72.5500      2.6250       360      Resistor                                                                                  
CN26       Comment                       TopLayer    Spacer+Nut_M3                         -278.1248    -200.7568    90       ""                                                                                        
CN27       Comment                       TopLayer    Spacer+Nut_M3                         -278.1248    -200.7568    90       ""                                                                                        
CN28       Comment                       TopLayer    Spacer+Nut_M3                         -278.1248    -200.7568    90       ""                                                                                        
CN29       Comment                       TopLayer    Spacer+Nut_M3                         -278.1248    -200.7568    90       ""                                                                                        
TP1        PT                            BottomLayer PTB                                   8.4721       43.1870      180      "Point de test"                                                                           
TP2        PT                            BottomLayer PTB                                   8.4721       41.7300      180      "Point de test"                                                                           
TP3        PT                            BottomLayer PTB                                   8.4721       40.2730      180      "Point de test"                                                                           
TP4        PT                            BottomLayer PTB                                   8.4721       38.8160      180      "Point de test"                                                                           
TP5        PT                            BottomLayer PTB                                   8.4721       37.3590      180      "Point de test"                                                                           
TP6        PT                            BottomLayer PTB                                   8.4721       35.9020      180      "Point de test"                                                                           
