Altium Designer Pick and Place Locations
C:\Users\Gasnot Jordane\Documents\Projets\ATE\STM_Le Mans\Projets\MB1400C\BASE\MB1400C\03-Manufacturing\MB1400C_PCB\Assembly\MB1400-C01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       06/04/20
Time:       18:41
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                  Layer       Footprint                                      Center-X(mm) Center-Y(mm) Rotation Description                                                            
SB8        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         8.8750       7.4125       270      "Solder Bridge 0402 ON"                                                
C4         Capacitor                TopLayer    C0603                                          12.8750      6.4000       360      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                 
C3         Capacitor                TopLayer    C0603                                          12.8750      7.7250       360      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                 
C2         Capacitor                TopLayer    C0402                                          20.5750      8.2500       90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                 
C1         Capacitor                TopLayer    C0603                                          19.3000      8.0000       90       "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                 
CN1        "Header 10x2 STMod+"     TopLayer    CON_SAMTEC_TMM-110-01-L-D-RA__STMOD+           12.4750      2.4250       360      "Header 10x2, 2mm, RA, TH, Height 3.20mm/3.50mm"                       
LD1        LED_green                TopLayer    LED_0603_VISHAY_VLMTG1300-GS08_GREEN_1A2K_H0P8 10.6750      7.0750       270      "LED Green, 0603 SMD, Fw Voltage = 2.8V - 3.6V"                        
R1         Resistor                 TopLayer    R0402                                          10.7750      8.9750       180      Resistor,510R,0402,1%,1/16W                                            
SB5        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         5.5000       7.4125       270      "Solder Bridge 0402 ON"                                                
SB6        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         6.6250       7.4125       270      "Solder Bridge 0402 ON"                                                
SB7        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         7.7500       7.4125       270      "Solder Bridge 0402 ON"                                                
U3         ST1L05CPU33R             TopLayer    ICC_DFN6-EPAD_3X3_P095                         15.9750      7.2500       90       "LDO, 3.3V, 1.3A, Very low quiescent current BiCMOS voltage regulator" 
CN2        DF40C-50DP-0.4V(51)      BottomLayer CON_HRS_DF40C-50DP-0.4V_51                     12.5000      22.0000      270      "Header 25x2, 0.4mm pitch, VR, SMT, Height 1.5mm"                      
U2         M24128-DFMC6TP           TopLayer    ICC_DFN8-EPAD_2X3_P050                         22.5250      7.2750       180      "I2C Memory 3V3, 256Kbits, 2x3,0.55mm, UFDFPN8"                        
U1         "WIFI MODULE INTERPOSER" TopLayer    CON_MOD2BOARD_WIFI_MURATA_LBEE5PA1LD           12.5000      20.2000      0        "44 pins Generic Interposer Connector (Not Fitted : Footprint only)"   
M1         EMW3080(BP)              TopLayer    MOD_WIFI_MXCHIP_EMW3080-BP                     13.3000      19.3625      360      "Wi-Fi module 33x18mm, UART-SPI interface"                             
MIRE3      Comment                  TopLayer    MIRE_PLACE_SMD_0P8MM                           1.1500       1.9750       0        ""                                                                     
MIRE2      Comment                  TopLayer    MIRE_PLACE_SMD_0P8MM                           23.6500      3.8000       0        ""                                                                     
MIRE1      Comment                  TopLayer    MIRE_PLACE_SMD_0P8MM                           22.7000      31.0000      0        ""                                                                     
MIRE6      Comment                  BottomLayer MIRE_PLACE_SMD_0P8MM                           22.4250      30.6500      180      ""                                                                     
MIRE7      Comment                  BottomLayer MIRE_PLACE_SMD_0P8MM                           23.7000      3.7250       180      ""                                                                     
MIRE8      Comment                  BottomLayer MIRE_PLACE_SMD_0P8MM                           1.4750       2.1500       180      ""                                                                     
MIRE4      Comment                  BottomLayer LOGO_ETIQUETTE                                 -876.7250    -826.9000    270      ""                                                                     
SB1        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         1.0000       7.4125       270      "Solder Bridge 0402 ON"                                                
SB2        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         2.1250       7.4125       270      "Solder Bridge 0402 ON"                                                
SB3        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         3.2500       7.4125       270      "Solder Bridge 0402 ON"                                                
SB4        SB_ON                    TopLayer    SOLDER-BRIDGE_R0402-0R                         4.3750       7.4125       270      "Solder Bridge 0402 ON"                                                
R2         Resistor                 TopLayer    R0402                                          1.9500       14.2500      270      Resistor,10K,0402,1%,1/16W                                             
R3         Resistor                 TopLayer    R0402                                          13.1250      8.9750       180      Resistor,10K,0402,1%,1/16W                                             
MIRE5      Comment                  BottomLayer LOGO_ETIQUETTE                                 -876.7250    -826.9000    270      ""                                                                     
