Altium Designer Pick and Place Locations
C:\Subversion\MB1642-Nucleo64_Display_Expansion\Trunk\02-Manufacturing\MB1642D_PCB\Assembly\MB1642D_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       19/08/21
Time:       15:23
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment              Layer       Footprint                          Center-X(mm) Center-Y(mm) Rotation Description                                               
CN2        "Socket 19x2"        BottomLayer CON_SAMTEC_SSW-119-01-X-D          4.5719       44.7040      90       "Socket, 19x2, 2.54mm, VR, TH, Height 8.51mm/2.64mm"      
R12        Resistor             BottomLayer R0603                              41.6470      53.6300      180      Resistor,10K,0603,1%,1/10W                                
R11        Resistor             BottomLayer R1206_H0P55                        21.5470      41.3300      270      Resistor,6.2R,1206,1%,0.5W                                
R10        Resistor             BottomLayer R1206_H0P55                        23.7470      41.3300      270      Resistor,6.2R,1206,1%,0.5W                                
R9         Resistor             BottomLayer R1206_H0P55                        25.9470      41.3300      270      Resistor,6.2R,1206,1%,0.5W                                
R8         Resistor             BottomLayer R1206_H0P55                        46.6470      41.3300      270      Resistor,6.2R,1206,1%,0.5W                                
R7         Resistor             BottomLayer R0603                              43.4470      41.1300      270      Resistor,10K,0603,1%,1/10W                                
C7         Capacitor            BottomLayer C0603                              28.1470      41.7300      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm" 
R6         Resistor             TopLayer    R0603                              59.9470      42.1300      180      Resistor,10K,0603,1%,1/10W                                
R5         Resistor             TopLayer    R0603                              58.3000      15.3300      270      Resistor,10K,0603,1%,1/10W                                
R4         Resistor             TopLayer    R0603                              55.4000      17.6300      90       Resistor,10K,0603,1%,1/10W                                
R3         Resistor             TopLayer    R0603                              55.4000      12.1300      270      Resistor,10K,0603,1%,1/10W                                
R2         Resistor             TopLayer    R0603                              57.6000      6.0300       270      Resistor,10K,0603,1%,1/10W                                
R1         Resistor             TopLayer    R0603                              67.9000      17.7300      360      Resistor,10K,0603,1%,1/10W                                
C6         Capacitor            BottomLayer C0603                              28.9470      53.6300      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm" 
C5         Capacitor            TopLayer    C0603                              59.6000      15.3300      90       Capacitor,10nF,100V,X7R,10%,0603                          
C4         Capacitor            TopLayer    C0603                              56.7000      17.6300      270      Capacitor,10nF,100V,X7R,10%,0603                          
C3         Capacitor            TopLayer    C0603                              56.7000      12.1300      90       Capacitor,10nF,100V,X7R,10%,0603                          
C2         Capacitor            TopLayer    C0603                              58.9000      6.0300       90       Capacitor,10nF,100V,X7R,10%,0603                          
C1         Capacitor            TopLayer    C0603                              67.9000      16.4300      360      Capacitor,10nF,100V,X7R,10%,0603                          
B1         "Joystick MT-008A_M" TopLayer    SWI_XIEJIA_MT-008A_6P              63.0516      10.2870      45       "Joystick, 4 dir, 1 OK"                                   
CN3        "Socket 19x2"        BottomLayer CON_SAMTEC_SSW-119-01-X-D          65.5320      44.7040      90       "Socket, 19x2, 2.54mm, VR, TH, Height 8.51mm/2.64mm"      
LCD1       DT022CTFT            TopLayer    LCD_DISPLAYTECH_DT022CTFT_45P_P050 34.9630      17.3250      0        "240x320 2.2inch display"                                 
U1         MX25L6433FM2I-08G    BottomLayer ICC_SOP8_5P23X5P28_P127            35.1790      51.3470      270      ""                                                        
CN1        FH12-45S-0.5SH(55)   BottomLayer CON_HRS_FH12-45S-05SH              34.9790      33.7600      180      "45 pins P 0.5 surface mount connector"                   
HW2        STICKER_PRODUCT      TopLayer    STICKER_PRODUCT_25X5               -252.8600    -205.2400    90       "Sticker product 25x5 mm"                                 
HW3        STICKER_BOARD        TopLayer    STICKER_BOARD_25X5                 -252.8600    -205.2400    90       "Sticker board 25x5 mm"                                   
SB1        SB_OFF               BottomLayer SOLDER-BRIDGE_R0603-0R             42.7470      50.6800      270      "Solder Bridge OFF"                                       
SB2        SB_OFF               BottomLayer SOLDER-BRIDGE_R0603-0R             28.0470      51.1800      90       "Solder Bridge OFF"                                       
SB3        SB_OFF               BottomLayer SOLDER-BRIDGE_R0603-0R             28.0470      48.1800      270      "Solder Bridge OFF"                                       
SB4        SB_OFF               BottomLayer SOLDER-BRIDGE_R0603-0R             41.0470      50.6800      270      "Solder Bridge OFF"                                       
SB5        SB_OFF               BottomLayer SOLDER-BRIDGE_R0603-0R             29.5470      51.1800      90       "Solder Bridge OFF"                                       
SB6        SB_OFF               BottomLayer SOLDER-BRIDGE_R0603-0R             29.5470      48.1800      270      "Solder Bridge OFF"                                       
