Altium Designer Pick and Place Locations
C:\Users\tguilhot\OneDrive - STMicroelectronics\Documents\_SubVersion\HW_Boards\MB1642-STM32G0_Nucleo64_Display_Expansion\02-Manufacturing\MB1642B_PCB\Assembly\MB1642B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       03-02-20
Time:       08:24
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment              Layer       Footprint                          Center-X(mm) Center-Y(mm) Rotation Description                                            
CN1        FH12-45S-0.5SH(55)   BottomLayer CON_HRS_FH12-45S-05SH              49.3320      33.5300      180      "45 pins P 0.5 surface mount connector"                
U1         MX25L6433FM2I-08G    BottomLayer ICC_SOP8_5P23X5P28_P127            49.5320      51.1170      270      ""                                                     
LCD1       DT022CTFT            TopLayer    LCD_DISPLAYTECH_DT022CTFT_45P_P050 49.3160      17.0950      0        "240x320 2.2inch display"                              
CN3        "Socket 19x2"        BottomLayer CON_SAMTEC_SSW-119-01-X-D          79.8850      44.4740      90       "Socket, 19x2, 2.54mm, VR, TH, Height 8.51mm/2.64mm"   
B1         "Joystick MT-008A_M" TopLayer    SWI_XIEJIA_MT-008A_6P              77.4046      10.0570      45       "Joystick, 4 dir, 1 OK"                                
C1         Capacitor            TopLayer    C0603                              82.2530      16.2000      360      Capacitor,10nF,100V,X7R,10%,0603                       
C2         Capacitor            TopLayer    C0603                              73.2530      5.8000       90       Capacitor,10nF,100V,X7R,10%,0603                       
C3         Capacitor            TopLayer    C0603                              71.0530      11.9000      90       Capacitor,10nF,100V,X7R,10%,0603                       
C4         Capacitor            TopLayer    C0603                              71.0530      17.4000      270      Capacitor,10nF,100V,X7R,10%,0603                       
C5         Capacitor            TopLayer    C0603                              73.9530      15.1000      90       Capacitor,10nF,100V,X7R,10%,0603                       
C6         Capacitor            BottomLayer C0603                              43.6530      52.3000      270      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm" 
R1         Resistor             TopLayer    R0603                              82.2530      17.5000      360      Resistor,10K,0603,1%,1/10W                             
R2         Resistor             TopLayer    R0603                              71.9530      5.8000       270      Resistor,10K,0603,1%,1/10W                             
R3         Resistor             TopLayer    R0603                              69.7530      11.9000      270      Resistor,10K,0603,1%,1/10W                             
R4         Resistor             TopLayer    R0603                              69.7530      17.4000      90       Resistor,10K,0603,1%,1/10W                             
R5         Resistor             TopLayer    R0603                              72.6530      15.1000      270      Resistor,10K,0603,1%,1/10W                             
R6         Resistor             TopLayer    R0603                              72.9000      31.8000      180      Resistor,10K,0603,1%,1/10W                             
C7         Capacitor            BottomLayer C0603                              44.0000      41.9000      270      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm" 
R7         Resistor             BottomLayer R0603                              57.8000      40.9000      270      Resistor,10K,0603,1%,1/10W                             
R8         Resistor             BottomLayer R1206_H0P55                        61.0000      41.1000      270      Resistor,6.2R,1206,1%,0.5W                             
R9         Resistor             BottomLayer R1206_H0P55                        40.3000      41.1000      270      Resistor,6.2R,1206,1%,0.5W                             
R10        Resistor             BottomLayer R1206_H0P55                        38.1000      41.1000      270      Resistor,6.2R,1206,1%,0.5W                             
R11        Resistor             BottomLayer R1206_H0P55                        35.9000      41.1000      270      Resistor,6.2R,1206,1%,0.5W                             
R12        Resistor             BottomLayer R0603                              55.3530      52.3000      90       Resistor,10K,0603,1%,1/10W                             
CN2        "Socket 19x2"        BottomLayer CON_SAMTEC_SSW-119-01-X-D          18.9249      44.4740      90       "Socket, 19x2, 2.54mm, VR, TH, Height 8.51mm/2.64mm"   
