Altium Designer Pick and Place Locations
C:\work\viper-asterix\RevD\02-Manufacturing\MB1736D_PCB\Assembly\MB1736D_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       18/10/23
Time:       11:17
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                        Layer       Footprint                                                                                    Center-X(mm) Center-Y(mm) Rotation Description                                                                                              
U5         NX3L1T3157GM                   BottomLayer ICC_SOT886_XSON6                                                                             8.8900       72.1360      90       "Analog Switch, Low-ohmic single-pole double-throw analog switch"                                        
SB55       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       81.6190      32.7660      180      "Solder Bridge ON"                                                                                       
SB54       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       19.3770      25.1420      0        "Solder Bridge ON"                                                                                       
SB52       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       19.3770      23.7450      0        "Solder Bridge OFF"                                                                                      
C5         Capacitor                      BottomLayer C0603                                                                                        17.2720      41.1480      0        "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                                                 
SB50       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       104.1820     72.8218      180      "Solder Bridge ON"                                                                                       
SB49       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       75.5142      55.1696      270      "Solder Bridge ON"                                                                                       
CN19       "Jumper_Header 2x1"            BottomLayer CON_SAMTEC_TSW-102-07-G-S                                                                    14.5542      77.9780      90       "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                           
TP43       "Test Point"                   BottomLayer TP_SMD_1MM                                                                                   10.4140      63.2460      90       "Test Point 1mm"                                                                                         
R9         Resistor                       BottomLayer R0402                                                                                        120.9040     48.7680      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
SB67       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                                                       73.9855      17.0941      0        "Solder Bridge 0402 ON"                                                                                  
SB66       SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R                                                                       49.6316      21.8065      270      "Solder Bridge 0402 ON"                                                                                  
C37        Capacitor                      TopLayer    C0402                                                                                        70.3584      31.6485      315      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                  
C25        Capacitor                      TopLayer    C0402                                                                                        66.5992      36.1951      135      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                  
C38        Capacitor                      TopLayer    C0402                                                                                        71.1966      36.3475      225      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
R55        Resistor                       BottomLayer R0402                                                                                        118.0531     63.2691      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
X1         XTAL_4_PINS                    BottomLayer CRY_NX2016SA_4P                                                                              115.3160     55.2450      90       "Crystal, 24MHz, 6pF, +/-20ppm, 80R, 2x1.6mm"                                                            
U12        STMPS2151STR                   BottomLayer MOS_SOT23-5L                                                                                 134.6205     39.8780      0        "500mA, Enhanced single channel power switches with active high enable pin"                              
U16        ST730M33R                      BottomLayer ICC_SOT23-5L_H1P45                                                                           125.3493     38.8620      270      "LDO, 3.3V, 300mA, High input voltage: 2.5V to 28V, SOT23-5L"                                            
SB20       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       85.8306      52.3232      270      "Solder Bridge ON"                                                                                       
R49        Resistor                       TopLayer    R0402                                                                                        120.3960     60.8331      90       "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R66        Resistor                       BottomLayer R0402                                                                                        137.4144     38.0999      180      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                     
R84        Resistor                       BottomLayer R0603                                                                                        122.0470     38.7351      270      "Resistor, 27K, 0603, +/-1%, 1/10W"                                                                      
R68        Resistor                       BottomLayer R0402                                                                                        137.4144     41.1479      180      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                     
R67        Resistor                       BottomLayer R0402                                                                                        133.4774     45.7199      180      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                      
R83        Resistor                       BottomLayer R0603                                                                                        122.0470     35.8141      270      "Resistor, 47K, 0603, 1%, 1/10W"                                                                         
R60        Resistor                       BottomLayer R0402                                                                                        146.5580     48.5141      270      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                        
R59        Resistor                       BottomLayer R0603                                                                                        148.0820     48.5141      270      "Resistor, 330R, 0603, +/-1%, 1/10W"                                                                     
R76        Resistor                       BottomLayer R0402                                                                                        132.8420     47.7521      270      "Resistor, 3K9, 0402, +/-1%, 1/16W, +/-100ppm/°C"                                                        
R80        Resistor                       BottomLayer R0402                                                                                        130.5560     47.7521      270      "Resistor, 1K8, 0402, +/-1%, 1/16W"                                                                      
R77        Resistor                       BottomLayer R0402                                                                                        131.6990     47.7521      270      "Resistor, 1K3, 0402, +/-1%, 1/16W"                                                                      
R50        Resistor                       TopLayer    R0402                                                                                        121.2850     54.8641      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
LD8        LED_BICOLOR                    TopLayer    LED_BI-GR_WE-150141SV73110                                                                   147.2696     49.6822      0        "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                              
D5         SCHOTTKY_1A_2K                 BottomLayer DIO_SOD523_1A_2K                                                                             126.3650     34.5438      90       "Small signal Schottky diodes"                                                                           
D4         SCHOTTKY_1A_2K                 BottomLayer DIO_SOD523_1A_2K                                                                             127.7620     34.5438      90       "Small signal Schottky diodes"                                                                           
D3         SCHOTTKY_1A_2K                 BottomLayer DIO_SOD523_1A_2K                                                                             129.1590     34.5438      90       "Small signal Schottky diodes"                                                                           
D6         SCHOTTKY_1A_2K                 BottomLayer DIO_SOD523_1A_2K                                                                             124.7140     34.5438      90       "Small signal Schottky diodes"                                                                           
C96        Capacitor                      BottomLayer C0402                                                                                        117.0940     56.3881      90       "Capacitor, MLCC, 5.6pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                              
C95        Capacitor                      BottomLayer C0402                                                                                        117.0940     54.6101      90       "Capacitor, MLCC, 5.6pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                              
C80        Capacitor                      BottomLayer C0603                                                                                        134.3660     42.7989      180      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                                 
C81        Capacitor                      BottomLayer C0402                                                                                        131.6424     35.8367      0        "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                                
C87        Capacitor                      BottomLayer C0603                                                                                        128.7780     40.2589      180      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                                 
C85        Capacitor                      BottomLayer C0805                                                                                        129.0319     37.3379      180      "Capacitor, MLCC, 2.2uF, 25V, X7R, +/-10%, 0805, T=1,25mm"                                               
C61        Capacitor                      TopLayer    C0402                                                                                        122.4280     60.8331      90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                                 
C77        Capacitor                      BottomLayer C0402                                                                                        139.0085     61.9987      180      "Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                 
C59        Capacitor                      TopLayer    C0402                                                                                        121.4120     60.8331      90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                                 
SB28       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       81.5340      36.2450      90       "Solder Bridge ON"                                                                                       
B1         SW_BLACK_KSC321JLFS            TopLayer    SWI_C&K_KSC321JLFS_BLACK                                                                     145.3200     28.2005      270      "Switch HW BLACK High3.5mm 2Newtons, BEND type"                                                          
B2         SW_BLUE_KSC721JLFS             TopLayer    SWI_C&K_KSC721JLFS_BLUE                                                                      145.3200     15.3613      270      "Switch HW BLUE High4.3mm 2.25 Newtons, BEND type"                                                       
C75        Capacitor                      TopLayer    C0402                                                                                        79.0956      30.3784      180      "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                                 
C109       Capacitor                      BottomLayer C0402                                                                                        82.3181      40.9335      270      "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                              
C108       Capacitor                      BottomLayer C0402                                                                                        82.3181      38.9015      90       "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                              
C107       Capacitor                      BottomLayer C0402                                                                                        85.2170      27.8131      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C43        Capacitor                      TopLayer    C0402                                                                                        75.1844      33.0199      0        "Capacitor, MLCC, 10uF, 4V, X5R, +/-20%, 0402, T=0.5mm"                                                  
C44        Capacitor                      TopLayer    C0402                                                                                        80.3910      35.9409      270      "Capacitor, MLCC, 220pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                 
C106       Capacitor                      BottomLayer C0603                                                                                        84.9630      35.3059      0        "Capacitor, MLCC, 10uF, 6V3, X5R, +/-20%, 0603, T=0.8mm"                                                 
C120       Capacitor                      BottomLayer C0603                                                                                        70.4088      46.0644      270      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C115       Capacitor                      BottomLayer C0603                                                                                        67.9450      23.2776      90       "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C121       Capacitor                      BottomLayer C0603                                                                                        57.5788      37.3126      0        "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C114       Capacitor                      BottomLayer C0603                                                                                        57.2404      25.2222      180      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C27        Capacitor                      TopLayer    C0603                                                                                        67.5640      40.1319      180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                  
C28        Capacitor                      TopLayer    C0402                                                                                        67.5138      32.1817      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C46        Capacitor                      TopLayer    C0402                                                                                        78.0034      31.7246      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C24        Capacitor                      TopLayer    C0402                                                                                        66.0406      34.7979      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C35        Capacitor                      TopLayer    C0402                                                                                        69.5456      34.7473      45       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C31        Capacitor                      TopLayer    C0402                                                                                        68.8090      33.2741      315      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C26        Capacitor                      TopLayer    C0402                                                                                        67.0560      37.5924      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C39        Capacitor                      TopLayer    C0402                                                                                        71.4508      32.4865      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C36        Capacitor                      TopLayer    C0402                                                                                        70.3078      37.1352      225      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C30        Capacitor                      TopLayer    C0402                                                                                        68.5550      35.3569      45       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C105       Capacitor                      BottomLayer C0603                                                                                        81.5340      31.2419      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C48        Capacitor                      TopLayer    C0402                                                                                        78.7400      33.7821      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                  
C40        Capacitor                      TopLayer    C0402                                                                                        71.5268      34.6201      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C45        Capacitor                      TopLayer    C0402                                                                                        77.0890      33.5281      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                  
C41        Capacitor                      TopLayer    C0402                                                                                        73.4318      34.5947      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C122       Capacitor                      BottomLayer C0603                                                                                        54.6740      11.1304      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C19        Capacitor                      TopLayer    C0402                                                                                        62.4846      13.3349      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C17        Capacitor                      TopLayer    C0402                                                                                        60.8336      8.0009       0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C14        Capacitor                      TopLayer    C0402                                                                                        57.0230      11.3034      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C119       Capacitor                      BottomLayer C0603                                                                                        58.9280      4.5719       0        "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C117       Capacitor                      BottomLayer C0603                                                                                        65.2780      12.8274      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C42        Capacitor                      TopLayer    C0402                                                                                        73.1520      11.1252      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C47        Capacitor                      TopLayer    C0402                                                                                        78.7406      13.2079      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C110       Capacitor                      BottomLayer C0603                                                                                        81.4070      12.8274      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C113       Capacitor                      BottomLayer C0603                                                                                        71.3740      10.7954      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C49        Capacitor                      TopLayer    C0402                                                                                        113.6656     28.8289      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C101       Capacitor                      BottomLayer C0402                                                                                        110.2551     42.8273      270      "Capacitor, MLCC, 470pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                 
C99        Capacitor                      BottomLayer C0402                                                                                        111.2711     42.8273      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                  
C50        Capacitor                      TopLayer    C0402                                                                                        114.7274     41.7788      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C98        Capacitor                      BottomLayer C0402                                                                                        111.3981     37.1123      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C100       Capacitor                      BottomLayer C0402                                                                                        119.1261     35.6869      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C102       Capacitor                      BottomLayer C0603                                                                                        119.1260     34.4169      0        "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                                 
C91        Capacitor                      TopLayer    C0402                                                                                        117.7291     25.0189      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C92        Capacitor                      TopLayer    C0402                                                                                        109.7281     25.0189      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C132       Capacitor                      BottomLayer C0603                                                                                        27.4860      23.7220      270      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C128       Capacitor                      BottomLayer C0402                                                                                        28.3210      30.0990      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C138       Capacitor                      BottomLayer C0603                                                                                        21.7170      33.2740      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                  
C144       Capacitor                      BottomLayer C0402                                                                                        28.3210      27.9400      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C127       Capacitor                      BottomLayer C0603                                                                                        28.4480      26.7970      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C140       Capacitor                      BottomLayer C0402                                                                                        22.0980      24.8920      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C129       Capacitor                      BottomLayer C0402                                                                                        19.4310      26.5430      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C141       Capacitor                      BottomLayer C0402                                                                                        23.3680      24.8920      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C139       Capacitor                      BottomLayer C0603                                                                                        28.3750      29.1030      180      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C135       Capacitor                      BottomLayer C0603                                                                                        19.4310      30.4800      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C134       Capacitor                      BottomLayer C0603                                                                                        19.4310      29.2100      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C133       Capacitor                      BottomLayer C0603                                                                                        16.8910      27.8130      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C130       Capacitor                      BottomLayer C0603                                                                                        26.2160      23.7220      270      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C131       Capacitor                      BottomLayer C0603                                                                                        24.9460      23.7220      270      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C137       Capacitor                      BottomLayer C0603                                                                                        23.2410      33.2740      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                  
C1         Capacitor                      BottomLayer C0402                                                                                        11.1506      72.1868      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C2         Capacitor                      BottomLayer C0402                                                                                        12.1412      76.1492      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                  
C3         Capacitor                      BottomLayer C0402                                                                                        11.2408      76.1582      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C150       Capacitor                      BottomLayer C0603                                                                                        22.0980      69.5964      270      "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                                                 
C157       Capacitor                      BottomLayer C0603                                                                                        14.0970      69.5964      270      "Capacitor, MLCC, 100nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                                                
C146       Capacitor                      BottomLayer C0402                                                                                        25.4006      58.2830      180      "Capacitor, MLCC, 560pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                 
C147       Capacitor                      BottomLayer C0402                                                                                        25.3427      60.9500      180      "Capacitor, MLCC, 560pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                 
C145       Capacitor                      BottomLayer C0603                                                                                        25.4000      59.5530      0        "Capacitor, MLCC, 100nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                                                
C136       Capacitor                      BottomLayer C0402                                                                                        29.2106      63.1189      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                  
C153       Capacitor                      BottomLayer C0603                                                                                        16.2560      39.6549      180      "Capacitor, MLCC, 100nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                                                
C125       Capacitor                      BottomLayer C0402                                                                                        46.9900      74.9304      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C13        Capacitor                      TopLayer    C0603                                                                                        49.2760      80.7719      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C76        Capacitor                      TopLayer    C0402                                                                                        142.3676     83.1849      0        "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                  
C18        Capacitor                      TopLayer    C0402                                                                                        61.1605      61.4989      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C16        Capacitor                      TopLayer    C0805                                                                                        61.1603      59.7209      0        "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm"                                                
C15        Capacitor                      TopLayer    C0402                                                                                        59.6359      69.8814      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C126       Capacitor                      BottomLayer C0402                                                                                        37.9665      51.8469      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C104       Capacitor                      BottomLayer C0805                                                                                        97.5360      30.7343      90       "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm"                                                
C103       Capacitor                      BottomLayer C0805                                                                                        105.1564     42.5449      180      "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm"                                                
C86        Capacitor                      BottomLayer C0603                                                                                        129.5400     29.3374      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C88        Capacitor                      BottomLayer C0603                                                                                        126.7460     26.6699      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C89        Capacitor                      BottomLayer C0402                                                                                        126.5691     32.2579      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C90        Capacitor                      BottomLayer C0402                                                                                        120.5489     71.4958      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C97        Capacitor                      BottomLayer C0603                                                                                        113.5644     72.5113      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C93        Capacitor                      BottomLayer C0603                                                                                        117.1951     68.7125      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C94        Capacitor                      BottomLayer C0402                                                                                        116.9674     58.5469      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C69        Capacitor                      TopLayer    C0603                                                                                        127.5781     58.5700      180      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C70        Capacitor                      TopLayer    C0603                                                                                        128.6033     54.0389      180      "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C83        Capacitor                      BottomLayer C0402                                                                                        131.1375     56.0379      0        "Capacitor, MLCC, 20pF, 50V, NPO, +/- 5%, 0402, T=0.5mm"                                                 
C82        Capacitor                      BottomLayer C0603                                                                                        131.1371     58.8319      0        "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                               
C65        Capacitor                      TopLayer    C0402                                                                                        124.5883     60.8247      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C51        Capacitor                      TopLayer    C0402                                                                                        117.9830     59.6901      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C55        Capacitor                      TopLayer    C0402                                                                                        119.2530     59.6901      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C52        Capacitor                      TopLayer    C0402                                                                                        119.1175     53.7882      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C62        Capacitor                      TopLayer    C0402                                                                                        123.3254     51.3909      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C64        Capacitor                      TopLayer    C0402                                                                                        124.3414     51.3920      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C60        Capacitor                      TopLayer    C0402                                                                                        121.9081     51.3881      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C56        Capacitor                      TopLayer    C0402                                                                                        119.5116     51.4110      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C57        Capacitor                      TopLayer    C0402                                                                                        120.8921     51.3892      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C73        Capacitor                      TopLayer    C0402                                                                                        128.2981     57.3361      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C68        Capacitor                      TopLayer    C0402                                                                                        125.8872     56.4742      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C71        Capacitor                      TopLayer    C0402                                                                                        128.2917     56.2627      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C53        Capacitor                      TopLayer    C0402                                                                                        119.1513     55.8390      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C72        Capacitor                      TopLayer    C0402                                                                                        128.2981     55.3269      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C67        Capacitor                      TopLayer    C0402                                                                                        125.6523     60.8207      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C58        Capacitor                      TopLayer    C0402                                                                                        121.2959     56.7595      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C54        Capacitor                      TopLayer    C0603                                                                                        119.1245     57.6566      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C66        Capacitor                      TopLayer    C0603                                                                                        125.6030     51.3079      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                  
C63        Capacitor                      TopLayer    C0402                                                                                        123.5735     60.8225      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C78        Capacitor                      BottomLayer C0402                                                                                        135.1280     51.1809      270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                                
C79        Capacitor                      BottomLayer C0603                                                                                        137.7950     49.1489      180      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                                 
C84        Capacitor                      BottomLayer C0402                                                                                        131.4450     50.9271      90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                                 
C23        Capacitor                      TopLayer    C0402                                                                                        65.8372      32.5627      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C29        Capacitor                      TopLayer    C0402                                                                                        67.4116      29.7184      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C34        Capacitor                      TopLayer    C0402                                                                                        68.9013      31.3981      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C33        Capacitor                      TopLayer    C0402                                                                                        68.9013      29.6201      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C111       Capacitor                      BottomLayer C0603                                                                                        74.5490      20.4471      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C21        Capacitor                      TopLayer    C0402                                                                                        62.5862      34.6963      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C22        Capacitor                      TopLayer    C0402                                                                                        64.2626      34.7979      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C20        Capacitor                      TopLayer    C0402                                                                                        62.5862      33.7819      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C118       Capacitor                      BottomLayer C0603                                                                                        60.0710      21.8441      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                
C156       Capacitor                      TopLayer    C0603_H0P8                                                                                   11.6271      57.1730      90       "Capacitor, MLCC, 2.2uF, 50V, X5R, +/-15%, 0603,T=0.8mm"                                                 
C4         Capacitor                      BottomLayer C0603                                                                                        135.3820     47.6249      270      "Capacitor, MLCC, 100nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                                                
CN10       RJ45_KRJ-CB4.2GYZNL            BottomLayer CON_RJ45_DGKYD_KRJ-CB4.2GYZNL                                                                114.3700     7.9500       180      "Connector_RJ45, single port, with LEDS, T= 11.05mm"                                                     
CN16       Jack_PJ3028B-3_4P              BottomLayer CON_PHONE-JACK-3P5_HY_PJ3028B                                                                27.9805      9.2808       90       "Jack_ Socket-Stereo, 3.5mm, 4 pins, RA, SMD, T=5mm"                                                     
CN1        "Socket 10x2"                  TopLayer    CON_FCI_20021311-XXX20XXLF                                                                   3.1750       74.3259      270      "Socket, 10x2, 1.27mm, VR, TH, T=4.30mm/2.40mm"                                                          
CN13       microSD-PJS008-2003            BottomLayer CON_MICROSD_YAMAICHI_PJS008-2003-1                                                           46.8321      87.4034      90       "Connector_uSD Card, Reversed-Type, Mnt Push-Push"                                                       
CN6        FPU330ZH-BT1D3-CA              TopLayer    CON_TOWNES_FPU330ZH-BT1D3-CA_P050                                                            145.8135     75.0378      90       "Socket_FFC/FPC, 30 pins, 0.5mm, RA, SMD, T=5.9mm"                                                       
CN2        "Header 25x2"                  TopLayer    CON_SAMTEC_FLE-125-01-G-DV                                                                   75.0032      65.3736      180      "Header, 25x2, 1.27mm, SMD, VR, T=4.55mm"                                                                
CN15       "Socket 10x1"                  BottomLayer CON_SAMTEC_SSW-110-22-X-S-VS                                                                 43.3042      46.8441      270      "Socket, 10x1, 2.54mm, VR, SMD, T=9.78mm"                                                                
CN12       "Socket 8x1"                   BottomLayer CON_SAMTEC_SSW-108-22-X-S-VS                                                                 91.6051      40.2401      90       "Socket, 8x1, 2.54mm, VR, SMD, T=9.78mm"                                                                 
CN11       "Socket 6x1"                   BottomLayer CON_SAMTEC_SSW-106-22-X-S-VS                                                                 91.6051      19.9201      90       "Socket, 6x1, 2.54mm, VR, SMD, T=9.78mm"                                                                 
CN3        "Socket 10X2 STMod+"           TopLayer    CON_SAMTEC_SQT-110-01-F-D-RA__STMOD+                                                         91.9066      87.3665      180      "Socket, 10x2, 2mm, RA, TH, T=6.35mm/2.29mm"                                                             
CN4        "Socket 6X2 PMOD"              TopLayer    CON_SAMTEC_SSW-106-02-F-D-RA__PMOD                                                           117.8560     84.7089      180      "Socket, 6x2, 2.54mm, RA, TH, T=8.51mm/7.62mm"                                                           
CN9        "Header 4x1"                   BottomLayer CON_SAMTEC_TSW-104-07-G-S                                                                    126.7460     44.8309      0        "Header, 4x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                           
CN8        "Header 10x2"                  BottomLayer CON_SAMTEC_FTSH-110-01-L-DV                                                                  129.7943     74.0663      90       "Header, 10x2, 1.27mm, VR, SMD, T=3.05mm"                                                                
CN5        Tag-10-C                       TopLayer    CON_TAG-C_TC2050-IDC-NL                                                                      144.8130     40.6709      90       "Header_Plug-of-nails, 5x2, 1.27mm, No legs"                                                             
D7         SCHOTTKY_1A_2K                 BottomLayer DIO_SOD523_1A_2K                                                                             13.2084      38.1309      0        "Small signal Schottky diodes"                                                                           
H7         "POSITION HOLE"                BottomLayer PTH_450_900                                                                                  16.7630      5.2300       180      "POSITION HOLE C9D4R5"                                                                                   
H8         "POSITION HOLE"                BottomLayer PTH_450_900                                                                                  16.7630      90.7698      180      "POSITION HOLE C9D4R5"                                                                                   
H5         "POSITION HOLE"                BottomLayer PTH_450_900                                                                                  133.2431     5.2300       180      "POSITION HOLE C9D4R5"                                                                                   
H6         "POSITION HOLE"                BottomLayer PTH_450_900                                                                                  133.2431     90.7698      180      "POSITION HOLE C9D4R5"                                                                                   
H2         "POSITION HOLE"                TopLayer    PTH_350_700                                                                                  5.0800       90.7701      0        "POSITION HOLE C7D3R5"                                                                                   
H3         "POSITION HOLE"                TopLayer    PTH_350_700                                                                                  144.9200     90.7698      0        "POSITION HOLE C7D3R5"                                                                                   
H1         "POSITION HOLE"                TopLayer    PTH_350_700                                                                                  5.0800       5.2300       0        "POSITION HOLE C7D3R5"                                                                                   
H4         "POSITION HOLE"                TopLayer    PTH_350_700                                                                                  144.9202     5.2300       0        "POSITION HOLE C7D3R5"                                                                                   
HW2        STICKER_BOARD                  BottomLayer STICKER_BOARD_25X9                                                                           -242.5000    -196.5730    180      "Sticker Board 25x9 mm"                                                                                  
HW1        STICKER_PRODUCT                BottomLayer STICKER_PRODUCT_25X9                                                                         -242.5000    -196.5730    180      "Sticker product 25x9 mm"                                                                                
JP6        "Jumper_Header 3x1 Fitted 1-2" BottomLayer CON_SAMTEC_TSW-103-07-F-S                                                                    67.5640      91.9479      180      "Header, 3x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                           
JP5        "Jumper_Header 2x1 Fitted"     BottomLayer CON_SAMTEC_TSW-102-07-G-S                                                                    84.5058      56.5403      180      "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                           
JP1        "Jumper_Header 4x2"            BottomLayer CON_SAMTEC_TSM-104-01-X-DV                                                                   143.6277     17.7799      270      "Header, 4x2, 2.54mm, VR, SMD, T=5.84mm/2.54mm"                                                          
JP3        "Jumper_Header 2x1"            BottomLayer CON_SAMTEC_TSW-102-07-G-S                                                                    113.7176     61.2266      90       "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                           
L4         Inductor                       BottomLayer IND_2016_MURATA_LQM2MPN2R2NG0                                                                80.8990      35.6869      90       "Inductor, 2.2uH, +/-30%, 1.2A, 0R138, 0806, T=0.9mm"                                                    
L1         BEAD                           BottomLayer L0603                                                                                        119.2531     32.6389      0        "Ferrite bead, 600R@100MHz, +/-25%, 500mA, 380mR, 0603, T=0.8mm"                                         
LD6        LED_green                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4                                                 10.6680      53.2131      270      "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                  
LD5        LED_green                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4                                                 10.6680      48.3871      270      "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                  
LD12       LED_green                      BottomLayer LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4                                                 27.4320      49.7844      90       "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                  
LD1        LED_green                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4                                                 4.7116       16.5099      0        "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                  
LD2        LED_orange                     TopLayer    LED_0603_OSRAM_LO-Q976-PS-25_ORANGE_1A2K_H0P8                                                4.7116       18.5419      0        "LED Orange, 0603 SMD, Forward Voltage Min=1.6V, Max=2.4V"                                               
LD3        LED_red                        TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8                                                  4.6996       20.7009      0        "LED Red, 0603 SMD, 2V Forward Voltage"                                                                  
LD4        LED_blue                       TopLayer    LED_0603_OSRAM_LB-Q39G-L2OO-35-1_BLUE_1A2K_H0P4                                              4.6996       22.6059      0        "LED Blue, 0603 SMD, Forward Voltage Min=2,8V, Max=3,8V"                                                 
LD7        LED_BICOLOR                    TopLayer    LED_BI-GR_WE-150141SV73110                                                                   143.1039     49.6822      0        "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                              
Q4         STL40DN3LLH5                   BottomLayer PowerFLAT_5x6                                                                                25.9080      71.6100      0        "MOSFET, Dual N-channel 30 V, 0.016 ? typ., 40 A, STripFET™ H5 Power MOSFET"                             
Q5         STL40DN3LLH5                   BottomLayer PowerFLAT_5x6                                                                                18.2880      71.6181      0        "MOSFET, Dual N-channel 30 V, 0.016 ? typ., 40 A, STripFET™ H5 Power MOSFET"                             
Q8         9013-SOT23                     BottomLayer NPN_SOT23                                                                                    13.9704      53.0861      270      "NPN Bipolar Transistor"                                                                                 
Q6         STL11N3LLH6                    BottomLayer MOS_POWERFLAT_3P3X3P3_P065                                                                   16.5100      43.4649      270      "N-channel 30 V, 6 mO typ, 11 A STripFET™ H6, Power MOSFET in a PowerFLAT™ 3.3x3.3 package"              
Q7         9013-SOT23                     BottomLayer NPN_SOT23                                                                                    13.9704      48.2601      270      "NPN Bipolar Transistor"                                                                                 
Q1         BSN20                          BottomLayer MOS_SOT23                                                                                    142.3796     77.0183      90       "Transistor, N-channel enhancement mode field-effect transistor"                                         
Q3         BSN20                          BottomLayer MOS_SOT23                                                                                    30.7346      49.7844      270      "Transistor, N-channel enhancement mode field-effect transistor"                                         
Q9         9013-SOT23                     BottomLayer NPN_SOT23                                                                                    7.7047       16.0214      90       "NPN Bipolar Transistor"                                                                                 
Q10        9013-SOT23                     BottomLayer NPN_SOT23                                                                                    7.7047       19.4454      90       "NPN Bipolar Transistor"                                                                                 
Q2         BSN20                          BottomLayer MOS_SOT23                                                                                    142.3587     80.8024      90       "Transistor, N-channel enhancement mode field-effect transistor"                                         
R1         Resistor                       TopLayer    R0402                                                                                        5.7888       30.5990      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R113       Resistor                       BottomLayer R0603                                                                                        24.7650      47.1169      180      "Resistor, 62K, 0603, +/-1%, 1/10W"                                                                      
R112       Resistor                       BottomLayer R0402                                                                                        80.8740      40.4860      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R114       Resistor                       BottomLayer R0402                                                                                        80.7947      27.4451      180      "Resistor, 51R, 0402, +/-1%, 1/16W"                                                                      
R110       Resistor                       BottomLayer R0402                                                                                        85.2170      25.9081      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R111       Resistor                       BottomLayer R0402                                                                                        80.8740      39.3511      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R109       Resistor                       BottomLayer R0603                                                                                        84.9630      32.3849      180      "Resistor, 0R, 0603, +/-5%, 1/10W"                                                                       
R118       Resistor                       BottomLayer R0402                                                                                        55.3151      8.6590       270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R116       Resistor                       BottomLayer R0402                                                                                        64.8926      7.5739       0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R117       Resistor                       BottomLayer R0402                                                                                        61.2780      4.7225       270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R115       Resistor                       BottomLayer R0402                                                                                        75.4384      5.0799       180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R102       Resistor                       BottomLayer R0402                                                                                        113.9840     44.6053      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R104       Resistor                       BottomLayer R0402                                                                                        112.8410     44.6053      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R48        Resistor                       TopLayer    R0402                                                                                        116.4781     44.6053      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R92        Resistor                       BottomLayer R0402                                                                                        117.7481     44.6053      90       "Resistor, 1K5, 0402, +/-1%, 1/16W"                                                                      
R90        Resistor                       BottomLayer R0402                                                                                        118.8917     42.0648      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R98        Resistor                       BottomLayer R0402                                                                                        115.6970     35.1794      270      "Resistor, 49R9, 0402, +/-1%, 1/16W"                                                                     
R95        Resistor                       BottomLayer R0402                                                                                        117.2210     35.1794      270      "Resistor, 49R9, 0402, +/-1%, 1/16W"                                                                     
R103       Resistor                       BottomLayer R0402                                                                                        113.0300     35.1794      270      "Resistor, 49R9, 0402, +/-1%, 1/16W"                                                                     
R100       Resistor                       BottomLayer R0402                                                                                        114.5540     35.1794      270      "Resistor, 49R9, 0402, +/-1%, 1/16W"                                                                     
R47        Resistor                       TopLayer    R0402                                                                                        113.9840     44.6053      270      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R46        Resistor                       TopLayer    R0402                                                                                        112.8410     44.6053      270      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R105       Resistor                       BottomLayer R0402                                                                                        111.8870     35.1794      270      "Resistor, 12K1, 0402, +/-1%, 1/16W"                                                                     
R96        Resistor                       BottomLayer R0402                                                                                        116.4781     44.6053      270      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R89        Resistor                       BottomLayer R0402                                                                                        118.8917     40.7948      180      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R85        Resistor                       BottomLayer R0402                                                                                        122.3010     13.3354      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R87        Resistor                       BottomLayer R0402                                                                                        120.9233     13.3534      270      "Resistor, 270R, 0402, +/-1%, 1/16W"                                                                     
R107       Resistor                       BottomLayer R0402                                                                                        106.5723     13.3534      270      "Resistor, 270R, 0402, +/-1%, 1/16W"                                                                     
R106       Resistor                       BottomLayer R0603                                                                                        84.9630      30.7339      180      "Resistor, 0R, 0603, +/-5%, 1/10W"                                                                       
R99        Resistor                       BottomLayer R0402                                                                                        115.2081     44.6053      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R131       Resistor                       BottomLayer R0603                                                                                        28.3860      34.0360      0        "Resistor, 0R, 0603, +/-5%, 1/10W"                                                                       
R129       Resistor                       BottomLayer R0603                                                                                        28.3860      32.7660      0        "Resistor, 0R, 0603, +/-5%, 1/10W"                                                                       
R127       Resistor                       BottomLayer R0603                                                                                        28.3860      31.4960      0        "Resistor, 0R, 0603, +/-5%, 1/10W"                                                                       
R145       Resistor                       BottomLayer R0603                                                                                        21.8440      22.3520      90       "Resistor, 20R, 0603, +/-1%, 1/10W"                                                                      
R146       Resistor                       BottomLayer R0603                                                                                        23.3680      22.3520      90       "Resistor, 20R, 0603, +/-1%, 1/10W"                                                                      
R132       Resistor                       BottomLayer R0402                                                                                        19.3580      27.8330      0        "Resistor, 2K2, 0402, +/-1%, 1/16W"                                                                      
R45        Resistor                       TopLayer    R0402                                                                                        81.7886      44.4499      180      "Resistor, 1K5, 0402, +/-1%, 1/16W"                                                                      
R7         Resistor                       TopLayer    R0402                                                                                        10.7950      71.7550      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R2         Resistor                       BottomLayer R0402                                                                                        11.2250      78.0753      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R134       Resistor                       TopLayer    R0603                                                                                        21.9141      64.2850      180      "Resistor, 22mR, 0603, +/-1%, 1/3W"                                                                      
R151       Resistor                       BottomLayer R0402                                                                                        24.7650      62.4054      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R147       Resistor                       BottomLayer R0402                                                                                        26.0350      62.4054      90       "Resistor, 2K4, 0402, +/-1%, 1/16W"                                                                      
R152       Resistor                       BottomLayer R0402                                                                                        22.8377      56.1270      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R167       Resistor                       BottomLayer R0402                                                                                        9.2710       53.0861      90       "Resistor, 270R, 0402, +/-1%, 1/16W"                                                                     
R136       Resistor                       BottomLayer R0603                                                                                        29.2100      66.4209      0        "Resistor, 330K, 0603, +/-1%, 1/10W"                                                                     
R163       Resistor                       TopLayer    R0603                                                                                        13.0241      57.1730      270      "Resistor, 47K, 0603, 1%, 1/10W"                                                                         
R135       Resistor                       BottomLayer R0603                                                                                        29.2100      64.5159      180      "Resistor, 49K9, 0603, +/-1%, 1/10W"                                                                     
R162       Resistor                       TopLayer    R0603                                                                                        14.9291      57.1730      90       "Resistor, 10K, 0603, +/-1%, 1/10W"                                                                      
R159       Resistor                       BottomLayer R0402                                                                                        18.2880      36.6074      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R156       Resistor                       BottomLayer R0402                                                                                        19.9390      36.6074      270      "Resistor, 2K4, 0402, +/-1%, 1/16W"                                                                      
R166       Resistor                       BottomLayer R0402                                                                                        9.2710       48.6411      90       "Resistor, 270R, 0402, +/-1%, 1/16W"                                                                     
R158       Resistor                       BottomLayer R0603                                                                                        17.8433      47.0991      180      "Resistor, 47K, 0603, 1%, 1/10W"                                                                         
R161       Resistor                       BottomLayer R0603                                                                                        17.2077      49.7666      90       "Resistor, 10K, 0603, +/-1%, 1/10W"                                                                      
R64        Resistor                       BottomLayer R0402                                                                                        139.6492     77.3434      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R21        Resistor                       TopLayer    R0603                                                                                        62.4840      57.4044      90       "Resistor, 0R, 0603, +/-5%, 1/10W"                                                                       
R17        Resistor                       TopLayer    R0603                                                                                        59.9440      57.4044      90       "Resistor, 0R, 0603, +/-5%, 1/10W"                                                                       
R150       Resistor                       BottomLayer R0402                                                                                        25.7810      49.7844      90       "Resistor, 330R, 0402, +/-1%, 1/16W"                                                                     
R130       Resistor                       BottomLayer R0402                                                                                        33.5280      49.7844      90       "Resistor, 1M, 0402, +/-1%, 1/16W"                                                                       
R108       Resistor                       BottomLayer R0402                                                                                        96.6476      49.1489      0        "Resistor, 1K, 0402, +/-1%,1/16W"                                                                        
R120       Resistor                       BottomLayer R0402                                                                                        37.9736      53.2129      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R5         Resistor                       TopLayer    R0402                                                                                        7.6326       16.5099      180      "Resistor, 510R, 0402, +/-1%, 1/16W"                                                                     
R168       Resistor                       BottomLayer R0603                                                                                        4.6990       15.9554      270      "Resistor, 100K, 0603, +/- 1%, 1/10W"                                                                    
R171       Resistor                       BottomLayer R0603                                                                                        3.0480       15.9554      270      "Resistor, 47K, 0603, 1%, 1/10W"                                                                         
R6         Resistor                       TopLayer    R0402                                                                                        7.6326       18.5419      180      "Resistor, 300R, 0402, +/-1%, 1/16W"                                                                     
R169       Resistor                       BottomLayer R0603                                                                                        4.6990       19.2574      270      "Resistor, 100K, 0603, +/- 1%, 1/10W"                                                                    
R170       Resistor                       BottomLayer R0603                                                                                        3.1750       19.3224      270      "Resistor, 47K, 0603, 1%, 1/10W"                                                                         
R3         Resistor                       TopLayer    R0402                                                                                        7.6206       20.7009      180      "Resistor, 680R, 0402, +/-1%, 1/16W"                                                                     
R4         Resistor                       TopLayer    R0402                                                                                        7.6206       22.6059      180      "Resistor, 510R, 0402, +/-1%, 1/16W"                                                                     
R82        Resistor                       BottomLayer R0402                                                                                        124.3330     30.4298      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R91        Resistor                       BottomLayer R0402                                                                                        117.7555     73.5273      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R97        Resistor                       BottomLayer R0603                                                                                        115.4689     70.4798      270      "Resistor, 27K, 0603, +/-1%, 1/10W"                                                                      
R101       Resistor                       BottomLayer R0603                                                                                        113.5644     70.9873      0        "Resistor, 56K, 0603, +/-1%, 1/10W"                                                                      
R63        Resistor                       BottomLayer R0402                                                                                        142.3670     48.5141      270      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                        
R62        Resistor                       BottomLayer R0603                                                                                        143.8910     48.5141      270      "Resistor, 330R, 0603, +/-1%, 1/10W"                                                                     
R94        Resistor                       BottomLayer R0402                                                                                        116.9753     61.6955      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R93        Resistor                       BottomLayer R0402                                                                                        116.9753     60.4953      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R88        Resistor                       BottomLayer R0402                                                                                        119.8672     63.2596      90       "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                      
R86        Resistor                       BottomLayer R0402                                                                                        121.1372     63.2596      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R78        Resistor                       BottomLayer R0402                                                                                        131.1375     54.7679      0        "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                                    
R79        Resistor                       BottomLayer R0402                                                                                        131.1375     57.3079      0        "Resistor, 3K, 0402, +/-1%, 1/16W"                                                                       
R53        Resistor                       TopLayer    R0402                                                                                        138.8811     59.7130      0        "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                     
R54        Resistor                       TopLayer    R0402                                                                                        138.8811     55.9030      0        "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                     
R72        Resistor                       BottomLayer R0402                                                                                        138.8812     59.7127      180      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                      
R71        Resistor                       BottomLayer R0402                                                                                        138.8812     55.9027      180      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                      
R75        Resistor                       BottomLayer R0402                                                                                        133.9850     47.7521      270      "Resistor, 3K, 0402, +/-1%, 1/16W"                                                                       
R74        Resistor                       TopLayer    R0402                                                                                        127.9591     60.7290      90       "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R73        Resistor                       TopLayer    R0402                                                                                        126.8161     60.7290      90       "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R51        Resistor                       BottomLayer R0402                                                                                        122.1740     48.7680      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R56        Resistor                       BottomLayer R0402                                                                                        123.4440     48.7680      270      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                      
R52        Resistor                       BottomLayer R0402                                                                                        124.9111     48.7911      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R153       Resistor                       BottomLayer R0402                                                                                        21.6947      56.1270      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R155       Resistor                       BottomLayer R0402                                                                                        20.4247      56.1270      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R61        Resistor                       BottomLayer R0402                                                                                        145.2118     80.5367      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R65        Resistor                       BottomLayer R0402                                                                                        139.6479     81.3104      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
R58        Resistor                       TopLayer    R0402                                                                                        142.3676     82.0419      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R57        Resistor                       TopLayer    R0402                                                                                        142.3676     80.8989      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R32        Resistor                       TopLayer    R0402                                                                                        67.5099      69.8814      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R29        Resistor                       TopLayer    R0402                                                                                        65.9859      69.9393      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                       
R44        Resistor                       TopLayer    R0402                                                                                        81.7886      43.1799      180      "Resistor, 1K5, 0402, +/-1%, 1/16W"                                                                      
R8         Resistor                       BottomLayer R0402                                                                                        6.9850       77.0560      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                      
SB34       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       76.3270      70.6624      90       "Solder Bridge ON"                                                                                       
SB45       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       67.2051      47.9505      90       "Solder Bridge OFF"                                                                                      
SB43       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       68.7291      52.0145      90       "Solder Bridge OFF"                                                                                      
SB31       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       80.7506      52.3231      270      "Solder Bridge ON"                                                                                       
SB46       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       67.2051      51.9144      270      "Solder Bridge ON"                                                                                       
SB42       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       68.7291      47.8504      270      "Solder Bridge ON"                                                                                       
SB29       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       85.0401      33.9089      180      "Solder Bridge ON"                                                                                       
SB44       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       79.5791      37.7189      180      "Solder Bridge ON"                                                                                       
SB39       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       76.5810      36.2449      90       "Solder Bridge OFF"                                                                                      
SB41       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       72.1360      47.8019      90       "Solder Bridge ON"                                                                                       
SB40       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       57.5222      26.7970      0        "Solder Bridge ON"                                                                                       
SB37       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       78.3590      36.2449      90       "Solder Bridge ON"                                                                                       
SB33       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       73.9140      47.7018      270      "Solder Bridge ON"                                                                                       
SB32       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       76.9121      46.6089      180      "Solder Bridge OFF"                                                                                      
SB36       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                                                       78.7400      35.8513      90       "Solder Bridge 0402 ON"                                                                                  
SB35       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       76.9121      48.5139      180      "Solder Bridge ON"                                                                                       
SB30       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       81.3571      43.5609      180      "Solder Bridge ON"                                                                                       
SB38       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                                                       73.0250      20.2825      90       "Solder Bridge 0402 ON"                                                                                  
SB48       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                                                       61.7220      21.8816      90       "Solder Bridge 0402 ON"                                                                                  
SB60       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                                                       28.4105      25.6540      180      "Solder Bridge 0402 ON"                                                                                  
SB57       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                                                       28.4275      35.1790      0        "Solder Bridge 0402 ON"                                                                                  
SB61       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       24.6313      75.9690      0        "Solder Bridge ON"                                                                                       
SB64       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       17.3421      77.3160      270      "Solder Bridge ON"                                                                                       
SB65       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       16.3261      60.0170      90       "Solder Bridge OFF"                                                                                      
SB62       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       21.9710      44.0585      90       "Solder Bridge ON"                                                                                       
SB63       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       20.3200      44.0234      90       "Solder Bridge ON"                                                                                       
SB53       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       72.2630      51.8928      270      "Solder Bridge ON"                                                                                       
SB19       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       141.5635     73.7869      180      "Solder Bridge OFF"                                                                                      
SB59       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       37.5007      55.9109      0        "Solder Bridge ON"                                                                                       
SB58       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       37.5086      58.4509      0        "Solder Bridge ON"                                                                                       
SB27       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       97.0985      17.8109      180      "Solder Bridge OFF"                                                                                      
SB24       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       97.1386      11.9689      180      "Solder Bridge OFF"                                                                                      
SB56       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       37.9165      48.0369      180      "Solder Bridge ON"                                                                                       
SB26       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       97.0985      16.0329      180      "Solder Bridge ON"                                                                                       
SB25       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       97.0985      13.7469      180      "Solder Bridge ON"                                                                                       
SB1        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       78.7225      81.1966      90       "Solder Bridge OFF"                                                                                      
SB2        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       80.2465      81.1966      90       "Solder Bridge ON"                                                                                       
SB5        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       84.8185      81.1966      90       "Solder Bridge OFF"                                                                                      
SB6        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       86.3425      81.1966      90       "Solder Bridge ON"                                                                                       
SB7        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       87.8665      81.1887      90       "Solder Bridge OFF"                                                                                      
SB8        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       89.3905      81.1966      90       "Solder Bridge ON"                                                                                       
SB21       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       131.7494     28.5749      0        "Solder Bridge ON"                                                                                       
SB23       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       113.1335     68.5743      180      "Solder Bridge ON"                                                                                       
SB47       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       84.0526      52.3231      270      "Solder Bridge OFF"                                                                                      
SB4        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       83.2945      81.0965      270      "Solder Bridge ON"                                                                                       
SB9        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       90.9145      81.0696      270      "Solder Bridge ON"                                                                                       
SB12       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       95.4865      81.0696      270      "Solder Bridge ON"                                                                                       
SB14       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       98.5345      81.0696      270      "Solder Bridge ON"                                                                                       
SB16       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       101.7095     81.0774      270      "Solder Bridge ON"                                                                                       
SB18       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       104.7575     81.0696      270      "Solder Bridge ON"                                                                                       
SB3        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       46.8122      71.3224      90       "Solder Bridge OFF"                                                                                      
SB10       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       45.4914      71.3066      90       "Solder Bridge OFF"                                                                                      
SB11       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       49.4284      71.3066      90       "Solder Bridge OFF"                                                                                      
SB13       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       50.7492      71.3320      90       "Solder Bridge OFF"                                                                                      
SB15       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       52.0700      71.3320      90       "Solder Bridge OFF"                                                                                      
SB17       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                                                       48.1330      71.3224      90       "Solder Bridge OFF"                                                                                      
SB22       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       131.7494     33.7819      0        "Solder Bridge ON"                                                                                       
SW1        SW_MECA_1K2                    TopLayer    SWI_EAO_09-03290-01_EXTENDED_STRAIGHT_BLACK                                                  5.5880       28.1939      90       "Mechanical Slide Switches 1K2 BLK ACT GOLD STRT MNT"                                                    
TP9        "Test Point"                   BottomLayer TP_SMD_1MM                                                                                   65.0880      6.0499       0        "Test Point 1mm"                                                                                         
TP10       "Test Point"                   BottomLayer TP_SMD_1MM                                                                                   65.0880      10.1139      270      "Test Point 1mm"                                                                                         
TP8        "Test Point"                   BottomLayer TP_SMD_2MM                                                                                   100.9650     42.6719      180      "Test Point 2mm"                                                                                         
TP5        "Test Point"                   BottomLayer TP_SMD_2MM                                                                                   133.4262     20.2184      180      "Test Point 2mm"                                                                                         
TP2        "Test Point"                   TopLayer    TP_SMD_1MM                                                                                   142.4940     79.5019      0        "Test Point 1mm"                                                                                         
TP1        "Test Point"                   TopLayer    TP_SMD_1MM                                                                                   142.3670     77.0889      0        "Test Point 1mm"                                                                                         
TP3        "Test Point"                   BottomLayer TP_SMD_2MM                                                                                   134.6200     28.8289      0        "Test Point 2mm"                                                                                         
TP6        "Test Point"                   BottomLayer TP_SMD_2MM                                                                                   121.4374     68.8339      270      "Test Point 2mm"                                                                                         
TP7        "Test Point"                   BottomLayer TP_SMD_2MM                                                                                   110.4349     68.3203      270      "Test Point 2mm"                                                                                         
TP4        "Test Point"                   BottomLayer TP_SMD_1MM                                                                                   133.1689     54.7679      90       "Test Point 1mm"                                                                                         
TP17       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 69.0057      24.0260      0        "Test Point 0.6mm"                                                                                       
TP18       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 69.9963      26.5660      0        "Test Point 0.6mm"                                                                                       
TP19       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 70.2503      24.0006      0        "Test Point 0.6mm"                                                                                       
TP15       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 67.5579      25.2960      0        "Test Point 0.6mm"                                                                                       
TP20       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 68.5739      22.7814      0        "Test Point 0.6mm"                                                                                       
TP16       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 64.7893      24.0768      0        "Test Point 0.6mm"                                                                                       
TP12       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 62.3509      24.0260      0        "Test Point 0.6mm"                                                                                       
TP11       "Test Point"                   TopLayer    TP_SMD_1MM                                                                                   10.6934      74.1934      90       "Test Point 1mm"                                                                                         
TP14       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 66.9991      26.5660      0        "Test Point 0.6mm"                                                                                       
TP13       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 67.2277      24.0768      0        "Test Point 0.6mm"                                                                                       
U22        STM32H7S7L8H6H                 BottomLayer ICC_TFBGA225_13X13_P080_H1P10_CODE-A0L2__SOCKET_IRONWOOD_CS1222291-D6524MF_WITHOUT-3D-SOCKET 68.7878      34.3854      180      "MCU, ARM Cortex M7 32-bit, 64KB Flash, 620KB RAM, No Crypto"                                            
U6         ESD-TRANSIL                    TopLayer    ESD_0201_H0P3_1K_2A                                                                          140.4042     32.0039      180      "Diode, ESD TVS, 5V5, 100nA, 10V, 0201"                                                                  
U7         ESD-TRANSIL                    TopLayer    ESD_0201_H0P3_1K_2A                                                                          140.4626     19.4309      180      "Diode, ESD TVS, 5V5, 100nA, 10V, 0201"                                                                  
U23        MX66UW1G45GXDI00               BottomLayer ICC_BGA24_5X5-BALL-ARRAY_6X8_P1                                                              60.2620      10.1139      0        "Memory, Octo-SPI-NOR, 1Gb,x1/x8, Read-While-Write, 133/200MHz, 1.8V, DTR, BGA24"                        
U21        APS256XXN-OBR-BG               BottomLayer ICC_BGA24_5X5-BALL-ARRAY_6X8_P1                                                              76.3872      10.1139      0        "Memory,Hexa-SPI-PSRAM,256Mb,x8x16,200MHz,1.8V,DDR,BGA24, PASR LVCMOS"                                   
U19        USBLC6-4SC6                    BottomLayer ESD_SOT23-6L                                                                                 114.0659     29.9905      180      "Very low capacitance ESD protection , 4 lines"                                                          
U18        LAN8742A-CZ-TR                 BottomLayer ICC_VQFN24-EPAD_4X4_P050                                                                     114.8277     39.7793      0        "10/100M RMII Ethernet transceiver"                                                                      
U24        WM8904CGEFL/RV                 BottomLayer ICC_QFN32-EPAD_4X4_P040                                                                      23.9675      29.2300      270      "Audio Codec, Ultra Low-Power Codec for Portable Audio Applications"                                     
U28        ESDA6V1BC6                     BottomLayer ESD_SOT23-6L                                                                                 20.7006      17.4304      270      "Quad Bidir ESD protection"                                                                              
U2         STG4160                        TopLayer    ESD_FLIP-CHIP-BGA8_1P9X0P9_P050                                                              8.7530       71.9040      270      "Low voltage 0.5 ohm single SPDT switch with break-before-make feature and 15 kV contact ESD protection" 
U26        TCPP03-M20                     BottomLayer ICC_QFN20-EPAD_4X4_P050                                                                      20.8063      60.1910      0        "USB Type-C Port Protection for USB DRP Power Delivery, PPS compliant"                                   
U31        ESD-TRANSIL                    TopLayer    ESD_QFN1610_2N_1K_2A                                                                         10.2301      57.1730      270      "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."                     
U30        ECMF2-40A100N6                 BottomLayer ESD_UQFN-6L_1P45X1P4_P040                                                                    11.1506      60.3884      90       "IC, ESD protection and Common Filter High Speed serial Interfaces, 10.7 GHz"                            
U32        ESD-TRANSIL                    BottomLayer ESD_QFN1610_2N_1K_2A                                                                         13.0810      43.9424      90       "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."                     
U27        TCPP01-M12                     BottomLayer ICC_QFN12L-EPAD_3X3_P050                                                                     20.9556      39.9094      270      "USB Type-C Port Protection for USB Power Delivery, PPS compliant"                                       
U29        ECMF2-40A100N6                 BottomLayer ESD_UQFN-6L_1P45X1P4_P040                                                                    10.5410      40.3859      90       "IC, ESD protection and Common Filter High Speed serial Interfaces, 10.7 GHz"                            
U3         EMIF06-MSD02N16                TopLayer    ESD_UQFN16L-EPAD_3P5X1P2_P040                                                                48.0060      74.9299      0        "ESD protection for SD card 2.0"                                                                         
U20        LD1117S50TR                    BottomLayer REG_SOT223-TAB                                                                               103.3578     36.4519      180      "IC REG LDO 5V 0.8A SOT223"                                                                              
U15        ST1L05CPU33R                   BottomLayer ICC_DFN6-EPAD_3X3_P095                                                                       127.0006     29.8454      0        "LDO, 3.3V, 1.3A, Very low quiescent current BiCMOS voltage regulator"                                   
U17        ST1L05BPUR                     BottomLayer ICC_DFN6-EPAD_3X3_P095                                                                       118.0095     70.9878      270      "LDO Linear Voltage Regulator IC Positive Adjustable 1 Output Adjustable 1.3A 6-DFN (3x3)"               
U14        STLINK-V3EC                    BottomLayer ICC_UFBGA201_176+25_10X10_P065                                                               123.6125     56.1095      0        "MCU, Arm Cortex-M7 32-bit MCU, 512KB Flash, 276KB RAM, With Crypto"                                     
U4         ESDALC6V1W5                    BottomLayer ESD_SOT323-5L                                                                                135.1981     78.2549      0        "Dual Transil array for ESD protection"                                                                  
U9         ESD-TRANSIL                    BottomLayer ESD_QFN1610_2N_1K_2A                                                                         139.0085     63.3957      180      "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."                     
U11        ESDALC6V1W5                    BottomLayer ESD_SOT323-5L                                                                                135.1981     74.3179      180      "Dual Transil array for ESD protection"                                                                  
U10        ESDALC6V1W5                    BottomLayer ESD_SOT323-5L                                                                                135.1981     69.7459      180      "Dual Transil array for ESD protection"                                                                  
U8         ECMF2-40A100N6                 BottomLayer ESD_UQFN-6L_1P45X1P4_P040                                                                    138.9380     58.2167      270      "IC, ESD protection and Common Filter High Speed serial Interfaces, 10.7 GHz"                            
U13        TPS259535DSG                   BottomLayer ICC_WSON8-EPAD_2X2_P050                                                                      133.3006     50.4613      270      "IC, eFuse with Fast Overvoltage Protection 2.7V to 18V 4A 34mOhm 8-Pin WSON"                            
X3         OSCILLATOR_4_PINS              BottomLayer CRY_NZ2016SH_4P                                                                              83.1370      26.9098      180      "Oscillator, SPXO, 24MHz, +/-50ppm, square wave, 3V3, 2x1.6mm"                                           
X2         XTAL_2_PINS                    BottomLayer CRY_NX2012SA_2P                                                                              84.3504      39.8766      90       "Crystal, 32.768kHz, 6pF, +/-20ppm, 80K, 2.05x1.2mm"                                                     
CN14       "Socket 8x1"                   BottomLayer CON_SAMTEC_SSW-108-22-X-S-VS                                                                 43.3451      22.4601      270      "Socket, 8x1, 2.54mm, VR, SMD, T=9.78mm"                                                                 
D1         SCHOTTKY_1A_2K                 BottomLayer DIO_SOD523_1A_2K                                                                             63.3728      4.8260       270      "Small signal Schottky diodes"                                                                           
LD10       LED_green                      BottomLayer LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4                                                 136.2706     25.6032      0        "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                  
R69        Resistor                       BottomLayer R0603                                                                                        135.4836     23.5204      90       "Resistor, 1K2, 0603, +/-1%, 1/10W"                                                                      
R70        Resistor                       BottomLayer R0603                                                                                        21.9710      47.1169      180      "Resistor, 33K, 0603, +/-1%, 1/10W"                                                                      
C32        Capacitor                      TopLayer    C0402                                                                                        68.6562      38.3544      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                
C158       Capacitor                      BottomLayer C1206_H1P6                                                                                   125.4760     9.7789       90       "Capacitor, MLCC, 1nF, 2KV, X7R, +/-10%, 1206, T=1.25mm"                                                 
C159       Capacitor                      BottomLayer C0402                                                                                        111.2772     39.1160      90       "Capacitor, MLCC, 8.2 pF, NPO, COG, 50V, +/-0.1pF, 0402, T=0.5mm"                                        
C160       Capacitor                      BottomLayer C0402                                                                                        111.2520     41.0210      270      "Capacitor, MLCC, 8.2 pF, NPO, COG, 50V, +/-0.1pF, 0402, T=0.5mm"                                        
CN7        USB_TYPE_C_Receptacle          BottomLayer CON_USB-TYPEC_AMPHENOL_12401826E412A                                                         144.5136     58.4197      270      "USB_TypeC, 24 pins, RA, SMD, T=2.96mm"                                                                  
CN17       USB_TYPE_C_Receptacle          BottomLayer CON_USB-TYPEC_AMPHENOL_12401826E412A                                                         5.4163       40.1572      90       "USB_TypeC, 24 pins, RA, SMD, T=2.96mm"                                                                  
CN18       USB_TYPE_C_Receptacle          BottomLayer CON_USB-TYPEC_AMPHENOL_12401826E412A                                                         5.4163       60.1979      90       "USB_TypeC, 24 pins, RA, SMD, T=2.96mm"                                                                  
R172       Resistor                       TopLayer    R0402                                                                                        113.6651     16.3829      180      "Resistor, 75R, 0402, +/-1%, 1/16W"                                                                      
R173       Resistor                       TopLayer    R0402                                                                                        113.6651     15.2399      180      "Resistor, 75R, 0402, +/-1%, 1/16W"                                                                      
R174       Resistor                       TopLayer    R0402                                                                                        118.3640     15.8749      270      "Resistor, 75R, 0402, +/-1%, 1/16W"                                                                      
R175       Resistor                       TopLayer    R0402                                                                                        117.0940     15.8749      270      "Resistor, 75R, 0402, +/-1%, 1/16W"                                                                      
R177       Resistor                       BottomLayer R0402                                                                                        132.3340     52.4510      0        "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                     
SB68       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       82.4016      52.3231      270      "Solder Bridge ON"                                                                                       
SB69       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       125.4760     5.0298       270      "Solder Bridge ON"                                                                                       
SB70       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       104.0130     5.0298       270      "Solder Bridge ON"                                                                                       
SB71       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       140.4620     41.3250      90       "Solder Bridge ON"                                                                                       
SB72       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       72.2630      55.1948      270      "Solder Bridge OFF"                                                                                      
SB73       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       77.0890      55.1696      270      "Solder Bridge OFF"                                                                                      
SB74       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       104.1820     71.1708      180      "Solder Bridge OFF"                                                                                      
SB75       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       143.8998     71.1454      180      "Solder Bridge OFF"                                                                                      
SB76       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       98.7044      72.2158      90       "Solder Bridge OFF"                                                                                      
SB77       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       143.9252     67.9450      180      "Solder Bridge OFF"                                                                                      
TP21       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 66.0085      24.0768      90       "Test Point 0.6mm"                                                                                       
TP22       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 65.7799      26.5660      90       "Test Point 0.6mm"                                                                                       
TP23       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 68.7771      26.5660      90       "Test Point 0.6mm"                                                                                       
TP24       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 64.5607      26.5660      90       "Test Point 0.6mm"                                                                                       
TP25       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 63.5701      24.0260      90       "Test Point 0.6mm"                                                                                       
TP26       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 63.3161      26.5660      90       "Test Point 0.6mm"                                                                                       
TP27       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 72.4347      26.5152      90       "Test Point 0.6mm"                                                                                       
TP28       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 74.1111      23.0608      90       "Test Point 0.6mm"                                                                                       
TP29       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 71.2155      26.5660      90       "Test Point 0.6mm"                                                                                       
TP30       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 72.5363      24.0006      90       "Test Point 0.6mm"                                                                                       
TP31       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 71.4187      22.6036      90       "Test Point 0.6mm"                                                                                       
TP32       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 58.7441      35.9640      90       "Test Point 0.6mm"                                                                                       
TP33       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 60.2681      34.4400      90       "Test Point 0.6mm"                                                                                       
TP34       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 58.7441      30.5030      90       "Test Point 0.6mm"                                                                                       
TP35       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 58.7441      31.7730      90       "Test Point 0.6mm"                                                                                       
TP36       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 60.3951      35.9640      90       "Test Point 0.6mm"                                                                                       
TP37       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 58.7441      29.1060      90       "Test Point 0.6mm"                                                                                       
TP38       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 60.1411      30.5030      90       "Test Point 0.6mm"                                                                                       
TP39       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 60.1411      28.9790      90       "Test Point 0.6mm"                                                                                       
TP40       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 60.2681      31.7730      90       "Test Point 0.6mm"                                                                                       
TP41       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 58.7441      33.0430      90       "Test Point 0.6mm"                                                                                       
TP42       "Test Point"                   TopLayer    TP_SMD_0-6MM                                                                                 58.7441      34.4400      90       "Test Point 0.6mm"                                                                                       
U33        KMS-1102NL                     BottomLayer TRS_DGKYD_KMS-1102NL                                                                         113.8621     20.4699      0        "Discrete Magnetic Transformer Module, 16 pins, SMT, 100 Base-TX"                                        
X4         XTAL_4_PINS                    BottomLayer CRY_NX2016SA_4P                                                                              109.6010     40.0048      90       "Crystal, 25MHz, 6pF, +/-20ppm, 80R, 2x1.6mm"                                                            
SB51       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                                                       101.6254     61.7308      90       "Solder Bridge ON"                                                                                       
U1         MP23DB01MMTR                   BottomLayer MIC_STM_MP23DB01MMTR                                                                         9.1945       78.0528      0        "MEMS sensors , omnidirectionnal digital microphone"                                                     
