Altium Designer Pick and Place Locations
E:\Documents\Projets\CAP1G\STM_Le Mans\Projets\MB1779B\BASE\MB1779B\02-Manufacturing\MB1779B_PCB\Assembly\MB1779-B01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       29/04/22
Time:       09:41
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment              Layer       Footprint                                       Center-X(mm) Center-Y(mm) Rotation Description                                                                                                       
R15         Resistor             TopLayer    R0201_H0P23                                     46.7250      23.9250      180      "Resistor, 0R, 0201, 1/20W"                                                                                       
R14         Resistor             TopLayer    R0201_H0P23                                     47.3250      23.9250      180      "Resistor, 0R, 0201, 1/20W"                                                                                       
R13         Resistor             TopLayer    R0201_H0P23                                     49.6150      21.9000      90       "Resistor, 0R, 0201, 1/20W"                                                                                       
R12         Resistor             TopLayer    R0201_H0P23                                     49.6150      21.3000      90       "Resistor, 0R, 0201, 1/20W"                                                                                       
C13         ""                   TopLayer    C0402                                           18.0500      18.9250      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
Designator1 Comment              TopLayer    Sheetbox_2L2S                                   29.7186      -17.8734     0        ""                                                                                                                
Designator4 Comment              BottomLayer MIRE_PLACE_SMD_0P8MM                            56.6000      7.8500       180      ""                                                                                                                
Designator2 Comment              BottomLayer MIRE_PLACE_SMD_0P8MM                            57.3750      27.8750      180      ""                                                                                                                
Designator3 Comment              BottomLayer MIRE_PLACE_SMD_0P8MM                            2.3750       27.7500      180      ""                                                                                                                
2           Comment              TopLayer    MIRE_PLACE_SMD_0P8MM                            2.3750       27.7500      0        ""                                                                                                                
3           Comment              TopLayer    MIRE_PLACE_SMD_0P8MM                            56.4250      9.4000       0        ""                                                                                                                
1           Comment              TopLayer    MIRE_PLACE_SMD_0P8MM                            57.3750      27.8750      0        ""                                                                                                                
U3          STM32WL5MOCH6S       TopLayer    MOD_LGA92_10X10_P055                            43.9750      18.3000      180      "RF module including STM32WL55JC MCU, oscillators and RF front-end"                                               
SB37        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          46.3125      3.8750       0        "Solder Bridge 0402 ON"                                                                                           
SB28        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          22.6375      12.7250      180      "Solder Bridge 0402 ON"                                                                                           
SB20        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          22.7125      16.1000      0        "Solder Bridge 0402 ON"                                                                                           
SB26        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          22.7125      13.8250      0        "Solder Bridge 0402 ON"                                                                                           
SB23        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          22.7125      15.0000      0        "Solder Bridge 0402 ON"                                                                                           
SB25        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          27.0875      13.8750      180      "Solder Bridge 0402 ON"                                                                                           
C23         ""                   TopLayer    C0402                                           22.1750      13.2750      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
SB31        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       9.3500       180      "Solder Bridge ON"                                                                                                
SB30        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       10.7500      180      "Solder Bridge ON"                                                                                                
SB29        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       12.1500      180      "Solder Bridge ON"                                                                                                
SB27        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       13.5500      180      "Solder Bridge ON"                                                                                                
SB11        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          7.0500       20.5500      0        "Solder Bridge ON"                                                                                                
SB10        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          7.0500       21.9500      0        "Solder Bridge ON"                                                                                                
SB12        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          17.0000      20.1375      270      "Solder Bridge 0402 ON"                                                                                           
SB32        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          15.3250      8.6625       270      "Solder Bridge 0402 ON"                                                                                           
SB38        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          3.0750       3.3750       180      "Solder Bridge ON"                                                                                                
R5          Resistor             TopLayer    R0402                                           22.0375      7.4675       0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                               
R4          Resistor             TopLayer    R0402                                           49.2250      11.2750      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                               
JP1         ""                   TopLayer    CON_SAMTEC_TSW-102-07-G-S                       35.3250      4.2000       270      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                     
SB15        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          21.3250      19.2000      180      "Solder Bridge ON"                                                                                                
SB14        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          24.1250      19.2250      180      "Solder Bridge ON"                                                                                                
CN5         ""                   TopLayer    CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1         9.7000       3.7750       90       "Header, 2x1, 2.54mm, VR, TH, Height 6mm/3mm"                                                                     
U9          ""                   TopLayer    ESD_ST0201                                      52.4250      6.8000       270      "ESD protection 6V1"                                                                                              
SB2         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          11.8250      26.2625      270      "Solder Bridge 0402 ON"                                                                                           
SB17        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          19.1750      18.3125      90       "Solder Bridge 0402 ON"                                                                                           
R11         ""                   TopLayer    R0402                                           52.5250      2.3000       90       Resistor,100R,0402,1%,1/16W                                                                                       
CN3         "Header 7x2"         TopLayer    CON_STDC14_Receiver_SMALL                       46.4250      5.0750       0        "Header, 7x2, 1.27mm, VR, SMD, T=5.97mm"                                                                          
U15         ""                   BottomLayer ESD_SOT323-5L                                   47.1750      7.1000       270      "Dual Transil array for ESD protection"                                                                           
U10         MX25L4006EZNI-12G    TopLayer    ICC_WSON8-EPAD_6X5_P127                         20.3750      3.8500       0        "Low Power, 3V, 4M-BIT Serial Flash Memory"                                                                       
U7          IIS2MDCTR            TopLayer    ICC_LGA12_2X2_P050_H0P7                         16.0250      13.8000      90       "High-accuracy, ultra-low-power, 3-axis, digital output magnetometer"                                             
U4          ILPS22QS             TopLayer    ICC_HLGA10_2X2_P050                             19.4000      21.8000      270      "Dual full-scale, 1.26 bar and 4 bar, absolute digital output barometer with QVAR detection in full-mold package" 
U2          ISM330DHCX           TopLayer    ICC_LGA14_3X2P5_P050                            14.2250      22.4750      0        "iNEMO inertial module: 3D accelerometer and 3D gyroscope, with digital output for industrial applications"       
U14         STTS22H              TopLayer    ICC_UDFN6-EPAD_2X2_P065                         13.8500      3.1000       180      "temperature sensor"                                                                                              
SB13        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          15.8750      19.7875      270      "Solder Bridge 0402 ON"                                                                                           
SB21        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          13.2625      15.8750      180      "Solder Bridge 0402 ON"                                                                                           
SB34        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          25.2500      7.7625       90       "Solder Bridge 0402 ON"                                                                                           
SB9         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          22.3500      21.8875      270      "Solder Bridge 0402 ON"                                                                                           
SB33        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          14.2250      8.7375       90       "Solder Bridge 0402 ON"                                                                                           
SB22        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       14.9500      180      "Solder Bridge ON"                                                                                                
SB19        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       16.3500      180      "Solder Bridge ON"                                                                                                
SB18        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       17.7500      180      "Solder Bridge ON"                                                                                                
SB16        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       19.1500      180      "Solder Bridge ON"                                                                                                
SB6         ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       23.3500      180      "Solder Bridge ON"                                                                                                
SB4         ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       24.7500      180      "Solder Bridge ON"                                                                                                
SB3         ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       26.1500      180      "Solder Bridge ON"                                                                                                
SB1         ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          6.9500       27.5500      180      "Solder Bridge ON"                                                                                                
R1          Resistor             TopLayer    R0402                                           39.0000      24.1250      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                               
R2          Resistor             TopLayer    R0402                                           37.5500      22.7000      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                               
CN4         ""                   TopLayer    CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1         6.6000       3.7750       90       "Header, 2x1, 2.54mm, VR, TH, Height 6mm/3mm"                                                                     
C24         Capacitor            TopLayer    C0402                                           15.8250      11.9250      0        "Capacitor, MLCC, 10uF, 10V, X5R, 20%, 0402, T=0,5mm"                                                             
C22         Capacitor            TopLayer    C0402                                           18.6000      13.5000      90       "Capacitor, MLCC, 220nF, 16V, 0402, X7R, 10%, T=0,5mm"                                                            
C25         ""                   TopLayer    C0402                                           19.4625      7.4675       0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C18         ""                   TopLayer    C0402                                           14.3500      15.8750      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C21         ""                   TopLayer    C0402                                           13.0250      14.8750      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C7          ""                   TopLayer    C0402                                           22.2250      21.9500      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C6          ""                   TopLayer    C0603                                           23.3500      21.7250      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                            
C5          ""                   TopLayer    C0402                                           10.9000      22.0750      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C3          ""                   TopLayer    C0402                                           17.0000      22.8500      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C27         ""                   TopLayer    C0402                                           12.0750      5.7250       0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
SW2         ""                   TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS             27.0750      2.6750       0        "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                               
SW1         ""                   TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS             55.7200      2.4250       180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                               
C29         ""                   TopLayer    C0402                                           29.1000      5.5750       0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C28         ""                   TopLayer    C0402                                           57.2950      5.6750       360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C4          ""                   TopLayer    C0402                                           27.7500      22.6500      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C9          ""                   TopLayer    C0603                                           29.8500      19.7000      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                              
C10         ""                   TopLayer    C0603                                           24.7000      19.7000      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                              
C11         ""                   TopLayer    C0402                                           23.5750      19.7000      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C2          ""                   TopLayer    C0402                                           48.3750      25.4000      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C8          ""                   TopLayer    C0603                                           34.3250      20.2250      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                            
C12         ""                   TopLayer    C0402                                           37.1750      19.7750      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C17         ""                   TopLayer    C0603                                           34.3250      17.5250      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                            
C14         ""                   TopLayer    C0603                                           34.3250      18.8750      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                            
C15         ""                   TopLayer    C0402                                           37.1750      18.8750      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C16         ""                   TopLayer    C0402                                           37.1750      17.9750      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                            
C1          ""                   TopLayer    C0603                                           48.7000      26.5250      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                            
C20         Capacitor            TopLayer    C0402                                           53.5300      15.4500      270      "Capacitor, MLCC, 3.3pF, 50V, NPO, +/-0.1pF, 0402, T=0,5mm"                                                       
C19         Capacitor            TopLayer    C0402                                           50.2790      15.4500      270      "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                                         
CN1         "Header 10x2 STMod+" TopLayer    CON_SAMTEC_TMM-110-01-L-D-RA__STMOD+            2.2700       15.0000      270      "Header 10x2, 2mm, RA, TH, Height 3.20mm/3.50mm"                                                                  
CN2         ""                   TopLayer    CON_SAMTEC_SMA-J-P-X-ST-EM1                     57.5500      15.0000      90       "RF SMA connector PCB edge"                                                                                       
JP2         ""                   TopLayer    CON_SAMTEC_TSW-102-07-G-S                       38.4750      4.2000       270      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                     
L1          Inductor             TopLayer    IND_0402_MURATA_LQW15AN_H0P5                    51.9040      14.9880      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                
LD4         ""                   TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4    4.2250       2.6250       270      "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                           
LD2         ""                   TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4    31.7295      2.6375       270      "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                           
LD3         ""                   TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8     33.0875      2.6375       270      "LED Red, 0603 SMD, 2V Forward Voltage"                                                                           
LD1         ""                   TopLayer    LED_0603_OSRAM_LB-Q39G-L2OO-35-1_BLUE_1A2K_H0P4 30.3845      2.6375       270      "LED Blue, 0603 SMD, Forward Voltage Min=2,8V, Max=3,8V"                                                          
R10         ""                   TopLayer    R0402                                           2.6750       3.3750       0        Resistor,620R,0402,1%,1/16W                                                                                       
R6          ""                   TopLayer    R0402                                           53.6700      5.2250       90       Resistor,1K,0402,1%,1/16W                                                                                         
R3          Resistor             TopLayer    R0402                                           49.2250      12.3250      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                               
R9          ""                   TopLayer    R0402                                           31.7375      4.8375       270      Resistor,270R,0402,1%,1/16W                                                                                       
R7          Resistor             TopLayer    R0402                                           32.7750      4.8250       270      "Resistor, 390R, 0402, +/-1%, 1/16W"                                                                              
R8          ""                   TopLayer    R0402                                           30.5750      4.8250       270      Resistor,120R,0402,1%,1/16W                                                                                       
SB35        ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          12.6500      6.9250       0        "Solder Bridge ON"                                                                                                
U12         ""                   TopLayer    ESD_ST0201                                      57.4450      4.8000       180      "ESD protection 6V1"                                                                                              
U13         ""                   TopLayer    ESD_ST0201                                      29.1750      4.7375       180      "ESD protection 6V1"                                                                                              
U6          ""                   TopLayer    ICC_DFN6-EPAD_3X3_P095                          27.2750      20.3000      180      "Low quiescent current and low noise voltage regulators"                                                          
U1          XS3A1T3157GSH        TopLayer    ICC_SOT1202_XSON6                               46.2500      26.3250      0        "DC switch - Ultra-Low 0.5ohm - SPDT analog switch"                                                               
U5          XS3A1T3157GSH        TopLayer    ICC_SOT1202_XSON6                               50.8000      21.9000      180      "DC switch - Ultra-Low 0.5ohm - SPDT analog switch"                                                               
SB8         ""                   BottomLayer SOLDER-BRIDGE_R0603-0R                          23.5500      21.5750      90       "Solder Bridge ON"                                                                                                
C26         Capacitor            TopLayer    C0402                                           12.0750      6.5250       0        "Capacitor, MLCC, 2.2uF, 6V3, X5R,+/-10%, 0402, T=0.5mm"                                                          
SB7         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          37.0625      23.0000      180      "Solder Bridge 0402 ON"                                                                                           
SB5         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          37.0625      24.1000      180      "Solder Bridge 0402 ON"                                                                                           
SB36        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          25.2500      3.8125       270      "Solder Bridge 0402 ON"                                                                                           
SB24        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          18.6000      13.6625      90       "Solder Bridge 0402 ON"                                                                                           
U8          M24128-DFMC6TP       TopLayer    ICC_DFN8-EPAD_2X3_P050                          27.0750      12.4000      90       "I2C Memory 3V3, 256Kbits, 2x3,0.55mm, UFDFPN8"                                                                   
U11         ""                   TopLayer    ESD_ST0201                                      52.4250      4.5750       270      "ESD protection 6V1"                                                                                              
