Altium Designer Pick and Place Locations
C:\Users\galvagng\OneDrive - STMicroelectronics\Documents\Validation Reference Design\Zip folder to stwebsite publication\MB2158\Project Outputs\02-Manufacturing\MB2158A_PCB\Assembly\MB2158A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       25/10/24
Time:       18:38
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator     Comment                             Layer       Footprint                       Center-X(mm) Center-Y(mm) Rotation Description                                                                        
R1             Resistor                            TopLayer    GRM155--GJM155-0_05-MFG         21.9000      50.4750      0        "0 ohm resistor"                                                                   
SB1            SB_ON                               TopLayer    SOLDER-BRIDGE_R0201_0R          19.0750      26.8000      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                    
SB7            SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.1649      12.8877      180      "Solder Bridge 0402 ON"                                                            
Cover1         "TopCover_WE-SHC Shielding Cabinet" TopLayer    3600637250S                     -265.4530    -237.3752    90       "two-piece frame 37.7*25*5.8 mm"                                                   
SC9            Shield-clip                         TopLayer    3690000                         34.1389      30.5786      270      "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC10           Shield-clip                         TopLayer    3690000                         8.9388       30.5787      90       "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC8            Shield-clip                         TopLayer    3690000                         8.9389       15.6377      90       "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC7            Shield-clip                         TopLayer    3690000                         13.0489      11.6287      0        "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC6            Shield-clip                         TopLayer    3690000                         30.0292      11.6287      0        "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC5            Shield-clip                         TopLayer    3690000                         34.1389      15.6377      270      "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC4            Shield-clip                         TopLayer    3690000                         34.1389      45.5197      270      "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC3            Shield-clip                         TopLayer    3690000                         30.0289      49.5287      0        "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC2            Shield-clip                         TopLayer    3690000                         13.0484      49.5287      0        "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
SC1            Shield-clip                         TopLayer    3690000                         8.9389       45.5194      90       "shield clip Wurth Elektronik  to fix RF shielded cavity"                          
Frame1         "Frame_WE-SHC Shielding Cabinet"    TopLayer    3610637256S                     -265.4530    -237.3752    90       "two-piece frame 37.7*25*5.8 mm"                                                   
C14            Capacitor                           TopLayer    C0402                           13.6250      26.5500      90       "Capacitor, MLCC, 100pF, 50V, COG, 1%, 0402, T=0.5mm"                              
U2             SKY66121-11                         TopLayer    SKY65367-11                     18.4750      40.5049      90       "169 to 170 MHz Transmit / Receive Front-End  Module for 27 dBm (no BYPASS funct)" 
L1             Inductor                            TopLayer    L0402                           21.5000      52.7750      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                 
C35            Capacitor                           TopLayer    C0402                           21.9500      41.3219      180      "Capacitor, MLCC,  22pF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
C31            Capacitor                           TopLayer    C0402                           12.0680      41.7672      90       "Capacitor, MLCC,  4.7nF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                         
C37            Capacitor                           TopLayer    C0402                           17.2250      37.6434      0        ""                                                                                 
L21            Inductor                            TopLayer    L0402                           17.6750      36.4100      90       "Inductor, 27nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"            
C40            Capacitor                           TopLayer    C0402                           17.2248      35.1725      0        "Capacitor, MLCC,  22pF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
C7             Capacitor                           TopLayer    C0402                           15.0772      25.0250      180      "Capacitor, MLCC, 10nF, 50V, COG, +/-1%, 0402, T=0.5mm"                            
C3             Capacitor                           TopLayer    C0402                           17.7875      24.0500      180      "Capacitor, MLCC, 1nF, 50V, C0G, +/-0.1pF, 0402, T=0.5mm"                          
SB20           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          9.2619       8.3799       180      "Solder Bridge 0402 ON"                                                            
L20            Inductor                            TopLayer    L0402                           10.8807      40.8421      90       "Inductor, 10nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"            
L19            Inductor                            TopLayer    L0402                           23.8000      48.2824      0        ""                                                                                 
L18            Inductor                            TopLayer    C0603_coilcraft                 21.5000      46.5025      90       "0R resistor"                                                                      
L17            Inductor                            TopLayer    L0402                           23.8000      44.7682      0        "Inductor, 4.7nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"           
L16            Inductor                            TopLayer    C0603_coilcraft                 21.5000      43.0922      90       "Inductor, 47nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"            
L15            Inductor                            TopLayer    C0603_coilcraft                 14.8177      41.3172      180      "Inductor, 10nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"            
L14            Inductor                            TopLayer    L0402                           14.9447      39.7172      180      "Inductor, 15nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"            
L13            Inductor                            TopLayer    C0603_coilcraft                 17.4435      45.2499      0        "Inductor, 27nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"            
L12            Inductor                            TopLayer    L0402                           15.6750      47.4500      90       "Inductor, 2.7nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"           
L11            Inductor                            TopLayer    C0603_coilcraft                 15.6745      43.5182      90       "Inductor, 7.5nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"           
C39            Capacitor                           TopLayer    C0402                           11.7697      39.2672      270      "Capacitor, MLCC,  1uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                           
C38            Capacitor                           TopLayer    C0402                           21.9500      48.2542      180      ""                                                                                 
C36            Capacitor                           TopLayer    C0402                           21.9500      44.7682      180      "Capacitor, MLCC,  18pF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
C34            Capacitor                           TopLayer    C0402                           19.2750      45.6999      270      "Capacitor, MLCC,  27pF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
C33            Capacitor                           TopLayer    C0402                           19.2750      43.8749      90       "Capacitor, MLCC,  2.2nF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                         
C32            Capacitor                           TopLayer    C0402                           15.6750      45.7182      270      "Capacitor, MLCC,  82pF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
C30            Capacitor                           TopLayer    C0402                           13.5477      39.2672      270      ""                                                                                 
C29            Capacitor                           TopLayer    C0402                           12.8441      41.7672      90       "Capacitor, MLCC,  1uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                           
C28            Capacitor                           TopLayer    C0402                           12.6587      39.2672      270      "Capacitor, MLCC,  1nF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                           
C27            Capacitor                           TopLayer    GRM185C80J475ME11D              10.8807      43.4159      90       "Capacitor, MLCC,  4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                         
SB11           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2125      7.1875       180      "Solder Bridge 0402 ON"                                                            
SB17           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2125      3.8125       180      "Solder Bridge 0402 ON"                                                            
SB6            SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2399      11.7516      0        "Solder Bridge 0402 ON"                                                            
SB9            SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2875      9.4375       0        "Solder Bridge 0402 ON"                                                            
STICKER-BOARD1 Comment                             TopLayer    STICKER_BOARD_25X5              -265.4530    -237.3752    90       ""                                                                                 
STICKER-PROD1  Comment                             TopLayer    STICKER_PRODUCT_25X5            -265.4530    -237.3752    90       ""                                                                                 
MIRE-6         Comment                             BottomLayer MIRE_PLACE_SMD_0P8MM            13.0000      2.4500       180      ""                                                                                 
MIRE-4         Comment                             BottomLayer MIRE_PLACE_SMD_0P8MM            39.5940      56.6250      180      ""                                                                                 
MIRE-5         Comment                             BottomLayer MIRE_PLACE_SMD_0P8MM            3.2500       56.6250      180      ""                                                                                 
MIRE-3         Comment                             TopLayer    MIRE_PLACE_SMD_0P8MM            2.5000       2.4500       0        ""                                                                                 
MIRE-2         Comment                             TopLayer    MIRE_PLACE_SMD_0P8MM            39.5940      56.6250      0        ""                                                                                 
MIRE-1         Comment                             TopLayer    MIRE_PLACE_SMD_0P8MM            3.2500       56.6250      0        ""                                                                                 
X1             XTAL_2_PINS                         TopLayer    CRY_NX2012SA_2P                 28.9000      30.5000      90       "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                               
X2             48MHz                               TopLayer    NT2016SJA                       15.5272      23.4500      0        "TCXO 48 MHz  NDK Spec. No.:END6296A"                                              
U1             STM32WL33                           TopLayer    ICC_QFN48-EPAD-4P5X4P5_6X6_P040 23.3500      23.4500      180      "IC, Programmable Sub-1GHz wireless SoC"                                           
SB2            SB_ON                               TopLayer    SOLDER-BRIDGE_R0201_0R          19.0750      25.9000      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                    
SB15           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2875      4.9375       0        "Solder Bridge 0402 ON"                                                            
SB14           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          9.3125       5.2000       0        "Solder Bridge 0402 ON"                                                            
SB3            SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.5875      31.2500      0        "Solder Bridge 0402 ON"                                                            
SB19           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2875      1.5625       0        "Solder Bridge 0402 ON"                                                            
SB4            SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.5875      30.1500      0        "Solder Bridge 0402 ON"                                                            
SB18           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2125      2.6875       180      "Solder Bridge 0402 ON"                                                            
SB12           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          9.2375       7.1250       180      "Solder Bridge 0402 ON"                                                            
SB16           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          9.3125       3.9500       0        "Solder Bridge 0402 ON"                                                            
SB13           SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2875      6.0625       0        "Solder Bridge 0402 ON"                                                            
SB8            SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.2125      10.5625      180      "Solder Bridge 0402 ON"                                                            
SB5            SB_ON                               BottomLayer SOLDER-BRIDGE_R0402-0R          33.7875      19.8250      0        "Solder Bridge 0402 ON"                                                            
R7             Resistor                            TopLayer    R0402                           26.9750      3.8750       270      Resistor,47R,0402,1%,1/16W                                                         
R6             Resistor                            TopLayer    R0402                           26.9750      7.0500       270      Resistor,47R,0402,1%,1/16W                                                         
R5             Resistor                            TopLayer    R0402                           24.0500      9.9500       90       Resistor,47R,0402,1%,1/16W                                                         
R8             Resistor                            TopLayer    R0402                           26.9750      2.0750       270      Resistor,47R,0402,1%,1/16W                                                         
R2             Resistor                            TopLayer    R0402                           31.7625      24.0500      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                               
R4             Resistor                            TopLayer    R0402                           20.2250      9.9500       90       Resistor,47R,0402,1%,1/16W                                                         
R3             Resistor                            TopLayer    R0402                           18.9500      9.9500       90       Resistor,47R,0402,1%,1/16W                                                         
L3             Inductor                            TopLayer    L0402                           24.5500      32.1601      0        "Inductor, MLCC, 5.6nH, ±0.3nH, 650mA, 180mR, 0402, T=0.5mm"                       
L4             Inductor                            TopLayer    L0402                           24.1000      30.9406      90       "Inductor, 6.8nH, +/-3%, 0.6A, 220mR, 0402, T=0.5mm"                               
L6             Inductor                            TopLayer    L0402                           21.5389      30.3837      90       "Inductor, 15nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"            
L2             Inductor                            TopLayer    L0402                           16.7364      32.8000      90       "Inductor, Wire-wound, 5.6nH, ±0.1nH, 1770mA, 40mR, 0402, T=0.5mm"                 
L5             Inductor                            TopLayer    L0402                           16.1750      30.0750      90       "Inductor, Wire-wound, 6.2nH, ±0.1nH, 1600mA, 56mR, 0402, T=0.5mm"                 
L7             Inductor                            TopLayer    L0402                           16.1614      27.5250      90       "Inductor, Wire-wound, 3.6nH, ±0.1nH, 1950mA, 30mR, 0402, T=0.5mm"                 
L8             Inductor                            TopLayer    L0402                           15.6985      26.1000      0        "Inductor, Wire-wound, 12nHH, ±2%, 500mA, 1405mR, 0402, T=0.5mm"                   
L10            Inductor                            TopLayer    LQM21FN_70-IPC_C                21.5419      15.5691      180      "Inductor, 10uH, +/-20%, 100mA, 1R36, 0805, T=0.8mm"                               
L9             Inductor                            TopLayer    L0402                           20.8660      18.1470      90       ""                                                                                 
CN4            mmcx                                TopLayer    CON_SMA-RF_CINCH_142-0701-851   21.5000      57.4600      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                            
CN3            "Header 7x2"                        TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A 21.5000      5.4650       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin"      
CN2            FTSH-125-02-L-DV                    BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV 38.6560      18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                          
CN1            FTSH-125-02-L-DV                    BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV 4.3660       18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                          
C13            Capacitor                           TopLayer    C0402                           29.3500      28.6250      180      "Capacitor, MLCC, 6.8pF, ±0.05pF, C0G, 50V, 0402, T=0.5mm"                         
C9             Capacitor                           TopLayer    C0402                           29.3500      32.3750      180      "Capacitor, MLCC, 6.8pF, ±0.05pF, C0G, 50V, 0402, T=0.5mm"                         
C5             Capacitor                           TopLayer    C0402                           17.6748      33.7000      270      "Capacitor, MLCC, 100pF, 50V, COG, 1%, 0402, T=0.5mm"                              
C1             Capacitor                           TopLayer    C0402                           21.9500      54.1000      180      "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                          
C2             Capacitor                           TopLayer    C0402                           21.9500      51.5250      180      "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                          
C21            Capacitor                           TopLayer    C0402                           23.7500      18.1750      90       "Capacitor, MLCC, 220nF, 35V, X6S, +/-10%, 0402, T=0.5mm"                          
C23            Capacitor                           TopLayer    C0402                           22.3910      17.7220      180      "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                          
C15            Capacitor                           TopLayer    C0402                           14.4202      26.5554      270      "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                          
C26            Capacitor                           TopLayer    C0603                           15.8750      3.0250       270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                               
C20            Capacitor                           TopLayer    C0402                           17.3650      18.1829      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                          
C24            Capacitor                           TopLayer    C0402                           7.2860       14.1647      90       "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
C10            Capacitor                           TopLayer    C0402                           21.1000      31.6750      0        "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                       
C12            Capacitor                           TopLayer    C0402                           21.0903      28.9000      0        "Capacitor, MLCC, 0.5pF, 50V, C0G, +/-0.1pF, 0402, T=0.5mm"                        
C16            Capacitor                           TopLayer    C0402                           18.1750      25.0250      0        "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                          
C17            Capacitor                           TopLayer    C0402                           27.3750      20.6000      90       "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                          
C4             Capacitor                           TopLayer    C0402                           15.6995      34.3250      0        "Capacitor, MLCC, 2.7pF, 50V, C0G, +/-0.05pF, C0G, 0402, T=0.5mm"                  
C8             Capacitor                           TopLayer    C0402                           15.7114      31.3000      0        "Capacitor, MLCC, 5.6pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                        
C11            Capacitor                           TopLayer    C0402                           15.7250      28.8410      0        "Capacitor, MLCC, 5.3pF, 50V, C0G, +/-0.1pF, 0402, T=0.5mm"                        
C25            Capacitor                           TopLayer    C0402                           21.5500      34.8500      90       "Capacitor, MLCC,  2.2nF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                         
C6             Capacitor                           TopLayer    C0402                           15.7114      32.8250      90       "Capacitor, Monolithic CC, 1.2pF, 50V, +/-0.05pf, 0402, T=0.5mm"                   
C22            Capacitor                           TopLayer    C0402                           22.3910      18.5720      0        "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
C19            Capacitor                           TopLayer    C0402                           19.7250      20.1750      90       "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                          
C18            Capacitor                           TopLayer    C0402                           18.8566      18.6960      90       "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                          
CART-1         Comment                             TopLayer    Sheetbox_4L2S                   21.8436      -21.1485     0        ""                                                                                 
