Altium Designer Pick and Place Locations
D:\CAP1G\STM Le Mans\MB2202B\BASE\MB2202B\02-Manufacturing\MB2202B_PCB\Assembly\MB2202B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       18/12/25
Time:       15:03
Revision:   Not in VersionControl
Variant:    WB09TF4LI
Units used: mm

Designator Comment               Layer       Footprint                          Center-X(mm) Center-Y(mm) Rotation Description                                                      
HW3        STICKER_ES            BottomLayer STICKER_ES_6X6                     -63.8710     -61.9050     180      "Sticker ES, 6x6mm"                                              
HW2        STICKER_PRODUCT       BottomLayer STICKER_PRODUCT_25X9               -63.8710     -61.9050     180      "Sticker product, 25x9mm"                                        
U2         MLPF-WB55-01E3        TopLayer    ICC_CSPG_6BUMPS_1X1P60_P050-P0577  33.3500      15.2500      270      "2.4 GHz low pass filter matched to BLUENRG-LP-LPS"              
CN3        SMA-J-P-H-ST-EM1      TopLayer    CON_SMA_AMPHENOL_132415            39.8250      15.5000      90       "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                          
SB4        SB_ON                 TopLayer    SOLDER-BRIDGE_R0402-0R             26.4875      19.6000      180      "Resistor, 0R, SB0402, 5%, 0.063W"                               
SB3        SB_ON                 TopLayer    SOLDER-BRIDGE_R0402-0R             16.4625      10.7500      180      "Resistor, 0R, SB0402, 5%, 0.063W"                               
C13        Capacitor             TopLayer    C0402                              25.5250      17.2000      0        "Capacitor, MLCC, 0.22uF, X5R, 6.3V, +/-10%, 0402, T=0.5mm"      
C5         Capacitor             TopLayer    C0402                              17.0500      13.8500      270      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"          
C10        Capacitor             TopLayer    C0201_H0P3                         26.4500      15.8000      0        "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"         
C12        Capacitor             TopLayer    C0201_H0P3                         27.4000      17.9000      0        "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"         
C11        Capacitor             TopLayer    C0402                              27.1000      18.7000      0        "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"         
L1         Inductor              TopLayer    IND_0805_MURATA_LQM21              23.9000      14.3500      270      "Inductor, MLCC, 10uH, +/-20%, 300mA, 845mR, 0805, T=1.45mm"     
L2         Inductor              TopLayer    IND_0402_MURATA_LQG15HSXXXX02_H0P5 27.4250      12.7250      0        "Inductor, MLCC, 22nH, +/-2%, 350mA, 0.58R, 0402, T=1.45mm"      
C3         Capacitor             TopLayer    C0201_H0P3                         31.6500      15.4940      0        "Capacitor, MLCC, 20pF, 25V, COG, +/-2%, 0201, T=0.3mm"          
X1         XTAL_4_PINS           TopLayer    CRY_NX2016SA_4P                    30.8332      11.1250      270      "Crystal, 32MHz, 8pF, +/-10ppm, 60R, 2x1.6mm"                    
SB2        SB_ON                 TopLayer    SOLDER-BRIDGE_R0402-0R             18.9375      10.7500      0        "Resistor, 0R, SB0402, 5%, 0.063W"                               
SB1        SB_ON                 TopLayer    SOLDER-BRIDGE_R0402-0R             32.7500      11.3625      270      "Resistor, 0R, SB0402, 5%, 0.063W"                               
C2         Capacitor             TopLayer    C0201_H0P3                         32.0500      13.6000      225      "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"         
C1         Capacitor             TopLayer    C0402                              33.0000      12.7500      180      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"         
X2         XTAL_2_PINS           TopLayer    CRY_NX2012SA_2P                    17.8500      12.1500      180      "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"             
U1         IC_STM32WB09TEF6TR    TopLayer    ICC_WLCSP36_2P83X2P99_P040         29.2266      15.1539      90       "MCU, ARM Cortex-M0+ 32-bit, 512KB Flash, 64KB RAM, With Crypto" 
C9         Capacitor             TopLayer    C0402                              25.2500      15.9500      90       "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"        
C7         Capacitor             TopLayer    C0402                              25.8250      14.3000      270      "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"        
C4         Capacitor             TopLayer    C0402                              18.6000      13.8500      90       "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"          
C8         Capacitor             TopLayer    C0201_H0P3                         26.6250      14.1500      270      "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"         
C6         Capacitor             TopLayer    C0402                              25.1000      18.0750      180      "Capacitor, MLCC, 10nF, 16V, X7R, +/-10%, 0402, T=0.5mm"         
SC7        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R              14.9754      15.9324      270      "RFI shield clip mini TIN SMD"                                   
SC8        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R              27.7254      8.3582       180      "RFI shield clip mini TIN SMD"                                   
SC9        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R              22.2254      8.3582       180      "RFI shield clip mini TIN SMD"                                   
SC6        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R              27.7100      23.3500      180      "RFI shield clip mini TIN SMD"                                   
SC5        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R              22.2254      23.3582      180      "RFI shield clip mini TIN SMD"                                   
SC4        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R              16.9754      10.3582      270      "Shield clip Harwin S0981-46R to fix RF shielded cavity"         
SC3        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R              32.9754      10.3582      0        "Shield clip Harwin S0981-46R to fix RF shielded cavity"         
SC2        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R              16.9754      21.3582      180      "Shield clip Harwin S0981-46R to fix RF shielded cavity"         
SC1        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R              32.9754      21.3582      90       "Shield clip Harwin S0981-46R to fix RF shielded cavity"         
CN1        "Header 12x1"         TopLayer    CON_SAMTEC_TSW-112-07-X-S          19.9550      27.5000      180      "Header, 12x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                  
CN2        "Header 12x1"         TopLayer    CON_SAMTEC_TSW-112-07-X-S          19.9550      3.5000       180      "Header, 12x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                  
