Altium Designer Pick and Place Locations
C:\Subversion\01_Boards\MB2408\Trunk\02-Manufacturing\MB2408A_PCB\Assembly\MB2408A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       05/03/26
Time:       17:26
Revision:   3
Variant:    No variations
Units used: mm

Designator     Comment               Layer       Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                                                  
U2             IC_MLPF-WL-09D3       TopLayer    ICC_CSPG5_1P5X1P9_P060              18.7155      28.9881      90       "IC, 315MHz low pass filter matched to WBA mini board"                                       
C7             Capacitor             TopLayer    C0402                               20.8403      28.4881      180      "Capacitor, MLCC, 100pF, 50V, C0G/NP0, +/-1%, 0402, T=0.5mm"                                 
SB19           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.2000       5.2250       180      "Solder Bridge 0402 ON"                                                                      
L9             Inductor              TopLayer    IND_0402_MURATA_LQG15HSXXXX02_H0P5  20.7648      19.5425      90       "Inductor, 270nH, +/-2%, 110mA, 4R94, 0402, T=0.5mm"                                         
U1             IC_STM32WL3R          TopLayer    ICC_VFQFPN32-EPAD_5X5_P050          22.7916      24.3271      90       "MCU, ARM Cortex-M0 32-bit, 128KB Flash, 16KB SRAM, With Crypto"                             
SB2            SB_ON                 TopLayer    SOLDER-BRIDGE_R0201_0R              19.0750      25.5250      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                              
SB1            SB_ON                 TopLayer    SOLDER-BRIDGE_R0201_0R              19.0746      26.2664      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                              
SC13           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               24.0900      11.7750      0        "RFI shield clip mini TIN SMD"                                                               
SC12           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      24.2780      270      "RFI shield clip mini TIN SMD"                                                               
SC11           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      24.2780      90       "RFI shield clip mini TIN SMD"                                                               
SC10           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      19.1200      270      "RFI shield clip mini TIN SMD"                                                               
SC9            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      19.1200      90       "RFI shield clip mini TIN SMD"                                                               
SB16           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      8.3125       180      "Solder Bridge 0402 ON"                                                                      
SB15           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      7.1875       180      "Solder Bridge 0402 ON"                                                                      
SB9            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.1750      10.5824      180      "Solder Bridge 0402 ON"                                                                      
SB14           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.1750      11.6881      180      "Solder Bridge 0402 ON"                                                                      
SB13           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.1750      13.0611      180      "Solder Bridge 0402 ON"                                                                      
STICKER-BOARD1 Comment               TopLayer    STICKER_BOARD_25X5                  -265.4530    -237.3752    90       ""                                                                                           
STICKER-PROD1  Comment               TopLayer    STICKER_PRODUCT_25X5                -265.4530    -237.3752    90       ""                                                                                           
MIRE-4         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                39.7500      44.2500      180      ""                                                                                           
MIRE-5         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                2.7500       44.2500      180      ""                                                                                           
MIRE-3         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                2.5000       2.4500       0        ""                                                                                           
MIRE-2         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                39.7500      44.2500      0        ""                                                                                           
MIRE-1         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                2.7500       44.2500      0        ""                                                                                           
HW1            S02-20150300          TopLayer    SHIELD_HARWIN_S02-25200300_20X25_H3 -265.4530    -237.3752    0        "RFI shield CAN, 25x20x3mm"                                                                  
X1             XTAL_2_PINS           TopLayer    CRY_NX2012SA_2P                     28.9000      30.5000      90       "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                                         
X2             XTAL_4_PINS           TopLayer    CRY_NX1612SA_4P                     15.3800      23.8750      0        "Crystal, 48MHz, 8pF, +/-10 ppm, 22R, 1.6x1.2mm"                                             
SC7            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               29.5000      13.7745      0        "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC3            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               29.5000      34.7745      90       "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC2            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               13.5000      34.7745      180      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC6            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               13.5000      13.7745      270      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC8            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               18.8900      11.7740      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC5            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      29.4330      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC1            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               18.7500      36.7750      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC4            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      29.4330      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SB3            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.6875      32.7474      0        "Solder Bridge 0402 ON"                                                                      
SB4            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.6875      31.6474      0        "Solder Bridge 0402 ON"                                                                      
SB6            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2085      5.8750       180      "Solder Bridge 0402 ON"                                                                      
SB11           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.3125       3.9500       0        "Solder Bridge 0402 ON"                                                                      
SB5            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.1750      9.4521       180      "Solder Bridge 0402 ON"                                                                      
R7             Resistor              TopLayer    R0402                               26.9750      3.8750       270      Resistor,47R,0402,1%,1/16W                                                                   
R6             Resistor              TopLayer    R0402                               26.9750      7.0500       270      Resistor,47R,0402,1%,1/16W                                                                   
R5             Resistor              TopLayer    R0402                               24.0500      9.9500       90       Resistor,47R,0402,1%,1/16W                                                                   
R8             Resistor              TopLayer    R0402                               27.0026      2.1750       270      Resistor,47R,0402,1%,1/16W                                                                   
R2             Resistor              TopLayer    R0402                               33.2750      23.8750      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                         
R4             Resistor              TopLayer    R0402                               20.2250      9.9500       90       Resistor,47R,0402,1%,1/16W                                                                   
R3             Resistor              TopLayer    R0402                               18.9500      9.9500       90       Resistor,47R,0402,1%,1/16W                                                                   
L1             Inductor              TopLayer    L0402                               21.5500      39.9000      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
L8             Inductor              TopLayer    IND_0402_MURATA_LQW15AN_H0P5        16.8000      26.1000      0        "Inductor, 56nH, +/-0.2nH, Itemp=200mA max, 1R17, 0402, T=0.6mm, Qmin=25"                    
L10            Inductor              TopLayer    IND_0805_MURATA_LQM21               21.7698      17.5048      180      "Inductor, 10uH, +/-20%, 0A1, 0R5, 0805, T=1.45mm"                                           
CN4            mmcx                  TopLayer    CON_SMA-RF_CINCH_142-0701-851       21.5500      44.4600      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                                      
CN3            "Header 7x2"          TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A     21.5000      5.4650       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin"                
CN2            FTSH-125-02-L-DV      BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV     38.6560      18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
CN1            FTSH-125-02-L-DV      BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV     4.3660       18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
C13            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         29.3500      28.6250      180      "Capacitor, MLCC, 6.8pF, 50V,C0G/NP0, +/-0.05pF, 0402, T=0.5mm"                              
C9             Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         29.3500      32.3750      180      "Capacitor, MLCC, 6.8pF, 50V,C0G/NP0, +/-0.05pF, 0402, T=0.5mm"                              
C5             Capacitor             TopLayer    C0402                               17.2250      28.0881      270      "Capacitor, MLCC, 100pF, 50V, C0G/NP0, +/-1%, 0402, T=0.5mm"                                 
C1             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             22.0000      41.2500      180      "Capacitor, MLCC"                                                                            
C2             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             21.9500      38.5500      180      "Capacitor, MLCC,"                                                                           
C21            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         23.8826      19.8585      90       "Capacitor, MLCC, 220nF, 35V, X6S, +/-10%, 0402, T=0.5mm"                                    
C23            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         22.6329      19.0772      0        "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                    
C15            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         14.5750      26.5000      270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                    
C14            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         13.6250      26.5000      270      "Capacitor, MLCC, 100pF, 50V, C0G/NP0, +/-1%, 0402, T=0.5mm"                                 
C26            Capacitor             TopLayer    C0603                               15.8750      3.0250       270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                         
C20            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         17.6500      20.6187      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C16            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         18.2503      24.7762      0        "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                    
C17            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         26.6850      23.1750      90       "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                    
C22            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         22.6330      19.8732      0        "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                                    
C19            Capacitor             TopLayer    C0402_MURATA_GJM-GRM15_H0P5         19.8750      20.7750      270      "Capacitor, MLCC, 330pF, 50V, C0G, 5%, 0402, T=0.5mm"                                        
C18            Capacitor             TopLayer    C0402                               18.8520      18.9900      90       "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                                    
CART-1         Comment               TopLayer    Sheetbox_4L2S                       21.8436      -21.1484     0        ""                                                                                           
