| CMSIS-CORE Version 3.01 CMSIS-CORE support for Cortex-M processor-based devices

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

Data Fields
ITM_Type Struct Reference

Structure type to access the Instrumentation Trace Macrocell Register (ITM).

## Data Fields
union {
__O uint8_t u8
| Offset: 0x000 ( /W) ITM Stimulus Port 8-bit.
__O uint16_t u16
| Offset: 0x000 ( /W) ITM Stimulus Port 16-bit.
__O uint32_t u32
| Offset: 0x000 ( /W) ITM Stimulus Port 32-bit.
} | PORT [32]
| Offset: 0x000 ( /W) ITM Stimulus Port Registers.
uint32_t | RESERVED0 [864]
| Reserved.
__IO uint32_t | TER
| Offset: 0xE00 (R/W) ITM Trace Enable Register.
uint32_t | RESERVED1 [15]
| Reserved.
__IO uint32_t | TPR
| Offset: 0xE40 (R/W) ITM Trace Privilege Register.
uint32_t | RESERVED2 [15]
| Reserved.
__IO uint32_t | TCR
| Offset: 0xE80 (R/W) ITM Trace Control Register.

## Field Documentation

__O { ... } ITM_Type::PORT[32]

uint32_t ITM_Type::RESERVED0[864]

uint32_t ITM_Type::RESERVED1[15]

uint32_t ITM_Type::RESERVED2[15]

__IO uint32_t ITM_Type::TCR

__IO uint32_t ITM_Type::TER

__IO uint32_t ITM_Type::TPR

__O uint16_t ITM_Type::u16

__O uint32_t ITM_Type::u32

__O uint8_t ITM_Type::u8