Altium Designer Pick and Place Locations
C:\Users\buonoliv\OneDrive - STMicroelectronics\Desktop\DOC. Liv\Prodotti\BMS\L9965\UR6W-L9965P\Promo board\EVL9965P-N-R.0.0\Sources\Project Outputs for EVL99BM2P-N-R.0.0\Pick Place\Pick Place for EVL9965P-N-R.0.0(EVL99BM2P-FN R.0.0).txt

========================================================================================================================
File Design Information:

Date:       27/05/26
Time:       11:27
Revision:   Not in VersionControl
Variant:    EVL99BM2P-FN R.0.0
Units used: mil

Designator     Comment                     Layer       Footprint                           Center-X(mil) Center-Y(mil) Rotation Description                                                                                                 
J2             "2-POLES CONNECTOR"         TopLayer    691214310002                        488.189       2706.693      180      "Term Blk 2P Side Ent 2.54MM Pcb"                                                                           
Log2           "LOGO RICICLO"              TopLayer    LOGO_CHINA_ROHS_10                  -1518.700     -449.803      0        "LOGO RICICLO"                                                                                              
SDO_SPC        Open                        TopLayer    JP2_SMD                             2326.772      2492.126      0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
STM_FAULTN_SPC "Solder Jumper"             TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805        2393.463      2378.110      0        "Close 1-2 in EVL99BM2P variant
Close 2-3 in EVL9965P variant"                                             
CN7            CN7                         TopLayer    Header_19x2_-_FEMALE                213.386       1803.740      270      "CONN HEADER 19X2 POS 2.54MM FEMALE"                                                                        
CN10           CN10                        TopLayer    Header_19x2_-_FEMALE                2613.425      1803.740      270      "CONN HEADER 19X2 POS 2.54MM FEMALE"                                                                        
VDD_STM        Open                        TopLayer    JP2_SMD                             79.724        2468.504      270      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
R10            RES                         TopLayer    R2512-RS                            489.173       2433.071      180      "RES SMD 2O, 5%, 1W, 2512"                                                                                  
REG_VIO_CSA    "Solder Jumper"             TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805        735.236       938.976       270      Resistor                                                                                                    
IC2            L99VR02XP                   TopLayer    SOP50P1030X245-37N                  1253.091      742.375       270      "Integrated Circuit"                                                                                        
Q1             ZXTP56060FDBQ-7             TopLayer    ZXTP56060FDBQ7                      1941.929      1934.055      0        "Transistor BJT PNP"                                                                                        
SDI            MOSI                        TopLayer    TEST_POINT_-_SIP1                   1231.871      2380.905      0        "Keystone 4952 Test point"                                                                                  
SCLK           SCLK                        TopLayer    TEST_POINT_-_SIP1                   1305.277      2381.890      0        "Keystone 4952 Test point"                                                                                  
CMC_H1         "100uH ACT45B-101-2P-TL003" TopLayer    CHOKE                               451.772       849.409       0        "Common Mode Chokes Dual 100uH 5.8kOhm 100kHz 0.15A 2Ohm DCR SMD Automotive T/R"                            
CWUP           CWUP                        TopLayer    TEST_POINT_-_SIP1                   1525.493      2381.890      0        "Keystone 4952 Test point"                                                                                  
NCS            NCS                         TopLayer    TEST_POINT_-_SIP1                   1378.682      2381.890      0        "Keystone 4952 Test point"                                                                                  
R7             RES                         TopLayer    R0603-RS                            945.105       1302.096      270      "RES SMD 4.7k"                                                                                              
C11            22nF/50V                    TopLayer    C0603-B                             433.071       2233.268      270      Capacitor                                                                                                   
C12            22nF/50V                    TopLayer    C0603-B                             580.709       2333.661      0        Capacitor                                                                                                   
SDI_SPC        Open                        TopLayer    JP2_SMD                             2154.183      2492.523      0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
RX_SPC         Open                        TopLayer    JP2_SMD                             409.003       1677.773      0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
STM_FENL_SPC   "Solder Jumper"             TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805        2157.480      2264.835      0        "Close 1-2 in EVL99BM2P variant
Close 2-3 in EVL9965P variant"                                             
CAN_EN_SPC     Open                        TopLayer    JP2_SMD                             409.002       1853.723      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
RX_STM         Open                        TopLayer    JP2_SMD                             628.937       1677.773      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
CAN_EN_STM     Open                        TopLayer    JP2_SMD                             628.937       1853.723      0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
SDO_STM        Open                        TopLayer    JP2_SMD                             627.952       1942.074      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
CWUP_SPC       Open                        TopLayer    JP2_SMD                             409.002       2029.673      0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
CWUP_STM       Open                        TopLayer    JP2_SMD                             2154.183      2378.110      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
TX_SPC         Open                        TopLayer    JP2_SMD                             409.002       1765.748      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
VDD_SPC        Open                        TopLayer    JP2_SMD                             79.724        2235.236      90       "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
TX_STM         Open                        TopLayer    JP2_SMD                             628.937       1765.748      0        "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
SDI_STM        Open                        TopLayer    JP2_SMD                             628.937       2029.673      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
R20            RES                         TopLayer    R0805-RS                            1795.276      698.819       90       "Fixed Resistor, Metal Glaze/thick Film, 0.25W, 10000ohm, 150V, 1% +/-Tol, 100ppm/Cel, Surface Mount, 0805" 
C31            GCM31CD71H106KE36K          TopLayer    GCM31C5C2E183FX03L                  925.325       603.978       180      Capacitor                                                                                                   
C30            KGM31AR71H475KU             TopLayer    CAPC3216X180N                       936.129       690.011       180      Capacitor                                                                                                   
C29            GCM31CD71H106KE36K          TopLayer    GCM31C5C2E183FX03L                  925.197       862.205       180      Capacitor                                                                                                   
C28            KGM31AR71H475KU             TopLayer    CAPC3216X180N                       936.129       948.239       180      Capacitor                                                                                                   
C27            VJ0603Y104JXAAC             TopLayer    CAPC1608X97N                        1575.787      670.276       0        Capacitor                                                                                                   
C26            GCM31CD71H106KE36K          TopLayer    GCM31C5C2E183FX03L                  1611.220      521.653       0        Capacitor                                                                                                   
C25            KGM31AR71H475KU             TopLayer    CAPC3216X180N                       1610.039      601.378       0        Capacitor                                                                                                   
C23            VJ0603Y104JXAAC             TopLayer    CAPC1608X97N                        1575.787      813.088       0        Capacitor                                                                                                   
C24            GCM31CD71H106KE36K          TopLayer    GCM31C5C2E183FX03L                  1612.205      972.441       0        Capacitor                                                                                                   
C22            KGM31AR71H475KU             TopLayer    CAPC3216X180N                       1610.039      892.716       0        Capacitor                                                                                                   
C20            GCM188R71H103KA37J          TopLayer    CAPC1608X90N                        2011.811      706.693       270      Capacitor                                                                                                   
C19            VJ0603Y104JXAAC             TopLayer    CAPC1608X97N                        1957.677      706.693       270      Capacitor                                                                                                   
C18            GCM21BM8EH225KE08L          TopLayer    GCM21                               1896.653      695.866       270      Capacitor                                                                                                   
C9             GCM188R71H103KA37J          TopLayer    CAPC1608X90N                        1490.158      2023.622      270      Capacitor                                                                                                   
C8             GCM188R71H103KA37J          TopLayer    CAPC1608X90N                        1438.976      2023.622      270      Capacitor                                                                                                   
R19            CRCW0402267KFKED            TopLayer    RESC1005X40N                        1085.630      475.703       180      Resistor                                                                                                    
R18            CRCW0402267KFKED            TopLayer    RESC1005X40N                        1134.842      1005.181      180      Resistor                                                                                                    
R17            ERJ-P06D1200V               TopLayer    ERJP06D1000V                        453.518       624.995       0        "Res Thick Film 0805 120 Ohm 0.5% 0.25W ±100ppm/°C Molded SMD Punched Carrier T/R"                          
IC1            TJA1057GT_3                 TopLayer    SOIC127P600X175-8N                  452.756       1293.307      270      "TJA1057 Series 5.25V Surface Mount High-Speed CAN Transceiver - SOIC-8"                                    
DB1            "Cannon 9M"                 TopLayer    DB9M                                637.598       267.520       180      "Socket Assembly, 9 Position, Right Angle"                                                                  
C16            GRM1885C2A470GA01J          TopLayer    CAPC1608X90N                        561.775       520.561       0        "Cap Ceramic 47pF 100V C0G 2% SMD 0603 125°C Paper T/R"                                                     
C14            GRM1885C2A470GA01J          TopLayer    CAPC1608X90N                        347.429       520.729       180      "Cap Ceramic 47pF 100V C0G 2% SMD 0603 125°C Paper T/R"                                                     
D7             ESDCAN03-2BWY               TopLayer    SOT65P210X110-3N                    453.518       524.012       270      "ESD Suppressor TVS Dual Bi-Dir ï¿½30kV@Air Gap/ï¿½30kV@Contact Disc 3-Pin SOT-323 T/R"                     
L9965P         U1                          TopLayer    VFQFN32_4L_EP                       1281.496      2102.362      270      "1-channel pyrofuse driver used with L9965 product family"                                                  
GND4           GND                         TopLayer    4952k                               2636.811      262.795       0        "Test Point"                                                                                                
FENL           FENL                        TopLayer    TEST_POINT_-_SIP1                   1012.795      2000.984      0        "Keystone 4952 Test point"                                                                                  
FENH           FENH                        TopLayer    TEST_POINT_-_SIP1                   1012.795      2074.570      0        "Keystone 4952 Test point"                                                                                  
GND3           GND                         TopLayer    4952k                               2203.740      2750.984      270      "Test Point"                                                                                                
GND2           GND                         TopLayer    4952k                               98.425        535.433       270      "Test Point"                                                                                                
GND1           GND                         TopLayer    4952k                               947.835       2444.882      180      "Test Point"                                                                                                
PR             TEST_POINT                  TopLayer    TEST_POINT_-_SIP1                   921.009       2074.570      0        "Keystone 4952 Test point"                                                                                  
VIO            TEST_POINT                  TopLayer    TEST_POINT_-_SIP1                   741.142       1121.063      0        "Keystone 4952 Test point"                                                                                  
SDO            MISO                        TopLayer    TEST_POINT_-_SIP1                   1158.466      2381.890      0        "Keystone 4952 Test point"                                                                                  
FAULTN         TEST_POINT                  TopLayer    TEST_POINT_-_SIP1                   1452.088      2381.890      0        "Keystone 4952 Test point"                                                                                  
PF             TEST_POINT                  TopLayer    TEST_POINT_-_SIP1                   875.984       1874.016      0        "Keystone 4952 Test point"                                                                                  
ERBST          TEST_POINT                  TopLayer    TEST_POINT_-_SIP1                   1823.511      1703.084      0        "Keystone 4952 Test point"                                                                                  
VBATMON        TEST_POINT                  TopLayer    TEST_POINT_-_SIP1                   1940.945      2198.819      0        "Keystone 4952 Test point"                                                                                  
ERBSTSW        ERBSTSW                     TopLayer    TEST_POINT_-_SIP1                   1483.268      2204.724      0        "Keystone 4952 Test point"                                                                                  
R16            100O                        TopLayer    0603_R                              552.713       1519.461      270      "SMD Chip Resistor, 100 ohm, ï¿½ 0.1%, 125 mW, 0603 [1608 Metric], Thin Film, High Stability"               
R15            100O                        TopLayer    0603_R                              366.142       1516.673      270      "SMD Chip Resistor, 100 ohm, ï¿½ 0.1%, 125 mW, 0603 [1608 Metric], Thin Film, High Stability"               
R14            RCA06030000ZSTA             TopLayer    RESC1608X50N                        1062.008      2176.181      180      Resistor                                                                                                    
R13            RCA06030000ZSTA             TopLayer    RESC1608X50N                        1289.370      2277.559      90       Resistor                                                                                                    
R12            RCA06030000ZSTA             TopLayer    RESC1608X50N                        1062.992      2131.890      180      Resistor                                                                                                    
R11            RES                         TopLayer    R0603-RS                            1126.968      1404.528      90       "RES SMD 1k"                                                                                                
R9             RES                         TopLayer    R0603-RS                            739.173       1219.488      180      "RES SMD 1k"                                                                                                
R8             RES                         TopLayer    R0603-RS                            687.008       1376.968      270      "RES SMD 4.7k"                                                                                              
R6             RNCE0805BTE10K0             TopLayer    RESC2012X65N                        2234.252      1812.992      90       Resistor                                                                                                    
R5             ERJP06J681V                 TopLayer    ERJP06D1000V                        1979.331      1772.638      270      Resistor                                                                                                    
R4             CRCW040210R0FKEDC           TopLayer    RESC1005X35N                        1473.425      2154.528      0        Resistor                                                                                                    
R3             RES                         TopLayer    R1020-RS                            1616.142      1991.142      90       "RES SMD 68O, 1%, 1W, 1020"                                                                                 
R2             ERJ-P06J2R2V                TopLayer    ERJP06D1000V                        2077.756      1977.362      90       Resistor                                                                                                    
Q3             PNP                         TopLayer    SOT-323                             1039.271      1263.710      180      "PNP GENERAL PURPOSE, 30V, 0.5A"                                                                            
Q2             NPN                         TopLayer    SOT-23-RS                           1025.591      1463.583      270      "NPN GENERAL PURPOSE, 100V, 0.5A, SOT23-3"                                                                  
L1             VLS4020CX-330M-H            TopLayer    VLS4020CX                           1696.850      2214.567      180      "SMD / SMT Inductors (Coils), L=33µH, L x W x T :"                                                          
J3             1377297                     TopLayer    1377297                             2606.201      583.661       90       Connector                                                                                                   
Fid1           Fiducial                    TopLayer    Fiducial_1mm                        2362.205      556.102       0        "Fiducial 1mm"                                                                                              
D8             STPS2L60ZFY                 TopLayer    SODFL3516X110N                      2115.157      674.212       270      "Schottky Diode"                                                                                            
D6             LED_RED                     TopLayer    0805_LED                            813.976       1303.149      180      "LED RED DIFFUSED, 0805 SMD"                                                                                
D5             LED_YELLOW                  TopLayer    0805_LED                            813.976       1406.496      180      "LED YELLOW DIFFUSED, 0805 SMD"                                                                             
D4             LED_GREEN                   TopLayer    0805_LED                            814.961       1509.842      180      "LED GREEN DIFFUSED, 0805 SMD"                                                                              
D3             SK34BHE3-LTP                TopLayer    DIOM5336X262N                       1538.386      1827.756      0        Diode                                                                                                       
D2             DIODE                       TopLayer    SOD123                              1555.118      2161.417      90       "SCHOTTKY DIODE 40V 1A SOD123FLAT"                                                                          
D1             SK34BHE3-LTP                TopLayer    DIOM5336X262N                       1843.504      1414.370      270      Diode                                                                                                       
C13            100nF/50V                   TopLayer    C0603-B                             1083.130      2245.502      180      Capacitor                                                                                                   
C4             CAP_POL                     TopLayer    CAP._10_X_12_-_SMD                  2214.562      1375.975      0        "CAP ELT 330uF 35V"                                                                                         
C3             CAP_POL                     TopLayer    CAP._10_X_12_-_SMD                  1478.188      1383.630      0        "CAP ELT 330uF 35V"                                                                                         
LOAD           Closed                      TopLayer    JP2_SMD                             399.606       2317.913      180      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
BST            Closed                      TopLayer    JP2_SMD                             1830.709      2240.157      270      "Circuit Breaker 0603 - NOT MOUNTED"                                                                        
R1             MMB02070C4708FB200          TopLayer    MMB0207_VIS-M                       1842.520      1106.299      90       "MMB 0207-50 1% B2 4R7"                                                                                     
Log4           "LOGO RAEE"                 TopLayer    LOGO_CESTINO                        -1518.700     -449.803      0        "LOGO RAEE"                                                                                                 
Log3           "LOGO ST SERIGRAFIA"        TopLayer    LOGO_ST_PICCOLO_-_NO_LIFE_AUGMENTED -1518.700     -449.803      0        "LOGO ST SERIGRAFIA"                                                                                        
Log1           "LOGO RoHS"                 TopLayer    LOGO_RoHS_-_3                       -1518.700     -449.803      0        "LOGO RoHS"                                                                                                 
LED_VS         LED_BLUE                    TopLayer    0805_LED                            1795.276      517.577       90       "LED BLUE DIFFUSED, 0805 SMD"                                                                               
3V3_VIO_5V     "Solder Jumper"             TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805        1361.220      458.661       180      Resistor                                                                                                    
J1             "2-POLES CONNECTOR"         TopLayer    691214310002                        2308.071      148.622       0        "Term Blk 2P Side Ent 2.54MM Pcb"                                                                           
STM_SCLK_SPC   ""                          TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805        2393.463      2264.773      0        "Close 1-2 in EVL99BM2P variant
Close 2-3 in EVL9965P variant"                                             
STM_FENH_SPC   "Solder Jumper"             TopLayer    JUMP_A_SALDARE_TRIPLO_-_0805        2157.481      2138.627      0        "Close 1-2 in EVL99BM2P variant
Close 2-3 in EVL9965P variant"                                             
Fid3           Fiducial                    TopLayer    Fiducial_1mm                        605.315       676.181       90       "Fiducial 1mm"                                                                                              
Fid2           Fiducial                    BottomLayer Fiducial_1mm                        778.543       1928.150      90       "Fiducial 1mm"                                                                                              
D10            SM6T16V5AY                  TopLayer    DIOM5436X265N                       1977.362      182.579       180      "TVS Diode (Uni-directional)"                                                                               
D9             SM6T33AY                    TopLayer    DIOM5436X265N                       1977.362      359.744       180      "TVS Diode (Uni-directional)"                                                                               
C21            GCM21BM8EH225KE08L          TopLayer    GCM21                               2271.653      349.409       180      Capacitor                                                                                                   
C17            CAP                         TopLayer    0805                                374.016       1082.677      270      "CAP CER 100nF 100V X7R 0805"                                                                               
C15            CAP                         TopLayer    0805                                456.693       1498.032      0        "CAP CER 100nF 100V X7R 0805"                                                                               
C10            C0402C221K5TACAUTO          TopLayer    C0402C104J4RACTU                    1469.488      2106.299      180      Capacitor                                                                                                   
C7             GCM21BR71H474KA55K          TopLayer    CAPC2012X140N                       1824.803      1966.732      270      Capacitor                                                                                                   
