Altium Designer Pick and Place Locations
C:\Subversion\MB1818-Nucleo144_Display_Expansion\Trunk\02-Manufacturing\MB1818B_PCB\Assembly\MB1818B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       02/07/21
Time:       15:49
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment              Layer       Footprint                          Center-X(mm) Center-Y(mm) Rotation Description                                                                             
U1         MX25L6433FM2I-08G    BottomLayer ICC_SOP8_5P23X5P28_P127            35.0520      67.4370      270      ""                                                                                      
R12        Resistor             BottomLayer R0603                              34.9758      71.2470      360      Resistor,10K,0603,1%,1/10W                                                              
R11        Resistor             BottomLayer R1206_H0P55                        21.4630      55.3720      270      Resistor,6.2R,1206,1%,0.5W                                                              
R10        Resistor             BottomLayer R1206_H0P55                        23.8760      55.3720      270      Resistor,6.2R,1206,1%,0.5W                                                              
R9         Resistor             BottomLayer R1206_H0P55                        26.2890      55.3720      270      Resistor,6.2R,1206,1%,0.5W                                                              
R8         Resistor             BottomLayer R1206_H0P55                        45.9740      54.6100      270      Resistor,6.2R,1206,1%,0.5W                                                              
R7         Resistor             BottomLayer R0603                              43.5610      54.7370      270      Resistor,10K,0603,1%,1/10W                                                              
R6         Resistor             BottomLayer R0603                              30.4800      54.9910      90       Resistor,10K,0603,1%,1/10W                                                              
R5         Resistor             TopLayer    R0603                              42.0370      10.9728      360      Resistor,10K,0603,1%,1/10W                                                              
R4         Resistor             TopLayer    R0603                              42.0766      7.6454       360      Resistor,10K,0603,1%,1/10W                                                              
R3         Resistor             TopLayer    R0603                              27.3954      4.7244       180      Resistor,10K,0603,1%,1/10W                                                              
R2         Resistor             TopLayer    R0603                              27.4066      7.8232       180      Resistor,10K,0603,1%,1/10W                                                              
R1         Resistor             TopLayer    R0603                              27.4320      10.9474      360      Resistor,10K,0603,1%,1/10W                                                              
LCD1       DT022CTFT            TopLayer    LCD_DISPLAYTECH_DT022CTFT_45P_P050 35.0520      32.2250      0        "240x320 2.2inch display"                                                               
CN10       "Header 17x2"        BottomLayer CON_SAMTEC_TSW-117-07-X-D_INV      57.9120      36.7030      270      "Header, 17x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm, pin inverted compare to datasheet" 
CN9        "Header 15x2"        BottomLayer CON_SAMTEC_TSW-115-07-G-D_INV      12.1920      34.1630      270      "Header, 15x2, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                         
CN8        "Header 8x2"         BottomLayer CON_SAMTEC_TSW-108-07-X-D_INV      12.1920      65.9130      270      "Header, 8x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                     
CN7        "Header 10x2"        BottomLayer CON_SAMTEC_TSW-110-07-G-D_INV      57.9120      72.5170      270      "Header, 10x2, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                         
CN1        FH12-45S-0.5SH(55)   BottomLayer CON_HRS_FH12-45S-05SH              35.0520      48.8750      180      "45 pins P 0.5 surface mount connector"                                                 
C7         Capacitor            BottomLayer C0603                              28.3210      54.9910      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                               
C6         Capacitor            BottomLayer C0603                              29.3370      68.5800      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                               
C5         Capacitor            TopLayer    C0603                              42.0370      9.5758       180      Capacitor,10nF,100V,X7R,10%,0603                                                        
C4         Capacitor            TopLayer    C0603                              42.0766      6.2484       180      Capacitor,10nF,100V,X7R,10%,0603                                                        
C3         Capacitor            TopLayer    C0603                              27.3954      5.9944       360      Capacitor,10nF,100V,X7R,10%,0603                                                        
C2         Capacitor            TopLayer    C0603                              27.4066      9.2202       360      Capacitor,10nF,100V,X7R,10%,0603                                                        
C1         Capacitor            TopLayer    C0603                              27.4320      12.3444      360      Capacitor,10nF,100V,X7R,10%,0603                                                        
B1         "Joystick MT-008A_M" TopLayer    SWI_XIEJIA_MT-008A_6P              34.9250      8.3820       45       "Joystick, 4 dir, 1 OK"                                                                 
HW2        STICKER_PRODUCT      TopLayer    STICKER_PRODUCT_25X5               -269.4740    -198.1464    90       "Sticker product 25x5 mm"                                                               
HW3        STICKER_BOARD        TopLayer    STICKER_BOARD_25X5                 -269.4740    -198.1464    90       "Sticker board 25x5 mm"                                                                 
