
-----------------------------------
ORCAD used release
-----------------------------------

IPS161HF ORCAD macromodels developed using the platform ORCAD Capture 17.4-2019 S013 SPB 64-bit Edition.



-----------------------------------
Install and Use the macromodels 
-----------------------------------

IPS161HF Orcad macromodels are inside the folder MODEL, 
those ones listed are for Transient simulations:


1) IPS161HF_encry.lib and IPS161HF_encry.lib:
   encrypted macromodel libraries.

2) IPS161HF.OLB and IPS161HF.OLB:
   symbol libraries.  
   
   
In order to use these macromodels the user has to select Edit Simulation Profile -> Configuration Files -> Library
Insert the filename of the model and click to "Add to Design" button.

To simulate correctly, also in Simulation Settings follow this setup:

1) Simulation Settings -> Options -> Analog Simulation -> Auto Converge, click on Autoconverge checkbox.

2) Simulation Settings -> Options -> Gate Level Simulation -> General -> DIGINITSTATE, set it as 0 (from default value of X)




-----------------------------------
Sample Testbenchs Applications
-----------------------------------

Some sample testbenches are contained inside the folder IPS161Hx_SAMPLE_TESTBENCHES.

-----------------------------------
Model History
-----------------------------------

v2.0) VCC function as vdc.

v1.0) Model file. 